Schedule:Compact,
   ZONE CONTROL TYPE SCHED,                         !Name
   Control Type,                         !ScheduleType
   Through:3/31,                         !Complex Field #1
   For: Alldays,                         !Complex Field #2
   Until:24:00,1,                         !Complex Field #3
   Through:9/30,                         !Complex Field #4
   For: Alldays,                         !Complex Field #5
   Until:24:00,2,                         !Complex Field #6
   Through:12/31,                         !Complex Field #7
   For: Alldays,                         !Complex Field #8
   Until:24:00,1;                         !Complex Field #9
Schedule:Compact,
   RADIANT HEATING SETPOINTS,                         !Name
   Temperature,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Alldays,                         !Complex Field #2
   Until:7:00,12,                         !Complex Field #3
   Until:17:00,17,                         !Complex Field #4
   Until:24:00,12;                         !Complex Field #5
Schedule:Compact,
   COOLING SETPOINTS,                         !Name
   Temperature,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Alldays,                         !Complex Field #2
   Until:7:00,30,                         !Complex Field #3
   Until:17:00,24,                         !Complex Field #4
   Until:24:00,30;                         !Complex Field #5
Schedule:Compact,
   ANNUAL SUPPLY AIR TEMP SCH,                         !Name
   TEMPERATURE,                         !ScheduleType
   Through: 3/31,                         !Complex Field #1
   For: Alldays,                         !Complex Field #2
   Until:24:00,25,                         !Complex Field #3
   Through: 9/30,                         !Complex Field #4
   For: Alldays,                         !Complex Field #5
   Until:24:00,17,                         !Complex Field #6
   Through: 12/31,                         !Complex Field #7
   For: Alldays,                         !Complex Field #8
   Until:24:00,25;                         !Complex Field #9
Schedule:Compact,
   COND Loop TEMP Schedule,                         !Name
   Temperature,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Alldays,                         !Complex Field #2
   Until:24:00,29;                         !Complex Field #3
NodeList,
   Chilled Water Loop Setpoint Node List,                         !Node List Name
   CW Supply Outlet Node;                         !Node_ID_1
NodeList,
   Hot Water Loop Setpoint Node List,                         !Node List Name
   HW Supply Outlet Node;                         !Node_ID_1
NodeList,
   COND Loop Setpoint nodelist,                         !Node List Name
   Condenser Supply Outlet Node;                         !Node_ID_1
BranchList,
   Cooling Supply Side Branches,                         !Branch List Name
   CW Pump Branch,                         !Branch Name 1
   Big Chiller Branch,                         !Branch Name 2
   Little Chiller Branch,                         !Branch Name 3
   Purchased Cooling Branch,                         !Branch Name 4
   Supply Bypass Branch,                         !Branch Name 5
   Cooling Supply Outlet;                         !Branch Name 6
BranchList,
   Cooling Demand Side Branches,                         !Branch List Name
   Cooling Demand Inlet,                         !Branch Name 1
   West Zone_Zone 1 Cooling Branch,                         !Branch Name 2
   EAST ZONE_Zone 2 Cooling Branch,                         !Branch Name 3
   NORTH ZONE_Zone 3 Cooling Branch,                         !Branch Name 4
   Demand Bypass Branch,                         !Branch Name 5
   Cooling Demand Outlet;                         !Branch Name 6
BranchList,
   Condenser Supply Side Branches,                         !Branch List Name
   Condenser Supply Inlet Branch,                         !Branch Name 1
   Condenser Supply Tower Branch,                         !Branch Name 2
   Condenser Supply Bypass Branch,                         !Branch Name 3
   Condenser Supply Outlet Branch;                         !Branch Name 4
BranchList,
   Condenser Demand Side Branches,                         !Branch List Name
   Condenser Demand Inlet Branch,                         !Branch Name 1
   Big Chiller Condenser Branch,                         !Branch Name 2
   Little Chiller Condenser Branch,                         !Branch Name 3
   Condenser Demand Bypass Branch,                         !Branch Name 4
   Condenser Demand Outlet Branch;                         !Branch Name 5
BranchList,
   Heating Supply Side Branches,                         !Branch List Name
   Heating Supply Inlet Branch,                         !Branch Name 1
   Heating Purchased Hot Water Branch,                         !Branch Name 2
   Heating Supply Bypass Branch,                         !Branch Name 3
   Heating Supply Outlet Branch;                         !Branch Name 4
BranchList,
   Heating Demand Side Branches,                         !Branch List Name
   Reheat Inlet Branch,                         !Branch Name 1
   West Zone_Zone 1 Radiant Branch,                         !Branch Name 2
   EAST ZONE_Zone 2 Radiant Branch,                         !Branch Name 3
   NORTH ZONE_Zone 3 Radiant Branch,                         !Branch Name 4
   Reheat Bypass Branch,                         !Branch Name 5
   Reheat Outlet Branch;                         !Branch Name 6
PlantLoop,
   Chilled Water Loop,                         !Plant Loop Name
   Water,                         !Fluid Type
   CW Loop Operation,                         !Plant Operation Scheme List Name
   CW Supply Outlet Node,                         !Loop Temperature Setpoint Node Name
   98,                         !Maximum Loop Temperature
   1,                         !Minimum Loop Temperature
   0.0039,                         !Maximum Loop Volumetric Flow Rate
   0,                         !Minimum Loop Volumetric Flow Rate
   autocalculate,                         !volume of the plant loop
   CW Supply Inlet Node,                         !Plant Side Inlet Node Name
   CW Supply Outlet Node,                         !Plant Side Outlet Node Name
   Cooling Supply Side Branches,                         !Plant Side Branch List Name
   Cooling Supply Side Connectors,                         !Plant Side Connector List Name
   CW Demand Inlet Node,                         !Demand Side Inlet Node Name
   CW Demand Outlet Node,                         !Demand Side Outlet Nodes Name
   Cooling Demand Side Branches,                         !Demand Side Branch List Name
   Cooling Demand Side Connectors,                         !Demand Side Connector List Name
   OPTIMAL,                         !Load Distribution Scheme
   ,                         !System Availability Manager List
   ,                         !Plant Loop Demand Calculation Scheme
   ,                         !Common Pipe Simulation
   ;                         !Pressure Simulation Type
PlantLoop,
   Hot Water Loop,                         !Plant Loop Name
   Water,                         !Fluid Type
   Hot Loop Operation,                         !Plant Operation Scheme List Name
   HW Supply Outlet Node,                         !Loop Temperature Setpoint Node Name
   100,                         !Maximum Loop Temperature
   10,                         !Minimum Loop Temperature
   0.0043,                         !Maximum Loop Volumetric Flow Rate
   0,                         !Minimum Loop Volumetric Flow Rate
   autocalculate,                         !volume of the plant loop
   HW Supply Inlet Node,                         !Plant Side Inlet Node Name
   HW Supply Outlet Node,                         !Plant Side Outlet Node Name
   Heating Supply Side Branches,                         !Plant Side Branch List Name
   Heating Supply Side Connectors,                         !Plant Side Connector List Name
   HW Demand Inlet Node,                         !Demand Side Inlet Node Name
   HW Demand Outlet Node,                         !Demand Side Outlet Nodes Name
   Heating Demand Side Branches,                         !Demand Side Branch List Name
   Heating Demand Side Connectors,                         !Demand Side Connector List Name
   OPTIMAL,                         !Load Distribution Scheme
   ,                         !System Availability Manager List
   ,                         !Plant Loop Demand Calculation Scheme
   ,                         !Common Pipe Simulation
   ;                         !Pressure Simulation Type
CondenserLoop,
   Chilled Water Condenser Loop,                         !Condenser Loop Name
   Water,                         !Fluid Type
   Tower Loop Operation,                         !Condenser Operation Scheme List Name
   Condenser Supply Outlet Node,                         !Condenser Loop Temperature Setpoint Node or reference
   80,                         !Maximum Loop Temperature
   10,                         !Minimum Loop Temperature
   0.0022,                         !Maximum Loop Volumetric Flow Rate
   0,                         !Minimum Loop Volumetric Flow Rate
   autocalculate,                         !volume of the condenser loop
   Condenser Supply Inlet Node,                         !Condenser Side Inlet Node Name
   Condenser Supply Outlet Node,                         !Condenser Side Outlet Node Name
   Condenser Supply Side Branches,                         !Condenser Side Branch List Name
   Condenser Supply Side Connectors,                         !Condenser Side Connector List Name
   Condenser Demand Inlet Node,                         !Demand Side Inlet Node Name
   Condenser Demand Outlet Node,                         !Demand Side Outlet Nodes Name
   Condenser Demand Side Branches,                         !Condenser Demand Side Branch List Name
   Condenser Demand Side Connectors,                         !Condenser Demand Side Connector List Name
   Sequential,                         !Load Distribution Scheme
   ;                         !Pressure Simulation Type
Branch,
   Cooling Demand Inlet,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Demand Side Inlet Pipe,                         !Comp1 Name
   CW Demand Inlet Node,                         !Comp1 Inlet Node Name
   CW Demand Entrance Pipe Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Demand Bypass Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Demand Side Bypass,                         !Comp1 Name
   CW Demand Bypass Inlet Node,                         !Comp1 Inlet Node Name
   CW Demand Bypass Outlet Node,                         !Comp1 Outlet Node Name
   BYPASS;                         !Comp1 Branch Control Type
Branch,
   Cooling Demand Outlet,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   CW Demand Side Outlet Pipe,                         !Comp1 Name
   CW Demand Exit Pipe Inlet Node,                         !Comp1 Inlet Node Name
   CW Demand Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Cooling Supply Outlet,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Supply Side Outlet Pipe,                         !Comp1 Name
   Supply Side Exit Pipe Inlet Node,                         !Comp1 Inlet Node Name
   CW Supply Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   CW Pump Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pump:VariableSpeed,                         !Comp1 Type
   Circ Pump,                         !Comp1 Name
   CW Supply Inlet Node,                         !Comp1 Inlet Node Name
   CW Pump Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Little Chiller Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Chiller:ConstantCOP,                         !Comp1 Type
   Little Chiller,                         !Comp1 Name
   Little Chiller Inlet Node,                         !Comp1 Inlet Node Name
   Little Chiller Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Big Chiller Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   CHILLER:ELECTRIC,                         !Comp1 Type
   Big Chiller,                         !Comp1 Name
   Big Chiller Inlet Node,                         !Comp1 Inlet Node Name
   Big Chiller Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Purchased Cooling Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   DistrictCooling,                         !Comp1 Type
   Purchased Cooling,                         !Comp1 Name
   Purchased Cooling Inlet Node,                         !Comp1 Inlet Node Name
   Purchased Cooling Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Supply Bypass Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Supply Side Bypass,                         !Comp1 Name
   CW Supply Bypass Inlet Node,                         !Comp1 Inlet Node Name
   CW Supply Bypass Outlet Node,                         !Comp1 Outlet Node Name
   BYPASS;                         !Comp1 Branch Control Type
Branch,
   Condenser Supply Inlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pump:VariableSpeed,                         !Comp1 Type
   Cond Circ Pump,                         !Comp1 Name
   Condenser Supply Inlet Node,                         !Comp1 Inlet Node Name
   Condenser Pump Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Condenser Supply Tower Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   COOLINGTOWER:SINGLESPEED,                         !Comp1 Type
   Big Tower,                         !Comp1 Name
   Condenser Tower Inlet Node,                         !Comp1 Inlet Node Name
   Condenser Tower Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Condenser Supply Bypass Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Condenser Supply Side Bypass,                         !Comp1 Name
   Cond Supply Bypass Inlet Node,                         !Comp1 Inlet Node Name
   Cond Supply Bypass Outlet Node,                         !Comp1 Outlet Node Name
   BYPASS;                         !Comp1 Branch Control Type
Branch,
   Condenser Supply Outlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Condenser Supply Outlet,                         !Comp1 Name
   Condenser Supply Exit Pipe Inlet Node,                         !Comp1 Inlet Node Name
   Condenser Supply Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Condenser Demand Inlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Condenser Demand Inlet Pipe,                         !Comp1 Name
   Condenser Demand Inlet Node,                         !Comp1 Inlet Node Name
   Condenser Demand Entrance Pipe Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Little Chiller Condenser Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Chiller:ConstantCOP,                         !Comp1 Type
   Little Chiller,                         !Comp1 Name
   Little Chiller Condenser Inlet Node,                         !Comp1 Inlet Node Name
   Little Chiller Condenser Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Big Chiller Condenser Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   CHILLER:ELECTRIC,                         !Comp1 Type
   Big Chiller,                         !Comp1 Name
   Big Chiller Condenser Inlet Node,                         !Comp1 Inlet Node Name
   Big Chiller Condenser Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Condenser Demand Bypass Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Condenser Demand Side Bypass,                         !Comp1 Name
   Cond Demand Bypass Inlet Node,                         !Comp1 Inlet Node Name
   Cond Demand Bypass Outlet Node,                         !Comp1 Outlet Node Name
   BYPASS;                         !Comp1 Branch Control Type
Branch,
   Condenser Demand Outlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Condenser Demand Outlet Pipe,                         !Comp1 Name
   Condenser Demand Exit Pipe Inlet Node,                         !Comp1 Inlet Node Name
   Condenser Demand Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Heating Supply Inlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pump:VariableSpeed,                         !Comp1 Type
   HW Circ Pump,                         !Comp1 Name
   HW Supply Inlet Node,                         !Comp1 Inlet Node Name
   HW Pump Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Heating Purchased Hot Water Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   DistrictHeating,                         !Comp1 Type
   Purchased Heating,                         !Comp1 Name
   Purchased Heat Inlet Node,                         !Comp1 Inlet Node Name
   Purchased Heat Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Heating Supply Bypass Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Heating Supply Side Bypass,                         !Comp1 Name
   Heating Supply Bypass Inlet Node,                         !Comp1 Inlet Node Name
   Heating Supply Bypass Outlet Node,                         !Comp1 Outlet Node Name
   BYPASS;                         !Comp1 Branch Control Type
Branch,
   Heating Supply Outlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Heating Supply Outlet,                         !Comp1 Name
   Heating Supply Exit Pipe Inlet Node,                         !Comp1 Inlet Node Name
   HW Supply Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Reheat Inlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Reheat Inlet Pipe,                         !Comp1 Name
   HW Demand Inlet Node,                         !Comp1 Inlet Node Name
   HW Demand Entrance Pipe Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Reheat Outlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Reheat Outlet Pipe,                         !Comp1 Name
   HW Demand Exit Pipe Inlet Node,                         !Comp1 Inlet Node Name
   HW Demand Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   West Zone_Zone 1 Radiant Branch,                      !Branch Name
   autosize,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   ZoneHVAC:LowTemperatureRadiant:ConstantFlow,                      !Comp1 Type
   West Zone_West Zone Radiant Floor,                      !Comp1 Name
   West Zone_West Zone Radiant Water Inlet Node,                      !Comp1 Inlet Node Name
   West Zone_West Zone Radiant Water Outlet Node,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   EAST ZONE_Zone 2 Radiant Branch,                      !Branch Name
   autosize,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   ZoneHVAC:LowTemperatureRadiant:ConstantFlow,                      !Comp1 Type
   EAST ZONE_East Zone Radiant Floor,                      !Comp1 Name
   EAST ZONE_East Zone Radiant Water Inlet Node,                      !Comp1 Inlet Node Name
   EAST ZONE_East Zone Radiant Water Outlet Node,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   NORTH ZONE_Zone 3 Radiant Branch,                      !Branch Name
   autosize,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   ZoneHVAC:LowTemperatureRadiant:ConstantFlow,                      !Comp1 Type
   NORTH ZONE_North Zone Radiant Floor,                      !Comp1 Name
   NORTH ZONE_North Zone Radiant Water Inlet Node,                      !Comp1 Inlet Node Name
   NORTH ZONE_North Zone Radiant Water Outlet Node,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   Reheat Bypass Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Reheat Bypass,                         !Comp1 Name
   Reheat Bypass Inlet Node,                         !Comp1 Inlet Node Name
   Reheat Bypass Outlet Node,                         !Comp1 Outlet Node Name
   BYPASS;                         !Comp1 Branch Control Type
Branch,
   West Zone_Zone 1 Cooling Branch,                      !Branch Name
   0.001,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   ZoneHVAC:LowTemperatureRadiant:ConstantFlow,                      !Comp1 Type
   West Zone_West Zone Radiant Floor,                      !Comp1 Name
   West Zone_Zone 1 Cooling Water Inlet Node,                      !Comp1 Inlet Node Name
   West Zone_Zone 1 Cooling Water Outlet Node,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   EAST ZONE_Zone 2 Cooling Branch,                      !Branch Name
   0.001,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   ZoneHVAC:LowTemperatureRadiant:ConstantFlow,                      !Comp1 Type
   EAST ZONE_East Zone Radiant Floor,                      !Comp1 Name
   EAST ZONE_Zone 2 Cooling Water Inlet Node,                      !Comp1 Inlet Node Name
   EAST ZONE_Zone 2 Cooling Water Outlet Node,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   NORTH ZONE_Zone 3 Cooling Branch,                      !Branch Name
   0.001,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   ZoneHVAC:LowTemperatureRadiant:ConstantFlow,                      !Comp1 Type
   NORTH ZONE_North Zone Radiant Floor,                      !Comp1 Name
   NORTH ZONE_Zone 3 Cooling Water Inlet Node,                      !Comp1 Inlet Node Name
   NORTH ZONE_Zone 3 Cooling Water Outlet Node,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
ConnectorList,
   Cooling Supply Side Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   CW Loop Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   CW Loop Mixer;                         !Name of Connector 2
ConnectorList,
   Cooling Demand Side Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   CW Demand Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   CW Demand Mixer;                         !Name of Connector 2
ConnectorList,
   Condenser Supply Side Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   Condenser Supply Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   Condenser Supply Mixer;                         !Name of Connector 2
ConnectorList,
   Condenser Demand Side Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   Condenser Demand Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   Condenser Demand Mixer;                         !Name of Connector 2
ConnectorList,
   Heating Supply Side Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   Heating Supply Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   Heating Supply Mixer;                         !Name of Connector 2
ConnectorList,
   Heating Demand Side Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   Reheat Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   Reheat Mixer;                         !Name of Connector 2
PlantEquipmentOperationSchemes,
   CW Loop Operation,                         !PlantOperationSchemeName
   PlantEquipmentOperation:CoolingLoad,                         !KEY--Control Scheme 1
   Peak Operation,                         !Control Scheme Name 1
   ON PEAK,                         !Control Scheme Schedule 1
   PlantEquipmentOperation:CoolingLoad,                         !KEY--Control Scheme 2
   Off Peak Operation,                         !Control Scheme Name 2
   OFF PEAK;                         !Control Scheme Schedule 2
PlantEquipmentOperationSchemes,
   Hot Loop Operation,                         !PlantOperationSchemeName
   PlantEquipmentOperation:HeatingLoad,                         !KEY--Control Scheme 1
   Purchased Only,                         !Control Scheme Name 1
   ON;                         !Control Scheme Schedule 1
CondenserEquipmentOperationSchemes,
   Tower Loop Operation,                         !CondenserOperationSchemeName
   PlantEquipmentOperation:CoolingLoad,                         !KEY--Control Scheme 1
   Year Round Tower Operation,                         !Control Scheme Name 1
   ON;                         !Control Scheme Schedule 1
PlantEquipmentOperation:CoolingLoad,
   Peak Operation,                         !Name
   0,                         !Load Range Lower Limit 1
   70000,                         !Load Range Upper Limit 1
   Chiller Plant,                         !Priority Control Equip List Name 1
   70000,                         !Load Range Lower Limit 2
   245000,                         !Load Range Upper Limit 2
   Chiller Plant and Purchased,                         !Priority Control Equip List Name 2
   245000,                         !Load Range Lower Limit 3
   500000,                         !Load Range Upper Limit 3
   Purchased Only;                         !Priority Control Equip List Name 3
PlantEquipmentOperation:CoolingLoad,
   Off Peak Operation,                         !Name
   0,                         !Load Range Lower Limit 1
   900000,                         !Load Range Upper Limit 1
   All Chillers;                         !Priority Control Equip List Name 1
PlantEquipmentOperation:CoolingLoad,
   Year Round Tower Operation,                         !Name
   0,                         !Load Range Lower Limit 1
   900000,                         !Load Range Upper Limit 1
   All Towers;                         !Priority Control Equip List Name 1
PlantEquipmentOperation:HeatingLoad,
   Purchased Only,                         !Name
   0,                         !Load Range Lower Limit 1
   1000000,                         !Load Range Upper Limit 1
   heating plant;                         !Priority Control Equip List Name 1
ZoneHVAC:EquipmentList,
   West Zone_Zone1Equipment,                      !Name
   ZoneHVAC:LowTemperatureRadiant:ConstantFlow,                      !KEY--Zone Equipment Type 1
   West Zone_West Zone Radiant Floor,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   EAST ZONE_Zone2Equipment,                      !Name
   ZoneHVAC:LowTemperatureRadiant:ConstantFlow,                      !KEY--Zone Equipment Type 1
   EAST ZONE_East Zone Radiant Floor,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   NORTH ZONE_Zone3Equipment,                      !Name
   ZoneHVAC:LowTemperatureRadiant:ConstantFlow,                      !KEY--Zone Equipment Type 1
   NORTH ZONE_North Zone Radiant Floor,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
PlantEquipmentList,
   Chiller Plant,                         !Equip List Name
   Chiller:ConstantCOP,                         !KEY--Plant Equip 1
   Little Chiller;                         !Equip Name 1
PlantEquipmentList,
   Chiller Plant and Purchased,                         !Equip List Name
   CHILLER:ELECTRIC,                         !KEY--Plant Equip 1
   Big Chiller,                         !Equip Name 1
   DistrictCooling,                         !KEY--Plant Equip 2
   Purchased Cooling;                         !Equip Name 2
PlantEquipmentList,
   Purchased Only,                         !Equip List Name
   DistrictCooling,                         !KEY--Plant Equip 1
   Purchased Cooling;                         !Equip Name 1
PlantEquipmentList,
   All Chillers,                         !Equip List Name
   CHILLER:ELECTRIC,                         !KEY--Plant Equip 1
   Big Chiller,                         !Equip Name 1
   Chiller:ConstantCOP,                         !KEY--Plant Equip 2
   Little Chiller;                         !Equip Name 2
PlantEquipmentList,
   heating plant,                         !Equip List Name
   DistrictHeating,                         !KEY--Plant Equip 1
   Purchased Heating;                         !Equip Name 1
CondenserEquipmentList,
   All Towers,                         !Equip List Name
   COOLINGTOWER:SINGLESPEED,                         !KEY--Condenser Equip 1
   Big Tower;                         !Equip Name 1
CONTROLLER:WaterCoil,
   Main Cooling Coil Controller,                         !Name
   Temperature,                         !Control variable
   REVERSE,                         !Action
   Flow,                         !Actuator variable
   ,                         !Control_Node
   ,                         !Actuator_Node
   0.1,                         !Controller Convergence Tolerance
   0.0011,                         !Max Actuated Flow
   0;                         !Min Actuated Flow
ZoneHVAC:LowTemperatureRadiant:SurfaceGroup,
   SurfaceGroup1,                         !name of this list of surfaces
   Zn001:Flr001,                         !surface name 1
   1;                         !flow fraction for surface 1
ZoneHVAC:LowTemperatureRadiant:SurfaceGroup,
   SurfaceGroup3,                         !name of this list of surfaces
   Zn003:Flr001,                         !surface name 1
   1;                         !flow fraction for surface 1
ZoneHVAC:LowTemperatureRadiant:SurfaceGroup,
   SurfaceGroup2,                         !name of this list of surfaces
   Zn002:Flr001,                         !surface name 1
   1;                         !flow fraction for surface 1
SetpointManager:Scheduled,
   Chilled Water Loop Setpoint Manager,                         !Name
   Temperature,                         !Control variable
   CW LOOP TEMP SCHEDULE,                         !Schedule Name
   Chilled Water Loop Setpoint Node List;                         !Name of the set point Node or Node List
SetpointManager:Scheduled,
   Hot Water Loop Setpoint Manager,                         !Name
   Temperature,                         !Control variable
   HW LOOP TEMP SCHEDULE,                         !Schedule Name
   Hot Water Loop Setpoint Node List;                         !Name of the set point Node or Node List
SetpointManager:Scheduled,
   COND Loop Setpoint Manager,                         !Name
   Temperature,                         !Control variable
   COND Loop TEMP Schedule,                         !Schedule Name
   COND Loop Setpoint nodelist;                         !Name of the set point Node or Node List
Sizing:Plant,
   Chilled Water Loop,                         !name of a PLANT LOOP or CONDENSER LOOP object
   Cooling,                         !loop type
   7,                         !Design loop exit temperature
   5;                         !Design loop delta T
Sizing:System,
   Air Loop,                         !name of an AIR PRIMARY LOOP object
   sensible,                         !type of load to size on
   autosize,                         !Design (minimum) outside air volumetric flow rate
   1,                         !minimum system air flow ratio
   7.2,                         !Preheat design temperature
   0.008,                         !Preheat design humidity ratio
   11,                         !Precool design temperature
   0.008,                         !Precool design humidity ratio
   17,                         !Central cooling design supply air temperature
   25,                         !Central heating design supply air temperature
   noncoincident,                         !Sizing Option
   no,                         !Cooling 100% Outside Air
   no,                         !Heating 100% Outside Air
   0.008,                         !Central cooling design supply air humidity ratio
   0.016,                         !Central heating design supply air humidity ratio
   designday,                         !Central heating design supply air humidity ratio
   ,                         !cooling design air flow rate
   designday,                         !heating design air flow method
   ;                         !heating design air flow rate
Sizing:Zone,
   EAST ZONE,                         !Name of a zone
   17,                         !Zone cooling design supply air temperature
   25,                         !Zone heating design supply air temperature
   0.0116,                         !Zone cooling design supply air humidity ratio
   0.008,                         !Zone heating design supply air humidity ratio
   flow/person,                         !outside air method
   0.0056,                         !outside air flow per person
   ,                         !outside air flow per zone area
   ,                         !outside air flow per zone
   1,                         !zone heating sizing factor
   1.2,                         !zone cooling sizing factor
   DesignDay,                         !cooling design air flow method
   ,                         !cooling design air flow rate
   0.000762,                         !cooling min air flow per zone area
   ,                         !cooling min air flow
   ,                         !cooling min air flow fraction
   designday,                         !heating design air flow method
   ,                         !heating design air flow rate
   0.002032,                         !heating max air flow per zone area
   0.1415762,                         !heating max air flow
   0.3;                         !heating max air flow fraction
Sizing:Zone,
   NORTH ZONE,                         !Name of a zone
   17,                         !Zone cooling design supply air temperature
   25,                         !Zone heating design supply air temperature
   0.0016,                         !Zone cooling design supply air humidity ratio
   0.008,                         !Zone heating design supply air humidity ratio
   flow/person,                         !outside air method
   0.0056,                         !outside air flow per person
   ,                         !outside air flow per zone area
   ,                         !outside air flow per zone
   1,                         !zone heating sizing factor
   1.2,                         !zone cooling sizing factor
   designday,                         !cooling design air flow method
   ,                         !cooling design air flow rate
   0.000762,                         !cooling min air flow per zone area
   ,                         !cooling min air flow
   ,                         !cooling min air flow fraction
   designday,                         !heating design air flow method
   ,                         !heating design air flow rate
   0.002032,                         !heating max air flow per zone area
   0.1415762,                         !heating max air flow
   0.3;                         !heating max air flow fraction
Sizing:Zone,
   West Zone,                         !Name of a zone
   17,                         !Zone cooling design supply air temperature
   25,                         !Zone heating design supply air temperature
   0.0016,                         !Zone cooling design supply air humidity ratio
   0.008,                         !Zone heating design supply air humidity ratio
   flow/person,                         !outside air method
   0.0056,                         !outside air flow per person
   ,                         !outside air flow per zone area
   ,                         !outside air flow per zone
   1,                         !zone heating sizing factor
   1.2,                         !zone cooling sizing factor
   designday,                         !cooling design air flow method
   ,                         !cooling design air flow rate
   0.000762,                         !cooling min air flow per zone area
   ,                         !cooling min air flow
   ,                         !cooling min air flow fraction
   designday,                         !heating design air flow method
   ,                         !heating design air flow rate
   0.002032,                         !heating max air flow per zone area
   0.1415762,                         !heating max air flow
   0.3;                         !heating max air flow fraction
ZoneHVAC:EquipmentConnections,
   West Zone,                      !Zone Name
   West Zone_Zone1Equipment,                      !List Name: Zone Equipment
   ,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   West Zone_Zone 1 Node,                      !Zone Air Node Name
   West Zone_Zone 1 Outlet Node;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   EAST ZONE,                      !Zone Name
   EAST ZONE_Zone2Equipment,                      !List Name: Zone Equipment
   ,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   EAST ZONE_Zone 2 Node,                      !Zone Air Node Name
   EAST ZONE_Zone 2 Outlet Node;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   NORTH ZONE,                      !Zone Name
   NORTH ZONE_Zone3Equipment,                      !List Name: Zone Equipment
   ,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   NORTH ZONE_Zone 3 Node,                      !Zone Air Node Name
   NORTH ZONE_Zone 3 Outlet Node;                      !Zone Return Air Node Name
CHILLER:ELECTRIC,
   Big Chiller,                         !Chiller Name
   WaterCooled,                         !Condenser Type
   45000,                         !Nominal Capacity
   2.75,                         !COP
   Big Chiller Inlet Node,                         !Plant_Side_Inlet_Node
   Big Chiller Outlet Node,                         !Plant_Side_Outlet_Node
   Big Chiller Condenser Inlet Node,                         !Condenser_Side_Inlet_Node
   Big Chiller Condenser Outlet Node,                         !Condenser_Side_Outlet_Node
   0.15,                         !Minimum Part Load Ratio
   1,                         !Maximum Part Load Ratio
   0.65,                         !Opt Part Load Ratio
   29.44,                         !Temp Design Condenser Inlet
   2.682759,                         !Temp Rise Coefficient
   6.667,                         !Temp Design Evaporator Outlet
   0.0011,                         !Design Evaporator Volumetric Water Flow Rate
   0.0005,                         !Design Condenser Volumetric Water Flow Rate
   0.944836,                         !Coefficient1 of the capacity ratio curve
   -0.0570088,                         !Coefficient2 of the capacity ratio curve
   -0.00185486,                         !Coefficient3 of the capacity ratio curve
   1.907846,                         !Coefficient1 of the power ratio curve
   -1.204987,                         !Coefficient2 of the power ratio curve
   0.2634623,                         !Coefficient3 of the power ratio curve
   0.03303,                         !Coefficient1 of the full load ratio curve
   0.6852,                         !Coefficient2 of the full load ratio curve
   0.2818,                         !Coefficient3 of the full load ratio curve
   5,                         !Temp Lower Limit Evaporator Outlet
   VariableFlow,                         !Chiller Flow Mode
   ,                         !Design heat recovery water flow rate
   ,                         !Heat_Recovery_Side_Inlet_Node
   ,                         !Heat_Recovery_Side_Outlet_Node
   ,                         !Sizing Factor
   ,                         !Basin Heater Capacity
   ,                         !Basin Heater Setpoint Temperature
   ;                         !Basin Heater Operating Schedule Name
Chiller:ConstantCOP,
   Little Chiller,                         !Chiller Name
   25000,                         !Nominal Capacity
   2.5,                         !COP
   0.0011,                         !Design Evaporator Volumetric Water Flow Rate
   0.0011,                         !Design Condenser Volumetric Water Flow Rate
   Little Chiller Inlet Node,                         !Plant_Side_Inlet_Node
   Little Chiller Outlet Node,                         !Plant_Side_Outlet_Node
   Little Chiller Condenser Inlet Node,                         !Condenser_Side_Inlet_Node
   Little Chiller Condenser Outlet Node,                         !Condenser_Side_Outlet_Node
   WaterCooled,                         !Condenser Type
   VariableFlow,                         !Chiller Flow Mode
   ,                         !Sizing Factor
   ,                         !Basin Heater Capacity
   ,                         !Basin Heater Setpoint Temperature
   ;                         !Basin Heater Operating Schedule Name
COOLINGTOWER:SINGLESPEED,
   Big Tower,                         !Tower Name
   Condenser Tower Inlet Node,                         !Water Inlet Node Name
   Condenser Tower Outlet Node,                         !Water Outlet Node Name
   0.0011,                         !Design Water Flow Rate
   16,                         !Design Air Flow Rate
   1000,                         !Fan Power at Design Air Flow Rate
   1750,                         !Tower UA Value at Design Air Flow Rate
   ,                         !Air Flow Rate in Free Convection Regime
   0,                         !Tower UA Value at Free Convection Air Flow Rate
   UFactorTimesAreaAndDesignWaterFlowRate,                         !Tower Performance Input Method
   ,                         !Tower Nominal Capacity
   ,                         !Tower Free Convection Capacity
   0.0,                         !Basin Heater Capacity
   2.0,                         !Basin Heater Setpoint Temperature
   ,                         !Basin Heater Operating Schedule Name
   ,                         !Evaporation Loss Mode
   ,                         !Evaporation Loss Factor
   ,                         !Drift Loss Percent
   ,                         !Blowdown Calculation Mode
   ,                         !Blowdown Concentration Ratio
   ,                         !Schedule Name for Makeup Water Usage due to Blowdown 
   ,                         !Name of Water Storage Tank for Supply
   ,                         !Outdoor Air Inlet Node Name
   FanCycling,                         !Capacity Control
   1,                         !Number of Cells
   MinimalCell,                         !Cell Control
   0.33,                         !Cell Minimum  Water Flow Rate Fraction
   2.5,                         !Cell Maximum Water Flow Rate Fraction
   1.0;                         !Sizing Factor
DistrictCooling,
   Purchased Cooling,                         !Purchased Chilled Water Name
   Purchased Cooling Inlet Node,                         !Plant_Loop_Inlet_Node
   Purchased Cooling Outlet Node,                         !Plant_Loop_Outlet_Node
   680000;                         !Nominal Capacity
DistrictHeating,
   Purchased Heating,                         !Purchased Hot Water Name
   Purchased Heat Inlet Node,                         !Plant_Loop_Inlet_Node
   Purchased Heat Outlet Node,                         !Plant_Loop_Outlet_Node
   1000000;                         !Nominal Capacity
Pipe:Adiabatic,
   Demand Side Bypass,                         !Name
   CW Demand Bypass Inlet Node,                         !Inlet Node Name
   CW Demand Bypass Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Heating Supply Side Bypass,                         !Name
   Heating Supply Bypass Inlet Node,                         !Inlet Node Name
   Heating Supply Bypass Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Reheat Bypass,                         !Name
   Reheat Bypass Inlet Node,                         !Inlet Node Name
   Reheat Bypass Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Supply Side Bypass,                         !Name
   CW Supply Bypass Inlet Node,                         !Inlet Node Name
   CW Supply Bypass Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Condenser Supply Side Bypass,                         !Name
   Cond Supply Bypass Inlet Node,                         !Inlet Node Name
   Cond Supply Bypass Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Heating Supply Outlet,                         !Name
   Heating Supply Exit Pipe Inlet Node,                         !Inlet Node Name
   HW Supply Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Reheat Inlet Pipe,                         !Name
   HW Demand Inlet Node,                         !Inlet Node Name
   HW Demand Entrance Pipe Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Reheat Outlet Pipe,                         !Name
   HW Demand Exit Pipe Inlet Node,                         !Inlet Node Name
   HW Demand Outlet Node;                         !Outlet Node Name
Pump:VariableSpeed,
   HW Circ Pump,                         !Pump Name
   HW Supply Inlet Node,                         !Inlet_Node
   HW Pump Outlet Node,                         !Outlet_Node
   0.0043,                         !Rated Volumetric Flow Rate
   300000,                         !Rated Pump Head
   2000,                         !Rated Power Consumption
   0.87,                         !Motor Efficiency
   0,                         !Fraction of Motor Inefficiencies to Fluid Stream
   0,                         !Coefficient1 of the Part Load Performance Curve
   1,                         !Coefficient2 of the Part Load Performance Curve
   0,                         !Coefficient3 of the Part Load Performance Curve
   0,                         !Coefficient4 of the Part Load Performance Curve
   0,                         !Min Flow Rate while operating in variable flow capacity
   INTERMITTENT,                         !Pump Control Type
   ;                         !Pump Flow Rate Schedule Name
Pipe:Adiabatic,
   Supply Side Outlet Pipe,                         !Name
   Supply Side Exit Pipe Inlet Node,                         !Inlet Node Name
   CW Supply Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Demand Side Inlet Pipe,                         !Name
   CW Demand Inlet Node,                         !Inlet Node Name
   CW Demand Entrance Pipe Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   CW Demand Side Outlet Pipe,                         !Name
   CW Demand Exit Pipe Inlet Node,                         !Inlet Node Name
   CW Demand Outlet Node;                         !Outlet Node Name
Pump:VariableSpeed,
   Circ Pump,                         !Pump Name
   CW Supply Inlet Node,                         !Inlet_Node
   CW Pump Outlet Node,                         !Outlet_Node
   0.0011,                         !Rated Volumetric Flow Rate
   300000,                         !Rated Pump Head
   500,                         !Rated Power Consumption
   0.87,                         !Motor Efficiency
   0,                         !Fraction of Motor Inefficiencies to Fluid Stream
   0,                         !Coefficient1 of the Part Load Performance Curve
   1,                         !Coefficient2 of the Part Load Performance Curve
   0,                         !Coefficient3 of the Part Load Performance Curve
   0,                         !Coefficient4 of the Part Load Performance Curve
   0,                         !Min Flow Rate while operating in variable flow capacity
   INTERMITTENT,                         !Pump Control Type
   ;                         !Pump Flow Rate Schedule Name
Pipe:Adiabatic,
   Condenser Supply Outlet,                         !Name
   Condenser Supply Exit Pipe Inlet Node,                         !Inlet Node Name
   Condenser Supply Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Condenser Demand Inlet Pipe,                         !Name
   Condenser Demand Inlet Node,                         !Inlet Node Name
   Condenser Demand Entrance Pipe Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Condenser Demand Outlet Pipe,                         !Name
   Condenser Demand Exit Pipe Inlet Node,                         !Inlet Node Name
   Condenser Demand Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Condenser Demand Side Bypass,                         !Name
   Cond Demand Bypass Inlet Node,                         !Inlet Node Name
   Cond Demand Bypass Outlet Node;                         !Outlet Node Name
Pump:VariableSpeed,
   Cond Circ Pump,                         !Pump Name
   Condenser Supply Inlet Node,                         !Inlet_Node
   Condenser Pump Outlet Node,                         !Outlet_Node
   0.0011,                         !Rated Volumetric Flow Rate
   300000,                         !Rated Pump Head
   500,                         !Rated Power Consumption
   0.87,                         !Motor Efficiency
   0,                         !Fraction of Motor Inefficiencies to Fluid Stream
   0,                         !Coefficient1 of the Part Load Performance Curve
   1,                         !Coefficient2 of the Part Load Performance Curve
   0,                         !Coefficient3 of the Part Load Performance Curve
   0,                         !Coefficient4 of the Part Load Performance Curve
   0,                         !Min Flow Rate while operating in variable flow capacity
   INTERMITTENT,                         !Pump Control Type
   ;                         !Pump Flow Rate Schedule Name
ZoneHVAC:LowTemperatureRadiant:ConstantFlow,
   West Zone_West Zone Radiant Floor,                      !name of constant flow (hydronic) low temperature radiant system
   RADIANTSYSAVAILSCHED,                      !availability schedule
   West Zone,                      !Zone name
   SurfaceGroup1,                      !Surface name or group
   0.012,                      !Hydronic tubing inside diameter
   400,                      !Hydronic tubing length
   MeanAirTemperature,                      !temperature control type
   0.0004,                      !Rated Volumetric Flow Rate
   ,                      !Pump Flow Rate Schedule Name
   75000,                      !Rated Pump Head
   50,                      !Rated Power Consumption
   0.87,                      !Motor Efficiency
   0.1,                      !Fraction of Motor Inefficiencies to Fluid Stream
   West Zone_West Zone Radiant Water Inlet Node,                      !heating water inlet node
   West Zone_West Zone Radiant Water Outlet Node,                      !heating water outlet node
   RADHEATHIGHWATERTEMP,                      !heating high water temperature schedule
   RADHEATLOWWATERTEMP,                      !heating low water temperature schedule
   RADHEATHIGHCONTROLTEMP,                      !heating high control temperature schedule
   RADHEATLOWCONTROLTEMP,                      !heating low control temperature schedule
   West Zone_Zone 1 Cooling Water Inlet Node,                      !cooling water inlet node
   West Zone_Zone 1 Cooling Water Outlet Node,                      !cooling water outlet node
   RADCOOLHIGHWATERTEMP,                      !cooling high water temperature schedule
   RADCOOLLOWWATERTEMP,                      !cooling low water temperature schedule
   RADCOOLHIGHCONTROLTEMP,                      !cooling high control temperature schedule
   RADCOOLLOWCONTROLTEMP,                      !cooling low control temperature schedule
   SimpleOff,                      !Condensation Control Type
   1;                      !Condensation Control Dewpoint Offset
ZoneHVAC:LowTemperatureRadiant:ConstantFlow,
   EAST ZONE_East Zone Radiant Floor,                      !name of constant flow (hydronic) low temperature radiant system
   RADIANTSYSAVAILSCHED,                      !availability schedule
   EAST ZONE,                      !Zone name
   SurfaceGroup2,                      !Surface name or group
   0.012,                      !Hydronic tubing inside diameter
   400,                      !Hydronic tubing length
   MeanAirTemperature,                      !temperature control type
   0.0004,                      !Rated Volumetric Flow Rate
   ,                      !Pump Flow Rate Schedule Name
   75000,                      !Rated Pump Head
   50,                      !Rated Power Consumption
   0.87,                      !Motor Efficiency
   0.1,                      !Fraction of Motor Inefficiencies to Fluid Stream
   EAST ZONE_East Zone Radiant Water Inlet Node,                      !heating water inlet node
   EAST ZONE_East Zone Radiant Water Outlet Node,                      !heating water outlet node
   RADHEATHIGHWATERTEMP,                      !heating high water temperature schedule
   RADHEATLOWWATERTEMP,                      !heating low water temperature schedule
   RADHEATHIGHCONTROLTEMP,                      !heating high control temperature schedule
   RADHEATLOWCONTROLTEMP,                      !heating low control temperature schedule
   EAST ZONE_Zone 2 Cooling Water Inlet Node,                      !cooling water inlet node
   EAST ZONE_Zone 2 Cooling Water Outlet Node,                      !cooling water outlet node
   RADCOOLHIGHWATERTEMP,                      !cooling high water temperature schedule
   RADCOOLHIGHWATERTEMP,                      !cooling low water temperature schedule
   RADCOOLHIGHCONTROLTEMP,                      !cooling high control temperature schedule
   RADCOOLLOWCONTROLTEMP,                      !cooling low control temperature schedule
   SimpleOff,                      !Condensation Control Type
   1;                      !Condensation Control Dewpoint Offset
ZoneHVAC:LowTemperatureRadiant:ConstantFlow,
   NORTH ZONE_North Zone Radiant Floor,                      !name of constant flow (hydronic) low temperature radiant system
   RADIANTSYSAVAILSCHED,                      !availability schedule
   NORTH ZONE,                      !Zone name
   SurfaceGroup3,                      !Surface name or group
   0.012,                      !Hydronic tubing inside diameter
   400,                      !Hydronic tubing length
   MeanAirTemperature,                      !temperature control type
   0.0005,                      !Rated Volumetric Flow Rate
   ,                      !Pump Flow Rate Schedule Name
   75000,                      !Rated Pump Head
   50,                      !Rated Power Consumption
   0.87,                      !Motor Efficiency
   0.1,                      !Fraction of Motor Inefficiencies to Fluid Stream
   NORTH ZONE_North Zone Radiant Water Inlet Node,                      !heating water inlet node
   NORTH ZONE_North Zone Radiant Water Outlet Node,                      !heating water outlet node
   RADHEATHIGHWATERTEMP,                      !heating high water temperature schedule
   RADHEATLOWWATERTEMP,                      !heating low water temperature schedule
   RADHEATHIGHCONTROLTEMP,                      !heating high control temperature schedule
   RADHEATLOWCONTROLTEMP,                      !heating low control temperature schedule
   NORTH ZONE_Zone 3 Cooling Water Inlet Node,                      !cooling water inlet node
   NORTH ZONE_Zone 3 Cooling Water Outlet Node,                      !cooling water outlet node
   RADCOOLHIGHWATERTEMP,                      !cooling high water temperature schedule
   RADCOOLLOWWATERTEMP,                      !cooling low water temperature schedule
   RADCOOLHIGHCONTROLTEMP,                      !cooling high control temperature schedule
   RADCOOLLOWCONTROLTEMP,                      !cooling low control temperature schedule
   SimpleOff,                      !Condensation Control Type
   1;                      !Condensation Control Dewpoint Offset
Connector:Splitter,
   Reheat Splitter,                         !SplitterName
   Reheat Inlet Branch,                         !Inlet Branch Name
   West Zone_Zone 1 Radiant Branch,                         !Outlet Branch Name 1
   EAST ZONE_Zone 2 Radiant Branch,                         !Outlet Branch Name 2
   NORTH ZONE_Zone 3 Radiant Branch,                         !Outlet Branch Name 3
   Reheat Bypass Branch;                         !Outlet Branch Name 4
Connector:Mixer,
   Reheat Mixer,                         !MixerName
   Reheat Outlet Branch,                         !Outlet Branch Name
   Reheat Bypass Branch,                         !Inlet Branch Name 1
   West Zone_Zone 1 Radiant Branch,                         !Inlet Branch Name 2
   EAST ZONE_Zone 2 Radiant Branch,                         !Inlet Branch Name 3
   NORTH ZONE_Zone 3 Radiant Branch;                         !Inlet Branch Name 4
Connector:Mixer,
   Heating Supply Mixer,                         !MixerName
   Heating Supply Outlet Branch,                         !Outlet Branch Name
   Heating Purchased Hot Water Branch,                         !Inlet Branch Name 1
   Heating Supply Bypass Branch;                         !Inlet Branch Name 2
Connector:Splitter,
   Heating Supply Splitter,                         !SplitterName
   Heating Supply Inlet Branch,                         !Inlet Branch Name
   Heating Purchased Hot Water Branch,                         !Outlet Branch Name 1
   Heating Supply Bypass Branch;                         !Outlet Branch Name 2
Connector:Splitter,
   CW Loop Splitter,                         !SplitterName
   CW Pump Branch,                         !Inlet Branch Name
   Big Chiller Branch,                         !Outlet Branch Name 1
   Little Chiller Branch,                         !Outlet Branch Name 2
   Purchased Cooling Branch,                         !Outlet Branch Name 3
   Supply Bypass Branch;                         !Outlet Branch Name 4
Connector:Mixer,
   CW Loop Mixer,                         !MixerName
   Cooling Supply Outlet,                         !Outlet Branch Name
   Big Chiller Branch,                         !Inlet Branch Name 1
   Little Chiller Branch,                         !Inlet Branch Name 2
   Purchased Cooling Branch,                         !Inlet Branch Name 3
   Supply Bypass Branch;                         !Inlet Branch Name 4
Connector:Mixer,
   CW Demand Mixer,                         !MixerName
   Cooling Demand Outlet,                         !Outlet Branch Name
   Demand Bypass Branch,                         !Inlet Branch Name 1
   West Zone_Zone 1 Cooling Branch,                         !Inlet Branch Name 2
   EAST ZONE_Zone 2 Cooling Branch,                         !Inlet Branch Name 3
   NORTH ZONE_Zone 3 Cooling Branch;                         !Inlet Branch Name 4
Connector:Splitter,
   CW Demand Splitter,                         !SplitterName
   Cooling Demand Inlet,                         !Inlet Branch Name
   Demand Bypass Branch,                         !Outlet Branch Name 1
   West Zone_Zone 1 Cooling Branch,                         !Outlet Branch Name 2
   EAST ZONE_Zone 2 Cooling Branch,                         !Outlet Branch Name 3
   NORTH ZONE_Zone 3 Cooling Branch;                         !Outlet Branch Name 4
Connector:Splitter,
   Condenser Supply Splitter,                         !SplitterName
   Condenser Supply Inlet Branch,                         !Inlet Branch Name
   Condenser Supply Tower Branch,                         !Outlet Branch Name 1
   Condenser Supply Bypass Branch;                         !Outlet Branch Name 2
Connector:Mixer,
   Condenser Supply Mixer,                         !MixerName
   Condenser Supply Outlet Branch,                         !Outlet Branch Name
   Condenser Supply Tower Branch,                         !Inlet Branch Name 1
   Condenser Supply Bypass Branch;                         !Inlet Branch Name 2
Connector:Splitter,
   Condenser Demand Splitter,                         !SplitterName
   Condenser Demand Inlet Branch,                         !Inlet Branch Name
   Big Chiller Condenser Branch,                         !Outlet Branch Name 1
   Little Chiller Condenser Branch,                         !Outlet Branch Name 2
   Condenser Demand Bypass Branch;                         !Outlet Branch Name 3
Connector:Mixer,
   Condenser Demand Mixer,                         !MixerName
   Condenser Demand Outlet Branch,                         !Outlet Branch Name
   Big Chiller Condenser Branch,                         !Inlet Branch Name 1
   Little Chiller Condenser Branch,                         !Inlet Branch Name 2
   Condenser Demand Bypass Branch;                         !Inlet Branch Name 3

