NodeList,
   West Zone_Zone1Inlets,                      !Node List Name
   West Zone_Zone 1 Inlet Node;                      !Node_ID_1
NodeList,
   EAST ZONE_Zone2Inlets,                      !Node List Name
   EAST ZONE_Zone 2 Inlet Node;                      !Node_ID_1
NodeList,
   NORTH ZONE_Zone3Inlets,                      !Node List Name
   NORTH ZONE_Zone 3 Inlet Node;                      !Node_ID_1
NodeList,
   West Zone List,                         !Node List Name
   Zone 1 Node;                         !Node_ID_1
NodeList,
   East Zone List,                         !Node List Name
   Zone 2 Node;                         !Node_ID_1
NodeList,
   North Zone List,                         !Node List Name
   Zone 3 Node;                         !Node_ID_1
BranchList,
   Air Loop Branches,                         !Branch List Name
   Air Loop Main Branch;                         !Branch Name 1
AirLoopHVAC,
   Typical Terminal Reheat 1,                         !Primary Air Loop Name
   ,                         !Name: Controller List
   Heat Pump 1 Avail List,                         !Name: System Availability Manager List
   autosize,                         !Primary air design volumetric flow rate
   Air Loop Branches,                         !Air Loop Branch List Name
   ,                         !Air Loop Connector List Name
   Outdoor Air Mixer Inlet Node,                         !ReturnAir AirLoop Inlet Node
   Return Air Mixer Outlet,                         !ZoneEquipGroup Outlet Node
   Zone Equipment Inlet Node,                         !SupplyAirPath ZoneEquipGroup Inlet Nodes
   Air Loop Outlet Node;                         !AirLoop Outlet Nodes
AirLoopHVAC:SupplyPath,
   HeatPumpSupplyPath,                         !Name
   Zone Equipment Inlet Node,                         !Supply Air Path Inlet Node Name
   AirLoopHVAC:ZoneSplitter,                         !Component 1 Object Type
   Zone Supply Air Splitter;                         !Component 1 Name
AirLoopHVAC:ReturnPath,
   HeatPumpReturnPath,                         !Name
   Return Air Mixer Outlet,                         !Return Air Path Outlet Node Name
   AirLoopHVAC:ZoneMixer,                         !Component 1 Object Type
   Zone Return Air Mixer;                         !Component 1 Name
Branch,
   Air Loop Main Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   AirLoopHVAC:OutdoorAirSystem,                         !Comp1 Type
   OA Sys 1,                         !Comp1 Name
   Outdoor Air Mixer Inlet Node,                         !Comp1 Inlet Node Name
   Mixed Air Node,                         !Comp1 Outlet Node Name
   PASSIVE,                         !Comp1 Branch Control Type
   AirLoopHVAC:UnitaryHeatPump:AirToAir:MultiSpeed,                         !Comp2 Type
   DXAC Heat Pump 1,                         !Comp2 Name
   Mixed Air Node,                         !Comp2 Inlet Node Name
   Air Loop Outlet Node,                         !Comp2 Outlet Node Name
   ACTIVE;                         !Comp2 Branch Control Type
ZoneHVAC:EquipmentList,
   West Zone_Zone1Equipment,                      !Name
   AirTerminal:SingleDuct:Uncontrolled,                      !KEY--Zone Equipment Type 1
   West Zone_Zone1DirectAir,                      !Type Name 1
   1,                      !Cooling Priority 1
   2;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   EAST ZONE_Zone2Equipment,                      !Name
   AirTerminal:SingleDuct:Uncontrolled,                      !KEY--Zone Equipment Type 1
   EAST ZONE_Zone2DirectAir,                      !Type Name 1
   1,                      !Cooling Priority 1
   2;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   NORTH ZONE_Zone3Equipment,                      !Name
   AirTerminal:SingleDuct:Uncontrolled,                      !KEY--Zone Equipment Type 1
   NORTH ZONE_Zone3DirectAir,                      !Type Name 1
   1,                      !Cooling Priority 1
   2;                      !Heating Priority 1
AirLoopHVAC:OutdoorAirSystem:EquipmentList,
   OA Sys 1 Equipment,                         !Name
   OutdoorAir:Mixer,                         !KEY--System Component 1
   OA Mixing Box 1;                         !Component Name 1
AirLoopHVAC:ControllerList,
   OA Sys 1 Controllers,                         !Name
   Controller:OutdoorAir,                         !Controller Type 1
   OA Controller 1;                         !Controller Name 1
Controller:OutdoorAir,
   OA Controller 1,                         !Name
   Relief Air Outlet Node,                         !Relief Air Outlet Node Name
   Outdoor Air Mixer Inlet Node,                         !Return Air Node Name
   Mixed Air Node,                         !Mixed Air Node Name
   Outside Air Inlet Node,                         !Actuator Node Name
   0.51,                         !Minimum Outdoor Air Flow Rate
   1.7,                         !Maximum Outdoor Air Flow Rate
   NoEconomizer,                         !Economizer Control Type
   ModulateFlow,                         !Economizer Control Action Type
   ,                         !Economizer Maximum Limit Dry-Bulb Temperature
   ,                         !Economizer Maximum Limit Enthalpy
   ,                         !Economizer Maximum Limit Dewpoint Temperature
   ,                         !Electronic Enthalpy Limit Curve Name
   ,                         !Economizer Minimum Limit Dry-Bulb Temperature
   NoLockout,                         !Lockout Type
   FixedMinimum,                         !Minimum Limit Type
   OAFractionSched,                         !Minimum Outdoor Air Schedule Name
   ,                         !Minimum Fraction of Outdoor Air Schedule Name
   ,                         !Maximum Fraction of Outdoor Air Schedule Name
   ,                         !Mechanical Ventilation Controller Name
   ,                         !Time of Day Economizer Control Schedule Name
   ,                         !High Humidity Control
   ,                         !Humidistat Control Zone Name
   ,                         !High Humidity Outdoor Air Flow Ratio
   ,                         !Control High Indoor Humidity Based on Outdoor Humidity Ratio
   ;                         !Heat Recovery Bypass Control Type
AvailabilityManagerAssignmentList,
   Heat Pump 1 Avail List,                         !Name
   AvailabilityManager:Scheduled,                         !System Availability Manager Type 1
   Heat Pump 1 Avail;                         !System Availability Manager Name 1
AvailabilityManagerAssignmentList,
   Outdoor Air 1 Avail List,                         !Name
   AvailabilityManager:Scheduled,                         !System Availability Manager Type 1
   Outdoor Air 1 Avail;                         !System Availability Manager Name 1
AvailabilityManager:Scheduled,
   Heat Pump 1 Avail,                         !Name
   FanAndCoilAvailSched;                         !Schedule name
AvailabilityManager:Scheduled,
   Outdoor Air 1 Avail,                         !Name
   OutdoorAirAvailSched;                         !Schedule name
OutdoorAir:Node,
   Outdoor Condenser Air Node,                         !Node Name
   1;                         !Height Above Ground
OutdoorAir:NodeList,
   Outside Air Inlet Node;                         !1st Node name or node list name
ThermostatSetpoint:SingleHeating,
   Heating Setpoint with SB,                         !Name
   Heating Setpoints;                         !Setpoint Temperature SCHEDULE Name
ThermostatSetpoint:SingleCooling,
   Cooling Setpoint with SB,                         !Name
   Cooling Setpoints;                         !Setpoint Temperature SCHEDULE Name
Sizing:System,
   Typical Terminal Reheat 1,                         !name of an AIR PRIMARY LOOP object
   sensible,                         !type of load to size on
   autosize,                         !Design (minimum) outside air volumetric flow rate
   0.1,                         !minimum system air flow ratio
   30,                         !Preheat design temperature
   0.008,                         !Preheat design humidity ratio
   10,                         !Precool design temperature
   0.001,                         !Precool design humidity ratio
   5,                         !Central cooling design supply air temperature
   35,                         !Central heating design supply air temperature
   noncoincident,                         !Sizing Option
   no,                         !Cooling 100% Outside Air
   no,                         !Heating 100% Outside Air
   0.008,                         !Central cooling design supply air humidity ratio
   0.008,                         !Central heating design supply air humidity ratio
   designday,                         !Central heating design supply air humidity ratio
   0,                         !cooling design air flow rate
   designday,                         !heating design air flow method
   0;                         !heating design air flow rate
Sizing:Zone,
   EAST ZONE,                         !Name of a zone
   10,                         !Zone cooling design supply air temperature
   20,                         !Zone heating design supply air temperature
   0.009,                         !Zone cooling design supply air humidity ratio
   0.004,                         !Zone heating design supply air humidity ratio
   flow/person,                         !outside air method
   0.00944,                         !outside air flow per person
   0,                         !outside air flow per zone area
   0,                         !outside air flow per zone
   0,                         !zone heating sizing factor
   0,                         !zone cooling sizing factor
   DesignDay,                         !cooling design air flow method
   0,                         !cooling design air flow rate
   0.000762,                         !cooling min air flow per zone area
   0,                         !cooling min air flow
   0,                         !cooling min air flow fraction
   DesignDay,                         !heating design air flow method
   0,                         !heating design air flow rate
   0.002032,                         !heating max air flow per zone area
   0.1415762,                         !heating max air flow
   0.3;                         !heating max air flow fraction
Sizing:Zone,
   NORTH ZONE,                         !Name of a zone
   10,                         !Zone cooling design supply air temperature
   50,                         !Zone heating design supply air temperature
   0.009,                         !Zone cooling design supply air humidity ratio
   0.005,                         !Zone heating design supply air humidity ratio
   flow/person,                         !outside air method
   0.00944,                         !outside air flow per person
   0,                         !outside air flow per zone area
   0,                         !outside air flow per zone
   0,                         !zone heating sizing factor
   0,                         !zone cooling sizing factor
   designday,                         !cooling design air flow method
   0,                         !cooling design air flow rate
   0.000762,                         !cooling min air flow per zone area
   0,                         !cooling min air flow
   0,                         !cooling min air flow fraction
   designday,                         !heating design air flow method
   0,                         !heating design air flow rate
   0.002032,                         !heating max air flow per zone area
   0.1415762,                         !heating max air flow
   0.3;                         !heating max air flow fraction
Sizing:Zone,
   West Zone,                         !Name of a zone
   10,                         !Zone cooling design supply air temperature
   50,                         !Zone heating design supply air temperature
   0.009,                         !Zone cooling design supply air humidity ratio
   0.004,                         !Zone heating design supply air humidity ratio
   flow/person,                         !outside air method
   0.00944,                         !outside air flow per person
   0,                         !outside air flow per zone area
   0,                         !outside air flow per zone
   0,                         !zone heating sizing factor
   0,                         !zone cooling sizing factor
   designday,                         !cooling design air flow method
   0,                         !cooling design air flow rate
   0.000762,                         !cooling min air flow per zone area
   0,                         !cooling min air flow
   0,                         !cooling min air flow fraction
   DesignDay,                         !heating design air flow method
   0,                         !heating design air flow rate
   0.002032,                         !heating max air flow per zone area
   0.1415762,                         !heating max air flow
   0.3;                         !heating max air flow fraction
ZoneControl:Thermostat,
   Zone 2 Thermostat,                         !Thermostat Name
   EAST ZONE,                         !Zone Name
   Zone Control Type Sched,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:SingleHeating,                         !Control Type #1
   Heating Setpoint with SB,                         !Control Type Name #1
   ThermostatSetpoint:SingleCooling,                         !Control Type #2
   Cooling Setpoint with SB;                         !Control Type Name #2
ZoneControl:Thermostat,
   Zone 1 Thermostat,                         !Thermostat Name
   West Zone,                         !Zone Name
   Zone Control Type Sched,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:SingleHeating,                         !Control Type #1
   Heating Setpoint with SB,                         !Control Type Name #1
   ThermostatSetpoint:SingleCooling,                         !Control Type #2
   Cooling Setpoint with SB;                         !Control Type Name #2
ZoneControl:Thermostat,
   Zone 3 Thermostat,                         !Thermostat Name
   NORTH ZONE,                         !Zone Name
   Zone Control Type Sched,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:SingleHeating,                         !Control Type #1
   Heating Setpoint with SB,                         !Control Type Name #1
   ThermostatSetpoint:SingleCooling,                         !Control Type #2
   Cooling Setpoint with SB;                         !Control Type Name #2
CURVE:QUADRATIC,
   HPACHeatEIRFF Speed 1,                         !Name
   1.3824,                         !Coeff1 Constant
   -0.4336,                         !Coeff2 x
   0.0512,                         !Coeff3 x**2
   0,                         !minimum value of x
   1,                         !maximum value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
CURVE:QUADRATIC,
   HPACHeatEIRFF Speed 2,                         !Name
   1.3824,                         !Coeff1 Constant
   -0.4336,                         !Coeff2 x
   0.0512,                         !Coeff3 x**2
   0,                         !minimum value of x
   1,                         !maximum value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
CURVE:QUADRATIC,
   HPACHeatEIRFF Speed 3,                         !Name
   1.3824,                         !Coeff1 Constant
   -0.4336,                         !Coeff2 x
   0.0512,                         !Coeff3 x**2
   0,                         !minimum value of x
   1,                         !maximum value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
CURVE:QUADRATIC,
   HPACHeatEIRFF Speed 4,                         !Name
   1.3824,                         !Coeff1 Constant
   -0.4336,                         !Coeff2 x
   0.0512,                         !Coeff3 x**2
   0,                         !minimum value of x
   1,                         !maximum value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
Curve:Cubic,
   HPACHeatCapFT Speed 1,                         !Name 
   0.758746,                         !Coefficient1 Constant
   0.027626,                         !Coefficient2 x 
   0.00148716,                         !Coefficient3 x**2
   0.0000034992,                         !Coefficient4 x**3
   -20,                         !Minimum Value of x 
   20,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Dimensionless;                         !Output Unit Type
Curve:Cubic,
   HPACHeatCapFT Speed 2,                         !Name 
   0.758746,                         !Coefficient1 Constant
   0.027662,                         !Coefficient2 x 
   0.00148716,                         !Coefficient3 x**2
   0.0000034992,                         !Coefficient4 x**3
   -20,                         !Minimum Value of x 
   20,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Dimensionless;                         !Output Unit Type
Curve:Cubic,
   HPACHeatCapFT Speed 3,                         !Name 
   0.758746,                         !Coefficient1 Constant
   0.027626,                         !Coefficient2 x 
   0.00148716,                         !Coefficient3 x**2
   0.0000034992,                         !Coefficient4 x**3
   -20,                         !Minimum Value of x 
   20,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Dimensionless;                         !Output Unit Type
Curve:Cubic,
   HPACHeatCapFT Speed 4,                         !Name 
   0.758746,                         !Coefficient1 Constant
   0.027626,                         !Coefficient2 x 
   0.00148716,                         !Coefficient3 x**2
   0.0000034992,                         !Coefficient4 x**3
   -20,                         !Minimum Value of x 
   20,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Dimensionless;                         !Output Unit Type
Curve:Cubic,
   HPACHeatCapFF Speed 1,                         !Name 
   0.84,                         !Coefficient1 Constant
   0.16,                         !Coefficient2 x 
   0,                         !Coefficient3 x**2
   0,                         !Coefficient4 x**3
   0.5,                         !Minimum Value of x 
   1.5,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
Curve:Cubic,
   HPACHeatCapFF Speed 2,                         !Name 
   0.84,                         !Coefficient1 Constant
   0.16,                         !Coefficient2 x 
   0,                         !Coefficient3 x**2
   0,                         !Coefficient4 x**3
   0.5,                         !Minimum Value of x 
   1.5,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
Curve:Cubic,
   HPACHeatCapFF Speed 3,                         !Name 
   0.84,                         !Coefficient1 Constant
   0.16,                         !Coefficient2 x 
   0,                         !Coefficient3 x**2
   0,                         !Coefficient4 x**3
   0.5,                         !Minimum Value of x 
   1.5,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
Curve:Cubic,
   HPACHeatCapFF Speed 4,                         !Name 
   0.84,                         !Coefficient1 Constant
   0.16,                         !Coefficient2 x 
   0,                         !Coefficient3 x**2
   0,                         !Coefficient4 x**3
   0.5,                         !Minimum Value of x 
   1.5,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
Curve:Cubic,
   HPACHeatEIRFT Speed 1,                         !Name 
   1.19248,                         !Coefficient1 Constant
   -0.0300438,                         !Coefficient2 x 
   0.00103648,                         !Coefficient3 x**2
   -0.000023328,                         !Coefficient4 x**3
   -20,                         !Minimum Value of x 
   20,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Dimensionless;                         !Output Unit Type
Curve:Cubic,
   HPACHeatEIRFT Speed 2,                         !Name 
   1.19248,                         !Coefficient1 Constant
   -0.0300438,                         !Coefficient2 x 
   0.00103748,                         !Coefficient3 x**2
   -0.000023328,                         !Coefficient4 x**3
   -20,                         !Minimum Value of x 
   20,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Dimensionless;                         !Output Unit Type
Curve:Cubic,
   HPACHeatEIRFT Speed 3,                         !Name 
   1.19248,                         !Coefficient1 Constant
   -0.0300438,                         !Coefficient2 x 
   0.00103748,                         !Coefficient3 x**2
   -0.000023328,                         !Coefficient4 x**3
   -20,                         !Minimum Value of x 
   20,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Dimensionless;                         !Output Unit Type
Curve:Cubic,
   HPACHeatEIRFT Speed 4,                         !Name 
   1.19248,                         !Coefficient1 Constant
   -0.0300438,                         !Coefficient2 x 
   0.00103748,                         !Coefficient3 x**2
   -0.000023328,                         !Coefficient4 x**3
   -20,                         !Minimum Value of x 
   20,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Dimensionless;                         !Output Unit Type
Curve:Cubic,
   HPACCoolCapFF Speed 1,                         !Name 
   0.47,                         !Coefficient1 Constant
   1.25,                         !Coefficient2 x 
   -1.04,                         !Coefficient3 x**2
   0.32,                         !Coefficient4 x**3
   0.5,                         !Minimum Value of x 
   1.5,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
Curve:Cubic,
   HPACCoolCapFF Speed 2,                         !Name 
   0.47,                         !Coefficient1 Constant
   1.25,                         !Coefficient2 x 
   -1.04,                         !Coefficient3 x**2
   0.32,                         !Coefficient4 x**3
   0.5,                         !Minimum Value of x 
   1.5,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
Curve:Cubic,
   HPACCoolCapFF Speed 3,                         !Name 
   0.47,                         !Coefficient1 Constant
   1.25,                         !Coefficient2 x 
   -1.04,                         !Coefficient3 x**2
   0.32,                         !Coefficient4 x**3
   0.5,                         !Minimum Value of x 
   1.5,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
Curve:Cubic,
   HPACCoolCapFF Speed 4,                         !Name 
   0.47,                         !Coefficient1 Constant
   1.25,                         !Coefficient2 x 
   -1.04,                         !Coefficient3 x**2
   0.32,                         !Coefficient4 x**3
   0.5,                         !Minimum Value of x 
   1.5,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
Curve:Cubic,
   HPACCOOLEIRFF Speed 1,                         !Name 
   0.47,                         !Coefficient1 Constant
   1.25,                         !Coefficient2 x 
   -1.04,                         !Coefficient3 x**2
   0.32,                         !Coefficient4 x**3
   0.5,                         !Minimum Value of x 
   1.5,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
Curve:Cubic,
   HPACCOOLEIRFF Speed 2,                         !Name 
   0.47,                         !Coefficient1 Constant
   1.25,                         !Coefficient2 x 
   -1.04,                         !Coefficient3 x**2
   0.32,                         !Coefficient4 x**3
   0.5,                         !Minimum Value of x 
   1.5,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
Curve:Cubic,
   HPACCOOLEIRFF Speed 3,                         !Name 
   0.47,                         !Coefficient1 Constant
   1.25,                         !Coefficient2 x 
   -1.04,                         !Coefficient3 x**2
   0.32,                         !Coefficient4 x**3
   0.5,                         !Minimum Value of x 
   1.5,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
Curve:Cubic,
   HPACCOOLEIRFF Speed 4,                         !Name 
   0.47,                         !Coefficient1 Constant
   1.25,                         !Coefficient2 x 
   -1.04,                         !Coefficient3 x**2
   0.32,                         !Coefficient4 x**3
   0.5,                         !Minimum Value of x 
   1.5,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HPACDefrostCAPFT,                         !Name
   1,                         !Coeff1 Constant
   0,                         !Coeff2 x
   0,                         !Coeff3 x**2
   0,                         !Coeff4 y
   0,                         !Coeff5 y**2
   0,                         !Coeff6 x*y
   0,                         !minimum value of x
   50,                         !maximum value of x
   0,                         !minimum value of y
   50,                         !maximum value of y
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HAPCHeatWHFT Speed 1,                         !Name
   1,                         !Coeff1 Constant
   0,                         !Coeff2 x
   0,                         !Coeff3 x**2
   0,                         !Coeff4 y
   0,                         !Coeff5 y**2
   0,                         !Coeff6 x*y
   0,                         !minimum value of x
   50,                         !maximum value of x
   0,                         !minimum value of y
   50,                         !maximum value of y
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HAPCHeatWHFT Speed 2,                         !Name
   1,                         !Coeff1 Constant
   0,                         !Coeff2 x
   0,                         !Coeff3 x**2
   0,                         !Coeff4 y
   0,                         !Coeff5 y**2
   0,                         !Coeff6 x*y
   0,                         !minimum value of x
   50,                         !maximum value of x
   0,                         !minimum value of y
   50,                         !maximum value of y
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HAPCHeatWHFT Speed 3,                         !Name
   1,                         !Coeff1 Constant
   0,                         !Coeff2 x
   0,                         !Coeff3 x**2
   0,                         !Coeff4 y
   0,                         !Coeff5 y**2
   0,                         !Coeff6 x*y
   0,                         !minimum value of x
   50,                         !maximum value of x
   0,                         !minimum value of y
   50,                         !maximum value of y
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HAPCHeatWHFT Speed 4,                         !Name
   1,                         !Coeff1 Constant
   0,                         !Coeff2 x
   0,                         !Coeff3 x**2
   0,                         !Coeff4 y
   0,                         !Coeff5 y**2
   0,                         !Coeff6 x*y
   0,                         !minimum value of x
   50,                         !maximum value of x
   0,                         !minimum value of y
   50,                         !maximum value of y
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HPACCoolCapFT Speed 1,                         !Name
   0.476428,                         !Coeff1 Constant
   0.0401147,                         !Coeff2 x
   0.000226411,                         !Coeff3 x**2
   -0.000827136,                         !Coeff4 y
   -0.0000073324,                         !Coeff5 y**2
   -0.000446278,                         !Coeff6 x*y
   12.77778,                         !minimum value of x
   23.88889,                         !maximum value of x
   23.88889,                         !minimum value of y
   46.11111,                         !maximum value of y
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HPACCoolCapFT Speed 2,                         !Name
   0.476428,                         !Coeff1 Constant
   0.0401147,                         !Coeff2 x
   0.000226411,                         !Coeff3 x**2
   -0.000827136,                         !Coeff4 y
   -0.0000073324,                         !Coeff5 y**2
   -0.000446278,                         !Coeff6 x*y
   12.77778,                         !minimum value of x
   23.88889,                         !maximum value of x
   23.88889,                         !minimum value of y
   46.11111,                         !maximum value of y
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HPACCoolCapFT Speed 3,                         !Name
   0.476428,                         !Coeff1 Constant
   0.0401147,                         !Coeff2 x
   0.000226411,                         !Coeff3 x**2
   -0.000827136,                         !Coeff4 y
   -0.0000073324,                         !Coeff5 y**2
   -0.000446278,                         !Coeff6 x*y
   12.77778,                         !minimum value of x
   23.88889,                         !maximum value of x
   23.88889,                         !minimum value of y
   46.11111,                         !maximum value of y
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HPACCoolCapFT Speed 4,                         !Name
   0.476428,                         !Coeff1 Constant
   0.0401147,                         !Coeff2 x
   0.000226411,                         !Coeff3 x**2
   -0.000827136,                         !Coeff4 y
   -0.0000073324,                         !Coeff5 y**2
   -0.000446278,                         !Coeff6 x*y
   12.77778,                         !minimum value of x
   23.88889,                         !maximum value of x
   23.88889,                         !minimum value of y
   46.11111,                         !maximum value of y
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HPACCOOLEIRFT Speed 1,                         !Name
   0.632475,                         !Coeff1 Constant
   -0.0121321,                         !Coeff2 x
   0.000507773,                         !Coeff3 x**2
   0.0155377,                         !Coeff4 y
   0.00027284,                         !Coeff5 y**2
   -0.000679201,                         !Coeff6 x*y
   12.77778,                         !minimum value of x
   23.88889,                         !maximum value of x
   23.88889,                         !minimum value of y
   46.11111,                         !maximum value of y
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HPACCOOLEIRFT Speed 2,                         !Name
   0.632475,                         !Coeff1 Constant
   -0.0121321,                         !Coeff2 x
   0.000507773,                         !Coeff3 x**2
   0.0155377,                         !Coeff4 y
   0.00027284,                         !Coeff5 y**2
   -0.000679201,                         !Coeff6 x*y
   12.77778,                         !minimum value of x
   23.88889,                         !maximum value of x
   23.88889,                         !minimum value of y
   46.11111,                         !maximum value of y
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HPACCOOLEIRFT Speed 3,                         !Name
   0.632475,                         !Coeff1 Constant
   -0.0121321,                         !Coeff2 x
   0.000507773,                         !Coeff3 x**2
   0.0155377,                         !Coeff4 y
   0.00027284,                         !Coeff5 y**2
   -0.000679201,                         !Coeff6 x*y
   12.77778,                         !minimum value of x
   23.88889,                         !maximum value of x
   23.88889,                         !minimum value of y
   46.11111,                         !maximum value of y
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HPACCOOLEIRFT Speed 4,                         !Name
   0.632475,                         !Coeff1 Constant
   -0.0121321,                         !Coeff2 x
   0.000507773,                         !Coeff3 x**2
   0.0155377,                         !Coeff4 y
   0.00027284,                         !Coeff5 y**2
   -0.000679201,                         !Coeff6 x*y
   12.77778,                         !minimum value of x
   23.88889,                         !maximum value of x
   23.88889,                         !minimum value of y
   46.11111,                         !maximum value of y
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HAPCCoolWHFT Speed 1,                         !Name
   1,                         !Coeff1 Constant
   0,                         !Coeff2 x
   0,                         !Coeff3 x**2
   0,                         !Coeff4 y
   0,                         !Coeff5 y**2
   0,                         !Coeff6 x*y
   0,                         !minimum value of x
   50,                         !maximum value of x
   0,                         !minimum value of y
   50,                         !maximum value of y
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HAPCCoolWHFT Speed 2,                         !Name
   1,                         !Coeff1 Constant
   0,                         !Coeff2 x
   0,                         !Coeff3 x**2
   0,                         !Coeff4 y
   0,                         !Coeff5 y**2
   0,                         !Coeff6 x*y
   0,                         !minimum value of x
   50,                         !maximum value of x
   0,                         !minimum value of y
   50,                         !maximum value of y
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HAPCCoolWHFT Speed 3,                         !Name
   1,                         !Coeff1 Constant
   0,                         !Coeff2 x
   0,                         !Coeff3 x**2
   0,                         !Coeff4 y
   0,                         !Coeff5 y**2
   0,                         !Coeff6 x*y
   0,                         !minimum value of x
   50,                         !maximum value of x
   0,                         !minimum value of y
   50,                         !maximum value of y
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HAPCCoolWHFT Speed 4,                         !Name
   1,                         !Coeff1 Constant
   0,                         !Coeff2 x
   0,                         !Coeff3 x**2
   0,                         !Coeff4 y
   0,                         !Coeff5 y**2
   0,                         !Coeff6 x*y
   0,                         !minimum value of x
   50,                         !maximum value of x
   0,                         !minimum value of y
   50,                         !maximum value of y
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
CURVE:QUADRATIC,
   HPACCOOLPLFFPLR Speed,                         !Name
   0.85,                         !Coeff1 Constant
   0.15,                         !Coeff2 x
   0,                         !Coeff3 x**2
   0,                         !minimum value of x
   1,                         !maximum value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
CURVE:QUADRATIC,
   HPACHEATPLFFPLR Speed1,                         !Name
   0.85,                         !Coeff1 Constant
   0.15,                         !Coeff2 x
   0,                         !Coeff3 x**2
   0,                         !minimum value of x
   1,                         !maximum value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
AirTerminal:SingleDuct:Uncontrolled,
   West Zone_Zone1DirectAir,                      !Direct Air Name
   FanAndCoilAvailSched,                      !Schedule name for on/off schedule
   West Zone_Zone 1 Inlet Node,                      !Zone Supply Air Node Name
   autosize;                      !Maximum air flow rate
AirTerminal:SingleDuct:Uncontrolled,
   EAST ZONE_Zone2DirectAir,                      !Direct Air Name
   FanAndCoilAvailSched,                      !Schedule name for on/off schedule
   EAST ZONE_Zone 2 Inlet Node,                      !Zone Supply Air Node Name
   autosize;                      !Maximum air flow rate
AirTerminal:SingleDuct:Uncontrolled,
   NORTH ZONE_Zone3DirectAir,                      !Direct Air Name
   FanAndCoilAvailSched,                      !Schedule name for on/off schedule
   NORTH ZONE_Zone 3 Inlet Node,                      !Zone Supply Air Node Name
   autosize;                      !Maximum air flow rate
AirLoopHVAC:UnitaryHeatPump:AirToAir:MultiSpeed,
   DXAC Heat Pump 1,                         !Name of multispeed heat pump
   FanAndCoilAvailSched,                         !Availability schedule name
   Mixed Air Node,                         !Heat pump air inlet node name
   Air Loop Outlet Node,                         !Heat pump air outlet node name
   East Zone,                         !Controlling zone or thermostat location
   Fan:OnOff,                         !Supply air fan type
   Supply Fan 1,                         !Supply air fan name
   blowthrough,                         !Supply air fan placement
   FanAndCoilAvailSched,                         !Supply air fan operating mode schedule name
   Coil:Heating:DX:MultiSpeed,                         !Heating coil type
   USMSHP_FanOnF1_HCoil,                         !Heating coil name
   -8.0,                         !Minimum outdoor dry-bulb temperature for compressor operation
   Coil:Cooling:DX:MultiSpeed,                         !Cooling coil type
   USMSHP_FanOnF1_CCoil,                         !Cooling coil name
   Coil:Heating:Electric,                         !Supplemental heating coil type
   USMSHP_FanOnF1_SHCoil,                         !Supplemental heating coil name
   50,                         !Maximum supply air temperature from supplemental heater
   21.0,                         !Maximum outdoor dry-bulb temperature for supplemental heater operation
   0,                         !Auxiliary On-Cycle Electric Power
   0,                         !Auxiliary Off-Cycle Electric Power
   0.0,                         !Design Heat Recovery Water Flow Rate
   80.0,                         !Maximum Temp for Heat Recovery
   ,                         !Heat recovery water inlet node name
   ,                         !Heat recovery water outlet node name
   0.2,                         !Supply air volumetric flow rate when no cooling or heating is needed
   4,                         !Number of speeds for heating
   4,                         !Number of speeds for cooling
   0.4,                         !Supply air volumetric flow rate during heating operation, Speed 1
   0.8,                         !Supply air volumetric flow rate during heating operation, Speed 2
   1.2,                         !Supply air volumetric flow rate during heating operation, Speed 3
   1.7,                         !Supply air volumetric flow rate during heating operation, Speed 4
   0.4,                         !Supply air volumetric flow rate during cooling operation, Speed 1
   0.8,                         !Supply air volumetric flow rate during cooling operation, Speed 2
   1.2,                         !Supply air volumetric flow rate during cooling operation, Speed 3
   1.7;                         !Supply air volumetric flow rate during cooling operation, Speed 4
FAN:OnOff,
   Supply Fan 1,                         !Fan Name
   FanAndCoilAvailSched,                         !Available Schedule
   0.7,                         !Fan Total Efficiency
   300,                         !Delta Pressure
   autosize,                         !Max Flow Rate
   0.9,                         !Motor Efficiency
   1,                         !Motor In Airstream Fraction
   Mixed Air Node,                         !Fan_Inlet_Node
   DX Cooling Coil Air Inlet Node,                         !Fan_Outlet_Node
   General;                         !End-Use Subcategory
COIL:Cooling:DX:MultiSpeed,
   USMSHP_FanOnF1_CCoil,                         !Name
   FanAndCoilAvailSched,                         !Availability Schedule
   DX Cooling Coil Air Inlet Node,                         !Air Inlet Node
   Heating Coil Air Inlet Node,                         !Air Outlet Node
   Outdoor Condenser Air Node,                         !Condenser Air Inlet Node Name
   AirCooled,                         !Condenser Type
   ,                         !Supply Water Storage Tank Name
   ,                         !Condensate Collection Water Storage Tank Name
   No,                         !Apply Part Load Fraction to Speeds greater than 1
   No,                         !Apply Latent Degradation to Speeds greater than 1
   ,                         !Crankcase Heater Capacity
   ,                         !Maximum Outdoor Dry-bulb Temperature for Crankcase Heater Operation
   ,                         !Basin Heater Capacity 
   ,                         !Basin Heater Setpoint Temperature
   ,                         !Basin Heater Operating Schedule Name
   NaturalGas,                         !Fuel Type
   4,                         !Number of speeds
   7500,                         !Speed(1)Rated Total Cooling Capacity
   0.75,                         !Speed(1)Rated Sensible Heat Ratio
   3.0,                         !Speed(1)Rated COP
   0.4,                         !Speed(1)Rated Air Volume Flow Rate
   HPACCoolCapFT Speed 1,                         !Speed(1)Total Cooling Capacity Function of Temperature Curve Name
   HPACCoolCapFF Speed 1,                         !Speed(1)Total Cooling Capacity Function of Flow Fraction Curve Name
   HPACCOOLEIRFT Speed 1,                         !Speed(1)Energy Input Ratio Function of Temperature Curve Name
   HPACCOOLEIRFF Speed 1,                         !Speed(1)Energy Input Ratio Function of Flow Fraction Curve Name
   HPACCOOLPLFFPLR Speed,                         !Speed(1)Part Load Fraction Correlation Curve Name
   1000,                         !Speed(1)Nominal Time for Condensate Removal to Begin
   1.5,                         !Speed(1)Ratio of Initial Moisture Evaporation Rate and Steady-state Latent Capacity
   3,                         !Speed(1)Maximum ON/OFF Cycling Rate
   45,                         !Speed(1)Latent Capacity Time Constant
   0.2,                         !Speed(1)Rated waste heat fraction of power input
   HAPCCoolWHFT Speed 1,                         !Speed(1)Waste heat Function of Temperature Curve Name
   0.9,                         !Speed(1)Evaporative Condenser Effectiveness
   0.05,                         !Speed(1)Evaporative Condenser Air Flow Rate
   50,                         !Speed(1)Evaporative Condenser Pump Rated Power Consumption
   17500,                         !Speed(2)Rated Total Cooling Capacity
   0.75,                         !Speed(2)Rated Sensible Heat Ratio
   3.0,                         !Speed(2)Rated COP
   0.85,                         !Speed(2)Rated Air Volume Flow Rate
   HPACCoolCapFT Speed 2,                         !Speed(2)Total Cooling Capacity Function of Temperature Curve Name
   HPACCoolCapFF Speed 2,                         !Speed(2)Total Cooling Capacity Function of Flow Fraction Curve Name
   HPACCOOLEIRFT Speed 2,                         !Speed(2)Energy Input Ratio Function of Temperature Curve Name
   HPACCOOLEIRFF Speed 2,                         !Speed(2)Energy Input Ratio Function of Flow Fraction Curve Name
   HPACCOOLPLFFPLR Speed,                         !Speed(2)Part Load Fraction Correlation Curve Name
   1000,                         !Speed(2)Nominal Time for Condensate Removal to Begin
   1.5,                         !Speed(2)Ratio of Initial Moisture Evaporation Rate and Steady-state Latent Capacity
   3,                         !Speed(2)Maximum ON/OFF Cycling Rate
   45,                         !Speed(2)Latent Capacity Time Constant
   0.2,                         !Speed(2)Rated waste heat fraction of power input
   HAPCCoolWHFT Speed 2,                         !Speed(2)Waste heat Function of Temperature Curve Name
   0.9,                         !Speed(2)Evaporative Condenser Effectiveness
   0.1,                         !Speed(2)Evaporative Condenser Air Flow Rate
   60,                         !Speed(2)Evaporative Condenser Pump Rated Power Consumption
   25500,                         !Speed(3)Rated Total Cooling Capacity
   0.75,                         !Speed(3)Rated Sensible Heat Ratio
   3.0,                         !Speed(3)Rated COP
   1.25,                         !Speed(3)Rated Air Volume Flow Rate
   HPACCoolCapFT Speed 3,                         !Speed(3)Total Cooling Capacity Function of Temperature Curve Name
   HPACCoolCapFF Speed 3,                         !Speed(3)Total Cooling Capacity Function of Flow Fraction Curve Name
   HPACCOOLEIRFT Speed 3,                         !Speed(3)Energy Input Ratio Function of Temperature Curve Name
   HPACCOOLEIRFF Speed 3,                         !Speed(3)Energy Input Ratio Function of Flow Fraction Curve Name
   HPACCOOLPLFFPLR Speed,                         !Speed(3)Part Load Fraction Correlation Curve Name
   1000,                         !Speed(3)Nominal Time for Condensate Removal to Begin
   1.5,                         !Speed(3)Ratio of Initial Moisture Evaporation Rate and Steady-state Latent Capacity
   3,                         !Speed(3)Maximum ON/OFF Cycling Rate
   45,                         !Speed(3)Latent Capacity Time Constant
   0.2,                         !Speed(3)Rated waste heat fraction of power input
   HAPCCoolWHFT Speed 3,                         !Speed(3)Waste heat Function of Temperature Curve Name
   0.9,                         !Speed(3)Evaporative Condenser Effectiveness
   0.2,                         !Speed(3)Evaporative Condenser Air Flow Rate
   80,                         !Speed(3)Evaporative Condenser Pump Rated Power Consumption
   35500,                         !Speed(4)Rated Total Cooling Capacity
   0.75,                         !Speed(4)Rated Sensible Heat Ratio
   3.0,                         !Speed(4)Rated COP
   1.75,                         !Speed(4)Rated Air Volume Flow Rate
   HPACCoolCapFT Speed 4,                         !Speed(4)Total Cooling Capacity Function of Temperature Curve Name
   HPACCoolCapFF Speed 4,                         !Speed(4)Total Cooling Capacity Function of Flow Fraction Curve Name
   HPACCOOLEIRFT Speed 4,                         !Speed(4)Energy Input Ratio Function of Temperature Curve Name
   HPACCOOLEIRFF Speed 4,                         !Speed(4)Energy Input Ratio Function of Flow Fraction Curve Name
   HPACCOOLPLFFPLR Speed,                         !Speed(4)Part Load Fraction Correlation Curve Name
   1000,                         !Speed(4)Nominal Time for Condensate Removal to Begin
   1.5,                         !Speed(4)Ratio of Initial Moisture Evaporation Rate and Steady-state Latent Capacity
   3,                         !Speed(4)Maximum ON/OFF Cycling Rate
   45,                         !Speed(4)Latent Capacity Time Constant
   0.2,                         !Speed(4)Rated waste heat fraction of power input
   HAPCCoolWHFT Speed 4,                         !Speed(4)Waste heat Function of Temperature Curve Name
   0.9,                         !Speed(4)Evaporative Condenser Effectiveness
   0.3,                         !Speed(4)Evaporative Condenser Air Flow Rate
   100;                         !Speed(4)Evaporative Condenser Pump Rated Power Consumption
COIL:Heating:DX:MultiSpeed,
   USMSHP_FanOnF1_HCoil,                         !Name
   FanAndCoilAvailSched,                         !Availability Schedule Name
   Heating Coil Air Inlet Node,                         !Air Inlet Node Name
   SuppHeating Coil Air Inlet Node,                         !Air Outlet Node Name
   -8.0,                         !Minimum Outdoor Dry-bulb Temperature for Compressor Operation
   200,                         !Crankcase Heater Capacity
   10,                         !Maximum Outdoor Dry-bulb Temperature for Crankcase Heater Operation
   HPACDefrostCAPFT,                         !Defrost energy input ratio modifier curve (function of temperature)
   7.22,                         !Maximum Outdoor Dry-bulb Temperature for Defrost Operation
   ReverseCycle,                         !Defrost Strategy
   Timed,                         !Defrost Control
   0.058333,                         !Defrost Time Period Fraction
   2000,                         !Resistive Defrost Heater Capacity
   No,                         !Apply Part Load Fraction to Speeds greater than 1
   NaturalGas,                         !Fuel Type
   4,                         !Number of speeds
   7500,                         !Speed(1)Rated Total Heating Capacity
   2.75,                         !Speed(1)Rated COP
   0.45,                         !Speed(1)Rated Air Flow Rate
   HPACHeatCapFT Speed 1,                         !Speed(1)Total Heating Capacity Function of Temperature Curve Name
   HPACHeatCapFF Speed 1,                         !Speed(1)Total Heating Capacity Function of Flow Fraction Curve Name
   HPACHeatEIRFT Speed 1,                         !Speed(1)Energy Input Ratio Function of Temperature Curve Name
   HPACHeatEIRFF Speed 1,                         !Speed(1)Energy Input Ratio Function of Flow Fraction Curve Name
   HPACHEATPLFFPLR Speed1,                         !Speed(1)Part Load Fraction Correlation Curve Name
   0.2,                         !Speed(1)Rated Waste Heat Fraction of Power Input
   HAPCHeatWHFT Speed 1,                         !Speed(1)Waste Heat Function of Temperature Curve Name
   17500,                         !Speed(2)Rated Total Heating Capacity
   2.75,                         !Speed(2)Rated COP
   0.85,                         !Speed(2)Rated Air Flow Rate
   HPACHeatCapFT Speed 2,                         !Speed(2)Total Heating Capacity Function of Temperature Curve Name
   HPACHeatCapFF Speed 2,                         !Speed(2)Total Heating Capacity Function of Flow Fraction Curve Name
   HPACHeatEIRFT Speed 2,                         !Speed(2)Energy Input Ratio Function of Temperature Curve Name
   HPACHeatEIRFF Speed 2,                         !Speed(2)Energy Input Ratio Function of Flow Fraction Curve Name
   HPACHEATPLFFPLR Speed1,                         !Speed(2)Part Load Fraction Correlation Curve Name
   0.2,                         !Speed(2)Rated Waste Heat Fraction of Power Input
   HAPCHeatWHFT Speed 2,                         !Speed(2)Waste Heat Function of Temperature Curve Name
   25500,                         !Speed(3)Rated Total Heating Capacity
   2.75,                         !Speed(3)Rated COP
   1.25,                         !Speed(3)Rated Air Flow Rate
   HPACHeatCapFT Speed 3,                         !Speed(3)Total Heating Capacity Function of Temperature Curve Name
   HPACHeatCapFF Speed 3,                         !Speed(3)Total Heating Capacity Function of Flow Fraction Curve Name
   HPACHeatEIRFT Speed 3,                         !Speed(3)Energy Input Ratio Function of Temperature Curve Name
   HPACHeatEIRFF Speed 3,                         !Speed(3)Energy Input Ratio Function of Flow Fraction Curve Name
   HPACHEATPLFFPLR Speed1,                         !Speed(3)Part Load Fraction Correlation Curve Name
   0.2,                         !Speed(3)Rated Waste Heat Fraction of Power Input
   HAPCHeatWHFT Speed 3,                         !Speed(3)Waste Heat Function of Temperature Curve Name
   35500,                         !Speed(4)Rated Total Heating Capacity
   2.75,                         !Speed(4)Rated COP
   1.75,                         !Speed(4)Rated Air Flow Rate
   HPACHeatCapFT Speed 4,                         !Speed(4)Total Heating Capacity Function of Temperature Curve Name
   HPACHeatCapFF Speed 4,                         !Speed(4)Total Heating Capacity Function of Flow Fraction Curve Name
   HPACHeatEIRFT Speed 4,                         !Speed(4)Energy Input Ratio Function of Temperature Curve Name
   HPACHeatEIRFF Speed 4,                         !Speed(4)Energy Input Ratio Function of Flow Fraction Curve Name
   HPACHEATPLFFPLR Speed1,                         !Speed(4)Part Load Fraction Correlation Curve Name
   0.2,                         !Speed(4)Rated Waste Heat Fraction of Power Input
   HAPCHeatWHFT Speed 4;                         !Speed(4)Waste Heat Function of Temperature Curve Name
COIL:Heating:Electric,
   USMSHP_FanOnF1_SHCoil,                         !Coil Name
   FanAndCoilAvailSched,                         !Available Schedule
   0.8,                         !Efficiency of the Coil
   45000,                         !Nominal Capacity of the Coil
   SuppHeating Coil Air Inlet Node,                         !Coil_Air_Inlet_Node
   Air Loop Outlet Node,                         !Coil_Air_Outlet_Node
   ;                         !Coil_Temp_Setpoint_Node
OutdoorAir:Mixer,
   OA Mixing Box 1,                         !Name
   Mixed Air Node,                         !Mixed_Air_Node
   Outside Air Inlet Node,                         !Outside_Air_Stream_Node
   Relief Air Outlet Node,                         !Relief_Air_Stream_Node
   Outdoor Air Mixer Inlet Node;                         !Return_Air_Stream_Node
AirLoopHVAC:OutdoorAirSystem,
   OA Sys 1,                         !Name
   OA Sys 1 Controllers,                         !Name: Controller List
   OA Sys 1 Equipment,                         !Name of an Air Loop Equipment List
   Outdoor Air 1 Avail List;                         !Name of a System Availability Manager List
ZoneHVAC:EquipmentConnections,
   West Zone,                      !Zone Name
   West Zone_Zone1Equipment,                      !List Name: Zone Equipment
   West Zone_Zone1Inlets,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   West Zone_Zone 1 Node,                      !Zone Air Node Name
   West Zone_Zone 1 Outlet Node;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   EAST ZONE,                      !Zone Name
   EAST ZONE_Zone2Equipment,                      !List Name: Zone Equipment
   EAST ZONE_Zone2Inlets,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   EAST ZONE_Zone 2 Node,                      !Zone Air Node Name
   EAST ZONE_Zone 2 Outlet Node;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   NORTH ZONE,                      !Zone Name
   NORTH ZONE_Zone3Equipment,                      !List Name: Zone Equipment
   NORTH ZONE_Zone3Inlets,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   NORTH ZONE_Zone 3 Node,                      !Zone Air Node Name
   NORTH ZONE_Zone 3 Outlet Node;                      !Zone Return Air Node Name
AirLoopHVAC:ZoneSplitter,
   Zone Supply Air Splitter,                         !Splitter Name
   Zone Equipment Inlet Node,                         !Inlet_Node
   West Zone_Zone 1 Inlet Node,                         !Outlet_Node_1
   EAST ZONE_Zone 2 Inlet Node,                         !Outlet_Node_2
   NORTH ZONE_Zone 3 Inlet Node;                         !Outlet_Node_3
AirLoopHVAC:ZoneMixer,
   Zone Return Air Mixer,                         !Mixer Name
   Return Air Mixer Outlet,                         !Outlet_Node
   West Zone_Zone 1 Outlet Node,                         !Inlet_Node_1
   EAST ZONE_Zone 2 Outlet Node,                         !Inlet_Node_2
   NORTH ZONE_Zone 3 Outlet Node;                         !Inlet_Node_3

