NodeList,
   OutsideAirInletNodes,                         !Node List Name
   Outside Air Inlet Node 1;                         !Node_ID_1
NodeList,
   SPACE1-1_SPACE1-1 In Nodes,                      !Node List Name
   SPACE1-1_SPACE1-1 In Node;                      !Node_ID_1
NodeList,
   SPACE2-1_SPACE2-1 In Nodes,                      !Node List Name
   SPACE2-1_SPACE2-1 In Node;                      !Node_ID_1
NodeList,
   SPACE3-1_SPACE3-1 In Nodes,                      !Node List Name
   SPACE3-1_SPACE3-1 In Node;                      !Node_ID_1
NodeList,
   SPACE4-1_SPACE4-1 In Nodes,                      !Node List Name
   SPACE4-1_SPACE4-1 In Node;                      !Node_ID_1
NodeList,
   SPACE5-1_SPACE5-1 In Nodes,                      !Node List Name
   SPACE5-1_SPACE5-1 In Node;                      !Node_ID_1
NodeList,
   Supply Air Temp Nodes 1,                         !Node List Name
   VAV Sys 1 Outlet Node;                         !Node_ID_1
NodeList,
   Hot Water Loop Setpoint Node List,                         !Node List Name
   HW Supply Outlet Node;                         !Node_ID_1
NodeList,
   Chilled Water Loop Setpoint Node List,                         !Node List Name
   CW Supply Outlet Node;                         !Node_ID_1
BranchList,
   VAV Sys 1 Branches,                         !Branch List Name
   VAV Sys 1 Main Branch;                         !Branch Name 1
BranchList,
   Heating Supply Side Branches,                         !Branch List Name
   Heating Supply Inlet Branch,                         !Branch Name 1
   Central Boiler Branch,                         !Branch Name 2
   Heating Supply Bypass Branch,                         !Branch Name 3
   Heating Supply Outlet Branch;                         !Branch Name 4
BranchList,
   Heating Demand Side Branches,                         !Branch List Name
   Heating Demand Inlet Branch,                         !Branch Name 1
   SPACE1-1_SPACE1-1 Reheat Branch,                         !Branch Name 2
   SPACE2-1_SPACE2-1 Baseboard Branch,                         !Branch Name 3
   SPACE3-1_SPACE3-1 Reheat Branch,                         !Branch Name 4
   SPACE4-1_SPACE4-1 Baseboard Branch,                         !Branch Name 5
   SPACE5-1_SPACE5-1 Reheat Branch,                         !Branch Name 6
   Main Heating Coil 1 Branch,                         !Branch Name 7
   Heating Demand Bypass Branch,                         !Branch Name 8
   Heating Demand Outlet Branch;                         !Branch Name 9
BranchList,
   Cooling Supply Side Branches,                         !Branch List Name
   CW Pump Branch,                         !Branch Name 1
   Central Chiller Branch,                         !Branch Name 2
   Cooling Supply Bypass Branch,                         !Branch Name 3
   Cooling Supply Outlet;                         !Branch Name 4
BranchList,
   Cooling Demand Side Branches,                         !Branch List Name
   Cooling Demand Inlet,                         !Branch Name 1
   Cooling Coil Branch,                         !Branch Name 2
   Cooling Demand Bypass Branch,                         !Branch Name 3
   Cooling Demand Outlet;                         !Branch Name 4
BranchList,
   Condenser Supply Side Branches,                         !Branch List Name
   Condenser Supply Inlet Branch,                         !Branch Name 1
   Condenser Supply Tower Branch,                         !Branch Name 2
   Condenser Supply Bypass Branch,                         !Branch Name 3
   Condenser Supply Outlet Branch;                         !Branch Name 4
BranchList,
   Condenser Demand Side Branches,                         !Branch List Name
   Condenser Demand Inlet Branch,                         !Branch Name 1
   Central Chiller Condenser Branch,                         !Branch Name 2
   Condenser Demand Bypass Branch,                         !Branch Name 3
   Condenser Demand Outlet Branch;                         !Branch Name 4
AirLoopHVAC,
   VAV Sys 1,                         !Primary Air Loop Name
   VAV Sys 1 Controllers,                         !Name: Controller List
   VAV Sys 1 Avail List,                         !Name: System Availability Manager List
   autosize,                         !Primary air design volumetric flow rate
   VAV Sys 1 Branches,                         !Air Loop Branch List Name
   ,                         !Air Loop Connector List Name
   VAV Sys 1 Inlet Node,                         !ReturnAir AirLoop Inlet Node
   Plenum-1 Outlet Node,                         !ZoneEquipGroup Outlet Node
   Zone Eq In Node,                         !SupplyAirPath ZoneEquipGroup Inlet Nodes
   VAV Sys 1 Outlet Node;                         !AirLoop Outlet Nodes
PlantLoop,
   Hot Water Loop,                         !Plant Loop Name
   Water,                         !Fluid Type
   Hot Loop Operation,                         !Plant Operation Scheme List Name
   HW Supply Outlet Node,                         !Loop Temperature Setpoint Node Name
   100,                         !Maximum Loop Temperature
   10,                         !Minimum Loop Temperature
   autosize,                         !Maximum Loop Volumetric Flow Rate
   0,                         !Minimum Loop Volumetric Flow Rate
   autocalculate,                         !volume of the plant loop
   HW Supply Inlet Node,                         !Plant Side Inlet Node Name
   HW Supply Outlet Node,                         !Plant Side Outlet Node Name
   Heating Supply Side Branches,                         !Plant Side Branch List Name
   Heating Supply Side Connectors,                         !Plant Side Connector List Name
   HW Demand Inlet Node,                         !Demand Side Inlet Node Name
   HW Demand Outlet Node,                         !Demand Side Outlet Nodes Name
   Heating Demand Side Branches,                         !Demand Side Branch List Name
   Heating Demand Side Connectors,                         !Demand Side Connector List Name
   SEQUENTIAL,                         !Load Distribution Scheme
   ,                         !System Availability Manager List
   SingleSetPoint,                         !Plant Loop Demand Calculation Scheme
   NONE,                         !Common Pipe Simulation
   None;                         !Pressure Simulation Type
PlantLoop,
   Chilled Water Loop,                         !Plant Loop Name
   Water,                         !Fluid Type
   CW Loop Operation,                         !Plant Operation Scheme List Name
   CW Supply Outlet Node,                         !Loop Temperature Setpoint Node Name
   98,                         !Maximum Loop Temperature
   1,                         !Minimum Loop Temperature
   autosize,                         !Maximum Loop Volumetric Flow Rate
   0,                         !Minimum Loop Volumetric Flow Rate
   autocalculate,                         !volume of the plant loop
   CW Supply Inlet Node,                         !Plant Side Inlet Node Name
   CW Supply Outlet Node,                         !Plant Side Outlet Node Name
   Cooling Supply Side Branches,                         !Plant Side Branch List Name
   Cooling Supply Side Connectors,                         !Plant Side Connector List Name
   CW Demand Inlet Node,                         !Demand Side Inlet Node Name
   CW Demand Outlet Node,                         !Demand Side Outlet Nodes Name
   Cooling Demand Side Branches,                         !Demand Side Branch List Name
   Cooling Demand Side Connectors,                         !Demand Side Connector List Name
   SEQUENTIAL,                         !Load Distribution Scheme
   ,                         !System Availability Manager List
   SingleSetPoint,                         !Plant Loop Demand Calculation Scheme
   NONE,                         !Common Pipe Simulation
   None;                         !Pressure Simulation Type
CondenserLoop,
   Condenser Water Loop,                         !Condenser Loop Name
   Water,                         !Fluid Type
   Tower Loop Operation,                         !Condenser Operation Scheme List Name
   AIR,                         !Condenser Loop Temperature Setpoint Node or reference
   80,                         !Maximum Loop Temperature
   10,                         !Minimum Loop Temperature
   autosize,                         !Maximum Loop Volumetric Flow Rate
   0,                         !Minimum Loop Volumetric Flow Rate
   autocalculate,                         !volume of the condenser loop
   Condenser Supply Inlet Node,                         !Condenser Side Inlet Node Name
   Condenser Supply Outlet Node,                         !Condenser Side Outlet Node Name
   Condenser Supply Side Branches,                         !Condenser Side Branch List Name
   Condenser Supply Side Connectors,                         !Condenser Side Connector List Name
   Condenser Demand Inlet Node,                         !Demand Side Inlet Node Name
   Condenser Demand Outlet Node,                         !Demand Side Outlet Nodes Name
   Condenser Demand Side Branches,                         !Condenser Demand Side Branch List Name
   Condenser Demand Side Connectors,                         !Condenser Demand Side Connector List Name
   Sequential,                         !Load Distribution Scheme
   None;                         !Pressure Simulation Type
AirLoopHVAC:SupplyPath,
   Zone Supply Air Path 1,                         !Name
   Zone Eq In Node,                         !Supply Air Path Inlet Node Name
   AirLoopHVAC:ZoneSplitter,                         !Component 1 Object Type
   Zone Supply Air Splitter 1;                         !Component 1 Name
AirLoopHVAC:ReturnPath,
   ReturnAirPath1,                         !Name
   Plenum-1 Outlet Node,                         !Return Air Path Outlet Node Name
   AirLoopHVAC:ReturnPlenum,                         !Component 1 Object Type
   Return-Plenum-1;                         !Component 1 Name
Branch,
   VAV Sys 1 Main Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   AirLoopHVAC:OutdoorAirSystem,                         !Comp1 Type
   OA Sys 1,                         !Comp1 Name
   VAV Sys 1 Inlet Node,                         !Comp1 Inlet Node Name
   Mixed Air Node 1,                         !Comp1 Outlet Node Name
   PASSIVE,                         !Comp1 Branch Control Type
   COIL:Cooling:Water,                         !Comp2 Type
   Main Cooling Coil 1,                         !Comp2 Name
   Mixed Air Node 1,                         !Comp2 Inlet Node Name
   Main Cooling Coil 1 Outlet Node,                         !Comp2 Outlet Node Name
   PASSIVE,                         !Comp2 Branch Control Type
   COIL:Heating:Water,                         !Comp3 Type
   Main Heating Coil 1,                         !Comp3 Name
   Main Cooling Coil 1 Outlet Node,                         !Comp3 Inlet Node Name
   Main Heating Coil 1 Outlet Node,                         !Comp3 Outlet Node Name
   PASSIVE,                         !Comp3 Branch Control Type
   Fan:VariableVolume,                         !Comp4 Type
   Supply Fan 1,                         !Comp4 Name
   Main Heating Coil 1 Outlet Node,                         !Comp4 Inlet Node Name
   VAV Sys 1 Outlet Node,                         !Comp4 Outlet Node Name
   ACTIVE;                         !Comp4 Branch Control Type
Branch,
   Heating Supply Inlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pump:VariableSpeed,                         !Comp1 Type
   HW Circ Pump,                         !Comp1 Name
   HW Supply Inlet Node,                         !Comp1 Inlet Node Name
   HW Pump Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Central Boiler Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Boiler:HotWater,                         !Comp1 Type
   Central Boiler,                         !Comp1 Name
   Central Boiler Inlet Node,                         !Comp1 Inlet Node Name
   Central Boiler Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Heating Supply Bypass Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Heating Supply Side Bypass,                         !Comp1 Name
   Heating Supply Bypass Inlet Node,                         !Comp1 Inlet Node Name
   Heating Supply Bypass Outlet Node,                         !Comp1 Outlet Node Name
   BYPASS;                         !Comp1 Branch Control Type
Branch,
   Heating Supply Outlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Heating Supply Outlet,                         !Comp1 Name
   Heating Supply Exit Pipe Inlet Node,                         !Comp1 Inlet Node Name
   HW Supply Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Heating Demand Inlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Heating Demand Inlet Pipe,                         !Comp1 Name
   HW Demand Inlet Node,                         !Comp1 Inlet Node Name
   HW Demand Entrance Pipe Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Heating Demand Outlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Heating Demand Outlet Pipe,                         !Comp1 Name
   HW Demand Exit Pipe Inlet Node,                         !Comp1 Inlet Node Name
   HW Demand Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   SPACE1-1_SPACE1-1 Reheat Branch,                      !Branch Name
   autosize,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   COIL:Heating:Water,                      !Comp1 Type
   SPACE1-1_SPACE1-1 Zone Coil,                      !Comp1 Name
   SPACE1-1_SPACE1-1 Zone Coil Water In Node,                      !Comp1 Inlet Node Name
   SPACE1-1_SPACE1-1 Zone Coil Water Out Node,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   SPACE2-1_SPACE2-1 Baseboard Branch,                      !Branch Name
   autosize,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   ZoneHVAC:Baseboard:RadiantConvective:Water,                      !Comp1 Type
   SPACE2-1_SPACE2-1 Baseboard,                      !Comp1 Name
   SPACE2-1_SPACE2-1_Zone Coil Water In Node,                      !Comp1 Inlet Node Name
   SPACE2-1_SPACE2-1_Zone Coil Water Out Node,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   SPACE3-1_SPACE3-1 Reheat Branch,                      !Branch Name
   autosize,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   COIL:Heating:Water,                      !Comp1 Type
   SPACE3-1_SPACE3-1 Zone Coil,                      !Comp1 Name
   SPACE3-1_SPACE3-1 Zone Coil Water In Node,                      !Comp1 Inlet Node Name
   SPACE3-1_SPACE3-1 Zone Coil Water Out Node,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   SPACE4-1_SPACE4-1 Baseboard Branch,                      !Branch Name
   autosize,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   ZoneHVAC:Baseboard:RadiantConvective:Water,                      !Comp1 Type
   SPACE4-1_SPACE4-1 Baseboard,                      !Comp1 Name
   SPACE4-1_SPACE4-1_Zone Coil Water In Node,                      !Comp1 Inlet Node Name
   SPACE4-1_SPACE4-1_Zone Coil Water Out Node,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   SPACE5-1_SPACE5-1 Reheat Branch,                      !Branch Name
   autosize,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   COIL:Heating:Water,                      !Comp1 Type
   SPACE5-1_SPACE5-1 Zone Coil,                      !Comp1 Name
   SPACE5-1_SPACE5-1 Zone Coil Water In Node,                      !Comp1 Inlet Node Name
   SPACE5-1_SPACE5-1 Zone Coil Water Out Node,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   Main Heating Coil 1 Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   COIL:Heating:Water,                         !Comp1 Type
   Main Heating Coil 1,                         !Comp1 Name
   Main Heating Coil 1 Water Inlet Node,                         !Comp1 Inlet Node Name
   Main Heating Coil 1 Water Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Heating Demand Bypass Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Heating Demand Bypass,                         !Comp1 Name
   Heating Demand Bypass Inlet Node,                         !Comp1 Inlet Node Name
   Heating Demand Bypass Outlet Node,                         !Comp1 Outlet Node Name
   BYPASS;                         !Comp1 Branch Control Type
Branch,
   Cooling Demand Inlet,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Cooling Demand Side Inlet Pipe,                         !Comp1 Name
   CW Demand Inlet Node,                         !Comp1 Inlet Node Name
   CW Demand Entrance Pipe Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Cooling Coil Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   COIL:Cooling:Water,                         !Comp1 Type
   Main Cooling Coil 1,                         !Comp1 Name
   Main Cooling Coil 1 Water Inlet Node,                         !Comp1 Inlet Node Name
   Main Cooling Coil 1 Water Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Cooling Demand Bypass Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Cooling Demand Side Bypass,                         !Comp1 Name
   CW Demand Bypass Inlet Node,                         !Comp1 Inlet Node Name
   CW Demand Bypass Outlet Node,                         !Comp1 Outlet Node Name
   BYPASS;                         !Comp1 Branch Control Type
Branch,
   Cooling Demand Outlet,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   CW Demand Side Outlet Pipe,                         !Comp1 Name
   CW Demand Exit Pipe Inlet Node,                         !Comp1 Inlet Node Name
   CW Demand Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Cooling Supply Outlet,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Supply Side Outlet Pipe,                         !Comp1 Name
   Supply Side Exit Pipe Inlet Node,                         !Comp1 Inlet Node Name
   CW Supply Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   CW Pump Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pump:VariableSpeed,                         !Comp1 Type
   CW Circ Pump,                         !Comp1 Name
   CW Supply Inlet Node,                         !Comp1 Inlet Node Name
   CW Pump Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Central Chiller Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   CHILLER:ELECTRIC,                         !Comp1 Type
   Central Chiller,                         !Comp1 Name
   Central Chiller Inlet Node,                         !Comp1 Inlet Node Name
   Central Chiller Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Cooling Supply Bypass Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Supply Side Bypass,                         !Comp1 Name
   CW Supply Bypass Inlet Node,                         !Comp1 Inlet Node Name
   CW Supply Bypass Outlet Node,                         !Comp1 Outlet Node Name
   BYPASS;                         !Comp1 Branch Control Type
Branch,
   Condenser Supply Tower Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   COOLINGTOWER:SINGLESPEED,                         !Comp1 Type
   Central Tower,                         !Comp1 Name
   Condenser Tower Inlet Node,                         !Comp1 Inlet Node Name
   Condenser Tower Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Condenser Supply Bypass Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Condenser Supply Side Bypass,                         !Comp1 Name
   Cond Supply Bypass Inlet Node,                         !Comp1 Inlet Node Name
   Cond Supply Bypass Outlet Node,                         !Comp1 Outlet Node Name
   BYPASS;                         !Comp1 Branch Control Type
Branch,
   Condenser Supply Outlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Condenser Supply Outlet,                         !Comp1 Name
   Condenser Supply Exit Pipe Inlet Node,                         !Comp1 Inlet Node Name
   Condenser Supply Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Condenser Demand Inlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Condenser Demand Inlet Pipe,                         !Comp1 Name
   Condenser Demand Inlet Node,                         !Comp1 Inlet Node Name
   Condenser Demand Entrance Pipe Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Central Chiller Condenser Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   CHILLER:ELECTRIC,                         !Comp1 Type
   Central Chiller,                         !Comp1 Name
   Central Chiller Condenser Inlet Node,                         !Comp1 Inlet Node Name
   Central Chiller Condenser Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Condenser Demand Bypass Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Condenser Demand Side Bypass,                         !Comp1 Name
   Cond Demand Bypass Inlet Node,                         !Comp1 Inlet Node Name
   Cond Demand Bypass Outlet Node,                         !Comp1 Outlet Node Name
   BYPASS;                         !Comp1 Branch Control Type
Branch,
   Condenser Demand Outlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Condenser Demand Outlet Pipe,                         !Comp1 Name
   Condenser Demand Exit Pipe Inlet Node,                         !Comp1 Inlet Node Name
   Condenser Demand Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Condenser Supply Inlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pump:VariableSpeed,                         !Comp1 Type
   Cond Circ Pump,                         !Comp1 Name
   Condenser Supply Inlet Node,                         !Comp1 Inlet Node Name
   Condenser Pump Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
ConnectorList,
   Heating Supply Side Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   Heating Supply Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   Heating Supply Mixer;                         !Name of Connector 2
ConnectorList,
   Heating Demand Side Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   Heating Demand Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   Heating Demand Mixer;                         !Name of Connector 2
ConnectorList,
   Cooling Supply Side Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   CW Loop Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   CW Loop Mixer;                         !Name of Connector 2
ConnectorList,
   Cooling Demand Side Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   CW Demand Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   CW Demand Mixer;                         !Name of Connector 2
ConnectorList,
   Condenser Supply Side Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   Condenser Supply Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   Condenser Supply Mixer;                         !Name of Connector 2
ConnectorList,
   Condenser Demand Side Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   Condenser Demand Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   Condenser Demand Mixer;                         !Name of Connector 2
PlantEquipmentOperationSchemes,
   Hot Loop Operation,                         !PlantOperationSchemeName
   PlantEquipmentOperation:HeatingLoad,                         !KEY--Control Scheme 1
   Central Boiler Only,                         !Control Scheme Name 1
   PlantOnSched;                         !Control Scheme Schedule 1
PlantEquipmentOperationSchemes,
   CW Loop Operation,                         !PlantOperationSchemeName
   PlantEquipmentOperation:CoolingLoad,                         !KEY--Control Scheme 1
   Central Chiller Only,                         !Control Scheme Name 1
   PlantOnSched;                         !Control Scheme Schedule 1
CondenserEquipmentOperationSchemes,
   Tower Loop Operation,                         !CondenserOperationSchemeName
   PlantEquipmentOperation:CoolingLoad,                         !KEY--Control Scheme 1
   Year Round Tower Operation,                         !Control Scheme Name 1
   PlantOnSched;                         !Control Scheme Schedule 1
PlantEquipmentOperation:CoolingLoad,
   Central Chiller Only,                         !Name
   0,                         !Load Range Lower Limit 1
   900000,                         !Load Range Upper Limit 1
   Cooling Plant;                         !Priority Control Equip List Name 1
PlantEquipmentOperation:CoolingLoad,
   Year Round Tower Operation,                         !Name
   0,                         !Load Range Lower Limit 1
   90000000,                         !Load Range Upper Limit 1
   All Towers;                         !Priority Control Equip List Name 1
PlantEquipmentOperation:HeatingLoad,
   Central Boiler Only,                         !Name
   0,                         !Load Range Lower Limit 1
   1000000,                         !Load Range Upper Limit 1
   heating plant;                         !Priority Control Equip List Name 1
ZoneHVAC:EquipmentList,
   SPACE1-1_SPACE1-1 Eq,                      !Name
   ZoneHVAC:AirDistributionUnit,                      !KEY--Zone Equipment Type 1
   SPACE1-1_SPACE1-1 ATU,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   SPACE2-1_SPACE2-1 Eq,                      !Name
   ZoneHVAC:AirDistributionUnit,                      !KEY--Zone Equipment Type 1
   SPACE2-1_SPACE2-1 ATU,                      !Type Name 1
   1,                      !Cooling Priority 1
   1,                      !Heating Priority 1
   ZoneHVAC:Baseboard:RadiantConvective:Water,                      !KEY--Zone Equipment Type 2
   SPACE2-1_SPACE2-1 Baseboard,                      !Type Name 2
   2,                      !Cooling Priority 2
   2;                      !Heating Priority 2
ZoneHVAC:EquipmentList,
   SPACE3-1_SPACE3-1 Eq,                      !Name
   ZoneHVAC:AirDistributionUnit,                      !KEY--Zone Equipment Type 1
   SPACE3-1_SPACE3-1 ATU,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   SPACE4-1_SPACE4-1 Eq,                      !Name
   ZoneHVAC:AirDistributionUnit,                      !KEY--Zone Equipment Type 1
   SPACE4-1_SPACE4-1 ATU,                      !Type Name 1
   1,                      !Cooling Priority 1
   1,                      !Heating Priority 1
   ZoneHVAC:Baseboard:RadiantConvective:Water,                      !KEY--Zone Equipment Type 2
   SPACE4-1_SPACE4-1 Baseboard,                      !Type Name 2
   2,                      !Cooling Priority 2
   2;                      !Heating Priority 2
ZoneHVAC:EquipmentList,
   SPACE5-1_SPACE5-1 Eq,                      !Name
   ZoneHVAC:AirDistributionUnit,                      !KEY--Zone Equipment Type 1
   SPACE5-1_SPACE5-1 ATU,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
AirLoopHVAC:OutdoorAirSystem:EquipmentList,
   OA Sys 1 Equipment,                         !Name
   OutdoorAir:Mixer,                         !KEY--System Component 1
   OA Mixing Box 1;                         !Component Name 1
PlantEquipmentList,
   heating plant,                         !Equip List Name
   Boiler:HotWater,                         !KEY--Plant Equip 1
   Central Boiler;                         !Equip Name 1
PlantEquipmentList,
   Cooling Plant,                         !Equip List Name
   CHILLER:ELECTRIC,                         !KEY--Plant Equip 1
   Central Chiller;                         !Equip Name 1
CondenserEquipmentList,
   All Towers,                         !Equip List Name
   COOLINGTOWER:SINGLESPEED,                         !KEY--Condenser Equip 1
   Central Tower;                         !Equip Name 1
AirLoopHVAC:ControllerList,
   OA Sys 1 Controllers,                         !Name
   Controller:OutdoorAir,                         !Controller Type 1
   OA Controller 1;                         !Controller Name 1
AirLoopHVAC:ControllerList,
   VAV Sys 1 Controllers,                         !Name
   CONTROLLER:WaterCoil,                         !Controller Type 1
   Central Heating Coil Contoller 1,                         !Controller Name 1
   CONTROLLER:WaterCoil,                         !Controller Type 2
   Central Cooling Coil Contoller 1;                         !Controller Name 2
Controller:OutdoorAir,
   OA Controller 1,                         !Name
   Relief Air Outlet Node 1,                         !Relief Air Outlet Node Name
   VAV Sys 1 Inlet Node,                         !Return Air Node Name
   Mixed Air Node 1,                         !Mixed Air Node Name
   Outside Air Inlet Node 1,                         !Actuator Node Name
   autosize,                         !Minimum Outdoor Air Flow Rate
   autosize,                         !Maximum Outdoor Air Flow Rate
   FixedDryBulb,                         !Economizer Control Type
   ModulateFlow,                         !Economizer Control Action Type
   19,                         !Economizer Maximum Limit Dry-Bulb Temperature
   ,                         !Economizer Maximum Limit Enthalpy
   ,                         !Economizer Maximum Limit Dewpoint Temperature
   ,                         !Electronic Enthalpy Limit Curve Name
   4,                         !Economizer Minimum Limit Dry-Bulb Temperature
   NoLockout,                         !Lockout Type
   FixedMinimum,                         !Minimum Limit Type
   Min OA Sched,                         !Minimum Outdoor Air Schedule Name
   ,                         !Minimum Fraction of Outdoor Air Schedule Name
   ,                         !Maximum Fraction of Outdoor Air Schedule Name
   ,                         !Mechanical Ventilation Controller Name
   ,                         !Time of Day Economizer Control Schedule Name
   No,                         !High Humidity Control
   ,                         !Humidistat Control Zone Name
   1.0,                         !High Humidity Outdoor Air Flow Ratio
   Yes,                         !Control High Indoor Humidity Based on Outdoor Humidity Ratio
   BypassWhenWithinEconomizerLimits;                         !Heat Recovery Bypass Control Type
CONTROLLER:WaterCoil,
   Central Cooling Coil Contoller 1,                         !Name
   TemperatureAndHumidityRatio,                         !Control variable
   REVERSE,                         !Action
   Flow,                         !Actuator variable
   VAV Sys 1 Outlet Node,                         !Control_Node
   Main Cooling Coil 1 Water Inlet Node,                         !Actuator_Node
   ,                         !Controller Convergence Tolerance
   autosize,                         !Max Actuated Flow
   0.0000001;                         !Min Actuated Flow
CONTROLLER:WaterCoil,
   Central Heating Coil Contoller 1,                         !Name
   Temperature,                         !Control variable
   NORMAL,                         !Action
   Flow,                         !Actuator variable
   VAV Sys 1 Outlet Node,                         !Control_Node
   Main Heating Coil 1 Water Inlet Node,                         !Actuator_Node
   ,                         !Controller Convergence Tolerance
   autosize,                         !Max Actuated Flow
   0.0000001;                         !Min Actuated Flow
ZoneHVAC:LowTemperatureRadiant:SurfaceGroup,
   SPACE2-1 SurfaceGroup,                         !name of this list of surfaces
   RIGHT-1,                         !surface name 1
   0.4,                         !flow fraction for surface 1
   C2-1,                         !surface name 2
   0.2,                         !flow fraction for surface 2
   SB25,                         !surface name 3
   0.1;                         !flow fraction for surface 3
ZoneHVAC:LowTemperatureRadiant:SurfaceGroup,
   SPACE4-1 SurfaceGroup,                         !name of this list of surfaces
   LEFT-1,                         !surface name 1
   0.4,                         !flow fraction for surface 1
   C4-1,                         !surface name 2
   0.2,                         !flow fraction for surface 2
   SB45,                         !surface name 3
   0.1;                         !flow fraction for surface 3
AvailabilityManagerAssignmentList,
   VAV Sys 1 Avail List,                         !Name
   AvailabilityManager:Scheduled,                         !System Availability Manager Type 1
   VAV Sys 1 Avail;                         !System Availability Manager Name 1
AvailabilityManager:Scheduled,
   VAV Sys 1 Avail,                         !Name
   FanAvailSched;                         !Schedule name
SetpointManager:Scheduled,
   Supply Air Temp Manager 1,                         !Name
   Temperature,                         !Control variable
   Seasonal Reset Supply Air Temp Sch,                         !Schedule Name
   Supply Air Temp Nodes 1;                         !Name of the set point Node or Node List
SetpointManager:Scheduled,
   Hot Water Loop Setpoint Manager,                         !Name
   Temperature,                         !Control variable
   HW Loop Temp Schedule,                         !Schedule Name
   Hot Water Loop Setpoint Node List;                         !Name of the set point Node or Node List
SetpointManager:Scheduled,
   Chilled Water Loop Setpoint Manager,                         !Name
   Temperature,                         !Control variable
   CW Loop Temp Schedule,                         !Schedule Name
   Chilled Water Loop Setpoint Node List;                         !Name of the set point Node or Node List
SetpointManager:SingleZone:Humidity:Maximum,
   Space2-1 Humidistat Manager,                         !Name
   ,                         !Control variable
   ,                         !Schedule name
   VAV Sys 1 Outlet Node,                         !Name of the set point Node or Node List
   SPACE2-1_SPACE2-1 Node;                         !Control zone air node name
SetpointManager:MixedAir,
   Mixed Air Temp Manager 1,                         !Name
   Temperature,                         !Control variable:
   VAV Sys 1 Outlet Node,                         !reference set point node name
   Main Heating Coil 1 Outlet Node,                         !fan inlet node name
   VAV Sys 1 Outlet Node,                         !fan outlet node name
   Mixed Air Node 1;                         !Name of the set point Node or Node List
OutdoorAir:NodeList,
   Outside Air Inlet Node 1;                         !1st Node name or node list name
ThermostatSetpoint:DualSetpoint,
   DualSetPoint,                         !Name
   Htg-SetP-Sch,                         !Heating Setpoint Temperature SCHEDULE Name
   Clg-SetP-Sch;                         !Cooling Setpoint Temperature SCHEDULE Name
SIZING:PARAMETERS,
   1.3,                         !Cooling Sizing Factor
   1.3,                         !Heating sizing factor
   ;                         !time steps in averaging window
Sizing:Plant,
   Hot Water Loop,                         !name of a PLANT LOOP or CONDENSER LOOP object
   Heating,                         !loop type
   82,                         !Design loop exit temperature
   11;                         !Design loop delta T
Sizing:Plant,
   Chilled Water Loop,                         !name of a PLANT LOOP or CONDENSER LOOP object
   Cooling,                         !loop type
   7.22,                         !Design loop exit temperature
   6.67;                         !Design loop delta T
Sizing:Plant,
   Condenser Water Loop,                         !name of a PLANT LOOP or CONDENSER LOOP object
   Condenser,                         !loop type
   29.4,                         !Design loop exit temperature
   5.6;                         !Design loop delta T
Sizing:System,
   VAV Sys 1,                         !name of an AIR PRIMARY LOOP object
   sensible,                         !type of load to size on
   autosize,                         !Design (minimum) outside air volumetric flow rate
   0.3,                         !minimum system air flow ratio
   7,                         !Preheat design temperature
   0.008,                         !Preheat design humidity ratio
   11,                         !Precool design temperature
   0.008,                         !Precool design humidity ratio
   12.8,                         !Central cooling design supply air temperature
   16.7,                         !Central heating design supply air temperature
   noncoincident,                         !Sizing Option
   no,                         !Cooling 100% Outside Air
   no,                         !Heating 100% Outside Air
   0.008,                         !Central cooling design supply air humidity ratio
   0.008,                         !Central heating design supply air humidity ratio
   DesignDay,                         !Central heating design supply air humidity ratio
   0,                         !cooling design air flow rate
   DesignDay,                         !heating design air flow method
   0;                         !heating design air flow rate
Sizing:Zone,
   SPACE1-1,                         !Name of a zone
   14,                         !Zone cooling design supply air temperature
   50,                         !Zone heating design supply air temperature
   0.009,                         !Zone cooling design supply air humidity ratio
   0.004,                         !Zone heating design supply air humidity ratio
   flow/person,                         !outside air method
   0.00944,                         !outside air flow per person
   0,                         !outside air flow per zone area
   0,                         !outside air flow per zone
   0,                         !zone heating sizing factor
   0,                         !zone cooling sizing factor
   DesignDay,                         !cooling design air flow method
   0,                         !cooling design air flow rate
   0.000762,                         !cooling min air flow per zone area
   0,                         !cooling min air flow
   0,                         !cooling min air flow fraction
   DesignDay,                         !heating design air flow method
   0,                         !heating design air flow rate
   0.002032,                         !heating max air flow per zone area
   0.1415762,                         !heating max air flow
   0.3;                         !heating max air flow fraction
Sizing:Zone,
   SPACE2-1,                         !Name of a zone
   14,                         !Zone cooling design supply air temperature
   50,                         !Zone heating design supply air temperature
   0.009,                         !Zone cooling design supply air humidity ratio
   0.004,                         !Zone heating design supply air humidity ratio
   flow/person,                         !outside air method
   0.00944,                         !outside air flow per person
   0,                         !outside air flow per zone area
   0,                         !outside air flow per zone
   0,                         !zone heating sizing factor
   0,                         !zone cooling sizing factor
   DesignDay,                         !cooling design air flow method
   0,                         !cooling design air flow rate
   0.000762,                         !cooling min air flow per zone area
   0,                         !cooling min air flow
   0,                         !cooling min air flow fraction
   DesignDay,                         !heating design air flow method
   0,                         !heating design air flow rate
   0.002032,                         !heating max air flow per zone area
   0.1415762,                         !heating max air flow
   0.3;                         !heating max air flow fraction
Sizing:Zone,
   SPACE3-1,                         !Name of a zone
   14,                         !Zone cooling design supply air temperature
   50,                         !Zone heating design supply air temperature
   0.009,                         !Zone cooling design supply air humidity ratio
   0.004,                         !Zone heating design supply air humidity ratio
   flow/person,                         !outside air method
   0.00944,                         !outside air flow per person
   0,                         !outside air flow per zone area
   0,                         !outside air flow per zone
   0,                         !zone heating sizing factor
   0,                         !zone cooling sizing factor
   DesignDay,                         !cooling design air flow method
   0,                         !cooling design air flow rate
   0.000762,                         !cooling min air flow per zone area
   0,                         !cooling min air flow
   0,                         !cooling min air flow fraction
   DesignDay,                         !heating design air flow method
   0,                         !heating design air flow rate
   0.002032,                         !heating max air flow per zone area
   0.1415762,                         !heating max air flow
   0.3;                         !heating max air flow fraction
Sizing:Zone,
   SPACE4-1,                         !Name of a zone
   14,                         !Zone cooling design supply air temperature
   50,                         !Zone heating design supply air temperature
   0.009,                         !Zone cooling design supply air humidity ratio
   0.004,                         !Zone heating design supply air humidity ratio
   flow/person,                         !outside air method
   0.00944,                         !outside air flow per person
   0,                         !outside air flow per zone area
   0,                         !outside air flow per zone
   0,                         !zone heating sizing factor
   0,                         !zone cooling sizing factor
   DesignDay,                         !cooling design air flow method
   0,                         !cooling design air flow rate
   0.000762,                         !cooling min air flow per zone area
   0,                         !cooling min air flow
   0,                         !cooling min air flow fraction
   DesignDay,                         !heating design air flow method
   0,                         !heating design air flow rate
   0.002032,                         !heating max air flow per zone area
   0.1415762,                         !heating max air flow
   0.3;                         !heating max air flow fraction
Sizing:Zone,
   SPACE5-1,                         !Name of a zone
   14,                         !Zone cooling design supply air temperature
   50,                         !Zone heating design supply air temperature
   0.009,                         !Zone cooling design supply air humidity ratio
   0.004,                         !Zone heating design supply air humidity ratio
   flow/person,                         !outside air method
   0.00944,                         !outside air flow per person
   0,                         !outside air flow per zone area
   0,                         !outside air flow per zone
   0,                         !zone heating sizing factor
   0,                         !zone cooling sizing factor
   DesignDay,                         !cooling design air flow method
   0,                         !cooling design air flow rate
   0.000762,                         !cooling min air flow per zone area
   0,                         !cooling min air flow
   0,                         !cooling min air flow fraction
   DesignDay,                         !heating design air flow method
   0,                         !heating design air flow rate
   0.002032,                         !heating max air flow per zone area
   0.1415762,                         !heating max air flow
   0.3;                         !heating max air flow fraction
ZoneControl:Humidistat,
   Space2-1 Humidistat,                         !Humidistat Name
   SPACE2-1,                         !Zone Name
   Seasonal Relative Humidity Sch;                         !Relative Humidity SCHEDULE Name
ZoneControl:Thermostat,
   SPACE1-1 Control,                         !Thermostat Name
   SPACE1-1,                         !Zone Name
   Zone Control Type Sched,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:DualSetpoint,                         !Control Type #1
   DualSetPoint;                         !Control Type Name #1
ZoneControl:Thermostat,
   SPACE2-1 Control,                         !Thermostat Name
   SPACE2-1,                         !Zone Name
   Zone Control Type Sched,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:DualSetpoint,                         !Control Type #1
   DualSetPoint;                         !Control Type Name #1
ZoneControl:Thermostat,
   SPACE3-1 Control,                         !Thermostat Name
   SPACE3-1,                         !Zone Name
   Zone Control Type Sched,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:DualSetpoint,                         !Control Type #1
   DualSetPoint;                         !Control Type Name #1
ZoneControl:Thermostat,
   SPACE4-1 Control,                         !Thermostat Name
   SPACE4-1,                         !Zone Name
   Zone Control Type Sched,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:DualSetpoint,                         !Control Type #1
   DualSetPoint;                         !Control Type Name #1
ZoneControl:Thermostat,
   SPACE5-1 Control,                         !Thermostat Name
   SPACE5-1,                         !Zone Name
   Zone Control Type Sched,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:DualSetpoint,                         !Control Type #1
   DualSetPoint;                         !Control Type Name #1
CURVE:QUADRATIC,
   BoilerEfficiency,                         !Name
   1,                         !Coeff1 Constant
   0,                         !Coeff2 x
   0,                         !Coeff3 x**2
   0,                         !minimum value of x
   1,                         !maximum value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Dimensionless,                         !Input Unit Type for X
   Dimensionless;                         !Output Unit Type
ZoneHVAC:Baseboard:RadiantConvective:Water,
   SPACE2-1_SPACE2-1 Baseboard,                      !Name
   ReheatCoilAvailSched,                      !Availability Schedule Name
   SPACE2-1_SPACE2-1_Zone Coil Water In Node,                      !Inlet Node Name
   SPACE2-1_SPACE2-1_Zone Coil Water Out Node,                      !Outlet Node Name
   87.78,                      !Rated Average Water Temperature
   0.063,                      ! Rated Water Mass Flow Rate 
   autosize,                      !Rated Capacity 
   autosize,                      !Maximum Water Flow Rate
   0.001,                      !Convergence Tolerance
   0.3,                      !Fraction Radiant 
   0.3,                      ! Fraction of Radiant Energy Incident on People
   RIGHT-1,                         !surface name 1
   0.4,                         !flow fraction for surface 1
   C2-1,                         !surface name 2
   0.2,                         !flow fraction for surface 2
   SB25,                         !surface name 3
   0.1;                         !flow fraction for surface 3
ZoneHVAC:Baseboard:RadiantConvective:Water,
   SPACE4-1_SPACE4-1 Baseboard,                      !Name
   ReheatCoilAvailSched,                      !Availability Schedule Name
   SPACE4-1_SPACE4-1_Zone Coil Water In Node,                      !Inlet Node Name
   SPACE4-1_SPACE4-1_Zone Coil Water Out Node,                      !Outlet Node Name
   87.78,                      !Rated Average Water Temperature
   0.063,                      ! Rated Water Mass Flow Rate 
   autosize,                      !Rated Capacity 
   autosize,                      !Maximum Water Flow Rate
   0.001,                      !Convergence Tolerance
   0.3,                      !Fraction Radiant 
   0.3,                      ! Fraction of Radiant Energy Incident on People
   LEFT-1,                         !surface name 1
   0.4,                         !flow fraction for surface 1
   C4-1,                         !surface name 2
   0.2,                         !flow fraction for surface 2
   SB45,                         !surface name 3
   0.1;                         !flow fraction for surface 3
AirTerminal:SingleDuct:VAV:NoReheat,
   SPACE2-1_SPACE2-1 VAV System,                      !Name of System
   ReheatCoilAvailSched,                      !System Availability schedule
   SPACE2-1_SPACE2-1 In Node,                      !UNIT Air Outlet Node
   SPACE2-1_SPACE2-1 ATU In Node,                      !UNIT Air Inlet Node
   autosize,                      !Maximum air flow rate
   Constant,                      !Zone Minimum Air Flow Input Method
   0.3,                      !Constant Minimum Air Flow Fraction
   ,                      !Fixed Minimum Air Flow Rate
   ,                      !Minimum Air Flow Fraction Schedule Name
   ;                      !Design Specification Outdoor Air Object Name
ZoneHVAC:AirDistributionUnit,
   SPACE2-1_SPACE2-1 ATU,                      !Air Distribution Unit Name
   SPACE2-1_SPACE2-1 In Node,                      !Air Dist Unit Outlet Node Name
   AirTerminal:SingleDuct:VAV:NoReheat,                      !KEY--System Component Type 1
   SPACE2-1_SPACE2-1 VAV System,                      !Component Name 1
   ,                      !upstream nominal leakage fraction
   ;                      !downstream constant leakage fraction
AirTerminal:SingleDuct:VAV:NoReheat,
   SPACE4-1_SPACE4-1 VAV System,                      !Name of System
   ReheatCoilAvailSched,                      !System Availability schedule
   SPACE4-1_SPACE4-1 In Node,                      !UNIT Air Outlet Node
   SPACE4-1_SPACE4-1 ATU In Node,                      !UNIT Air Inlet Node
   autosize,                      !Maximum air flow rate
   Constant,                      !Zone Minimum Air Flow Input Method
   0.3,                      !Constant Minimum Air Flow Fraction
   ,                      !Fixed Minimum Air Flow Rate
   ,                      !Minimum Air Flow Fraction Schedule Name
   ;                      !Design Specification Outdoor Air Object Name
ZoneHVAC:AirDistributionUnit,
   SPACE4-1_SPACE4-1 ATU,                      !Air Distribution Unit Name
   SPACE4-1_SPACE4-1 In Node,                      !Air Dist Unit Outlet Node Name
   AirTerminal:SingleDuct:VAV:NoReheat,                      !KEY--System Component Type 1
   SPACE4-1_SPACE4-1 VAV System,                      !Component Name 1
   ,                      !upstream nominal leakage fraction
   ;                      !downstream constant leakage fraction
AirTerminal:SingleDuct:VAV:Reheat,
   SPACE1-1_SPACE1-1 VAV Reheat,                      !Name of System
   ReheatCoilAvailSched,                      !System Availability schedule
   SPACE1-1_SPACE1-1 Zone Coil Air In Node,                      !DAMPER Air Outlet Node
   SPACE1-1_SPACE1-1 ATU In Node,                      !UNIT Air Inlet Node
   autosize,                      !Maximum air flow rate
   Constant,                      !Zone Minimum Air Flow Input Method
   0.3,                      !Constant Minimum Air Flow Fraction
   ,                      !Fixed Minimum Air Flow Rate
   ,                      !Minimum Air Flow Fraction Schedule Name
   COIL:Heating:Water,                      !Reheat Component Object
   SPACE1-1_SPACE1-1 Zone Coil,                      !Name of Reheat Component
   autosize,                      !Max Reheat Water Flow
   0,                      !Min Reheat Water Flow
   SPACE1-1_SPACE1-1 In Node,                      !UNIT Air Outlet Node
   0.001,                      !Convergence Tolerance
   REVERSEACTION,                      !Damper Heating Action
   ,                      !Maximum Flow per Zone Floor Area During Reheat
   ,                      !Maximum Flow Fraction During Reheat
   ,                      !Maximum Reheat Air Temperature
   ;                      !Design Specification Outdoor Air Object Name
COIL:Heating:Water,
   SPACE1-1_SPACE1-1 Zone Coil,                      !Coil Name
   ReheatCoilAvailSched,                      !Available Schedule
   autosize,                      !UA of the Coil
   autosize,                      !Max Water Flow Rate of Coil
   SPACE1-1_SPACE1-1 Zone Coil Water In Node,                      !Coil_Water_Inlet_Node
   SPACE1-1_SPACE1-1 Zone Coil Water Out Node,                      !Coil_Water_Outlet_Node
   SPACE1-1_SPACE1-1 Zone Coil Air In Node,                      !Coil_Air_Inlet_Node
   SPACE1-1_SPACE1-1 In Node,                      !Coil_Air_Outlet_Node
   UFactorTimesAreaAndDesignWaterFlowRate,                      !Coil Performance Input Method
   autosize,                      !Nominal Capacity
   82.2,                      !Design Inlet Water Temperature
   16.6,                      !Design Inlet Air Temperature
   71.1,                      !Design Outlet Water Temperature
   32.2,                      !Design Outlet Air Temperature
   0.5;                      !Rated Ratio for Air and Water Convection
ZoneHVAC:AirDistributionUnit,
   SPACE1-1_SPACE1-1 ATU,                      !Air Distribution Unit Name
   SPACE1-1_SPACE1-1 In Node,                      !Air Dist Unit Outlet Node Name
   AirTerminal:SingleDuct:VAV:Reheat,                      !KEY--System Component Type
   SPACE1-1_SPACE1-1 VAV Reheat,                      !Component Name
   ,                      !upstream nominal leakage fraction
   ;                      !downstream constant leakage fraction
AirTerminal:SingleDuct:VAV:Reheat,
   SPACE3-1_SPACE3-1 VAV Reheat,                      !Name of System
   ReheatCoilAvailSched,                      !System Availability schedule
   SPACE3-1_SPACE3-1 Zone Coil Air In Node,                      !DAMPER Air Outlet Node
   SPACE3-1_SPACE5-1 ATU In Node,                      !UNIT Air Inlet Node
   autosize,                      !Maximum air flow rate
   Constant,                      !Zone Minimum Air Flow Input Method
   0.3,                      !Constant Minimum Air Flow Fraction
   ,                      !Fixed Minimum Air Flow Rate
   ,                      !Minimum Air Flow Fraction Schedule Name
   COIL:Heating:Water,                      !Reheat Component Object
   SPACE3-1_SPACE3-1 Zone Coil,                      !Name of Reheat Component
   autosize,                      !Max Reheat Water Flow
   0,                      !Min Reheat Water Flow
   SPACE3-1_SPACE3-1 In Node,                      !UNIT Air Outlet Node
   0.001,                      !Convergence Tolerance
   REVERSEACTION,                      !Damper Heating Action
   ,                      !Maximum Flow per Zone Floor Area During Reheat
   ,                      !Maximum Flow Fraction During Reheat
   ,                      !Maximum Reheat Air Temperature
   ;                      !Design Specification Outdoor Air Object Name
COIL:Heating:Water,
   SPACE3-1_SPACE3-1 Zone Coil,                      !Coil Name
   ReheatCoilAvailSched,                      !Available Schedule
   autosize,                      !UA of the Coil
   autosize,                      !Max Water Flow Rate of Coil
   SPACE3-1_SPACE3-1 Zone Coil Water In Node,                      !Coil_Water_Inlet_Node
   SPACE3-1_SPACE3-1 Zone Coil Water Out Node,                      !Coil_Water_Outlet_Node
   SPACE3-1_SPACE3-1 Zone Coil Air In Node,                      !Coil_Air_Inlet_Node
   SPACE3-1_SPACE3-1 In Node,                      !Coil_Air_Outlet_Node
   UFactorTimesAreaAndDesignWaterFlowRate,                      !Coil Performance Input Method
   autosize,                      !Nominal Capacity
   82.2,                      !Design Inlet Water Temperature
   16.6,                      !Design Inlet Air Temperature
   71.1,                      !Design Outlet Water Temperature
   32.2,                      !Design Outlet Air Temperature
   0.5;                      !Rated Ratio for Air and Water Convection
ZoneHVAC:AirDistributionUnit,
   SPACE3-1_SPACE3-1 ATU,                      !Air Distribution Unit Name
   SPACE3-1_SPACE3-1 In Node,                      !Air Dist Unit Outlet Node Name
   AirTerminal:SingleDuct:VAV:Reheat,                      !KEY--System Component Type
   SPACE3-1_SPACE3-1 VAV Reheat,                      !Component Name
   ,                      !upstream nominal leakage fraction
   ;                      !downstream constant leakage fraction
AirTerminal:SingleDuct:VAV:Reheat,
   SPACE5-1_SPACE5-1 VAV Reheat,                      !Name of System
   ReheatCoilAvailSched,                      !System Availability schedule
   SPACE5-1_SPACE5-1 Zone Coil Air In Node,                      !DAMPER Air Outlet Node
   SPACE5-1_SPACE5-1 ATU In Node,                      !UNIT Air Inlet Node
   autosize,                      !Maximum air flow rate
   Constant,                      !Zone Minimum Air Flow Input Method
   0.3,                      !Constant Minimum Air Flow Fraction
   ,                      !Fixed Minimum Air Flow Rate
   ,                      !Minimum Air Flow Fraction Schedule Name
   COIL:Heating:Water,                      !Reheat Component Object
   SPACE5-1_SPACE5-1 Zone Coil,                      !Name of Reheat Component
   autosize,                      !Max Reheat Water Flow
   0,                      !Min Reheat Water Flow
   SPACE5-1_SPACE5-1 In Node,                      !UNIT Air Outlet Node
   0.001,                      !Convergence Tolerance
   REVERSEACTION,                      !Damper Heating Action
   ,                      !Maximum Flow per Zone Floor Area During Reheat
   ,                      !Maximum Flow Fraction During Reheat
   ,                      !Maximum Reheat Air Temperature
   ;                      !Design Specification Outdoor Air Object Name
COIL:Heating:Water,
   SPACE5-1_SPACE5-1 Zone Coil,                      !Coil Name
   ReheatCoilAvailSched,                      !Available Schedule
   autosize,                      !UA of the Coil
   autosize,                      !Max Water Flow Rate of Coil
   SPACE5-1_SPACE5-1 Zone Coil Water In Node,                      !Coil_Water_Inlet_Node
   SPACE5-1_SPACE5-1 Zone Coil Water Out Node,                      !Coil_Water_Outlet_Node
   SPACE5-1_SPACE5-1 Zone Coil Air In Node,                      !Coil_Air_Inlet_Node
   SPACE5-1_SPACE5-1 In Node,                      !Coil_Air_Outlet_Node
   UFactorTimesAreaAndDesignWaterFlowRate,                      !Coil Performance Input Method
   autosize,                      !Nominal Capacity
   82.2,                      !Design Inlet Water Temperature
   16.6,                      !Design Inlet Air Temperature
   71.1,                      !Design Outlet Water Temperature
   32.2,                      !Design Outlet Air Temperature
   0.5;                      !Rated Ratio for Air and Water Convection
ZoneHVAC:AirDistributionUnit,
   SPACE5-1_SPACE5-1 ATU,                      !Air Distribution Unit Name
   SPACE5-1_SPACE5-1 In Node,                      !Air Dist Unit Outlet Node Name
   AirTerminal:SingleDuct:VAV:Reheat,                      !KEY--System Component Type
   SPACE5-1_SPACE5-1 VAV Reheat,                      !Component Name
   ,                      !upstream nominal leakage fraction
   ;                      !downstream constant leakage fraction
Fan:VariableVolume,
   Supply Fan 1,                         !Fan Name
   FanAvailSched,                         !Available Schedule
   0.7,                         !Fan Total Efficiency
   600,                         !Delta Pressure
   autosize,                         !Max Flow Rate
   Fraction,                         !Fan Power Minimum Flow Rate Input Method
   0.25,                         !Fan Power Minimum Flow Fraction
   ,                         !Fan Power Minimum Air Flow Rate
   0.9,                         !Motor Efficiency
   1.0,                         !Motor In Airstream Fraction
   .35071223,                         !FanCoefficient 1
   .30850535,                         !FanCoefficient 2
   -.54137364,                         !FanCoefficient 3
   .87198823,                         !FanCoefficient 4
   0,                         !FanCoefficient 5
   Main Heating Coil 1 Outlet Node,                         !Fan_Inlet_Node
   VAV Sys 1 Outlet Node,                         !Fan_Outlet_Node
   General;                         !End-Use Subcategory
COIL:Cooling:Water,
   Main Cooling Coil 1,                         !Coil Name
   CoolingCoilAvailSched,                         !Available Schedule
   autosize,                         !Design Water Flow Rate of Coil
   autosize,                         !Design Air Volume Flow Rate
   autosize,                         !Design Inlet Water Temperature
   autosize,                         !Design Inlet Air Temperature
   12.5018,                         !Design Outlet Air Temperature
   autosize,                         !Design Inlet Air Humidity Ratio 
   0.008,                         !Design Outlet Air Humidity Ratio
   Main Cooling Coil 1 Water Inlet Node,                         !Coil_Water_Inlet_Node
   Main Cooling Coil 1 Water Outlet Node,                         !Coil_Water_Outlet_Node
   Mixed Air Node 1,                         !Coil_Air_Inlet_Node
   Main Cooling Coil 1 Outlet Node,                         !Coil_Air_Outlet_Node
   SIMPLEANALYSIS,                         !Type of Analysis
   CrossFlow,                         !Heat Exchanger Configuration
   ;                         !Name of Water Storage Tank for Condensate Collection
COIL:Heating:Water,
   Main Heating Coil 1,                         !Coil Name
   ReheatCoilAvailSched,                         !Available Schedule
   autosize,                         !UA of the Coil
   autosize,                         !Max Water Flow Rate of Coil
   Main Heating Coil 1 Water Inlet Node,                         !Coil_Water_Inlet_Node
   Main Heating Coil 1 Water Outlet Node,                         !Coil_Water_Outlet_Node
   Main Cooling Coil 1 Outlet Node,                         !Coil_Air_Inlet_Node
   Main Heating Coil 1 Outlet Node,                         !Coil_Air_Outlet_Node
   UFactorTimesAreaAndDesignWaterFlowRate,                         !Coil Performance Input Method
   autosize,                         !Nominal Capacity
   82.2,                         !Design Inlet Water Temperature
   16.6,                         !Design Inlet Air Temperature
   71.1,                         !Design Outlet Water Temperature
   32.2,                         !Design Outlet Air Temperature
   0.5;                         !Rated Ratio for Air and Water Convection
ZoneHVAC:EquipmentConnections,
   SPACE1-1,                      !Zone Name
   SPACE1-1_SPACE1-1 Eq,                      !List Name: Zone Equipment
   SPACE1-1_SPACE1-1 In Node,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   SPACE1-1_SPACE1-1 Node,                      !Zone Air Node Name
   SPACE1-1_SPACE1-1 Out Node;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   SPACE2-1,                      !Zone Name
   SPACE2-1_SPACE2-1 Eq,                      !List Name: Zone Equipment
   SPACE2-1_SPACE2-1 In Node,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   SPACE2-1_SPACE2-1 Node,                      !Zone Air Node Name
   SPACE2-1_SPACE2-1 Out Node;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   SPACE3-1,                      !Zone Name
   SPACE3-1_SPACE3-1 Eq,                      !List Name: Zone Equipment
   SPACE3-1_SPACE3-1 In Node,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   SPACE3-1_SPACE3-1 Node,                      !Zone Air Node Name
   SPACE3-1_SPACE3-1 Out Node;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   SPACE4-1,                      !Zone Name
   SPACE4-1_SPACE4-1 Eq,                      !List Name: Zone Equipment
   SPACE4-1_SPACE4-1 In Node,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   SPACE4-1_SPACE4-1 Node,                      !Zone Air Node Name
   SPACE4-1_SPACE4-1 Out Node;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   SPACE5-1,                      !Zone Name
   SPACE5-1_SPACE5-1 Eq,                      !List Name: Zone Equipment
   SPACE5-1_SPACE5-1 In Node,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   SPACE5-1_SPACE5-1 Node,                      !Zone Air Node Name
   SPACE5-1_SPACE5-1 Out Node;                      !Zone Return Air Node Name
OutdoorAir:Mixer,
   OA Mixing Box 1,                         !Name
   Mixed Air Node 1,                         !Mixed_Air_Node
   Outside Air Inlet Node 1,                         !Outside_Air_Stream_Node
   Relief Air Outlet Node 1,                         !Relief_Air_Stream_Node
   VAV Sys 1 Inlet Node;                         !Return_Air_Stream_Node
AirLoopHVAC:OutdoorAirSystem,
   OA Sys 1,                         !Name
   OA Sys 1 Controllers,                         !Name: Controller List
   OA Sys 1 Equipment,                         !Name of an Air Loop Equipment List
   VAV Sys 1 Avail List;                         !Name of a System Availability Manager List
Pump:VariableSpeed,
   HW Circ Pump,                         !Pump Name
   HW Supply Inlet Node,                         !Inlet_Node
   HW Pump Outlet Node,                         !Outlet_Node
   autosize,                         !Rated Volumetric Flow Rate
   179352,                         !Rated Pump Head
   autosize,                         !Rated Power Consumption
   0.9,                         !Motor Efficiency
   0,                         !Fraction of Motor Inefficiencies to Fluid Stream
   0,                         !Coefficient1 of the Part Load Performance Curve
   1,                         !Coefficient2 of the Part Load Performance Curve
   0,                         !Coefficient3 of the Part Load Performance Curve
   0,                         !Coefficient4 of the Part Load Performance Curve
   0,                         !Min Flow Rate while operating in variable flow capacity
   INTERMITTENT,                         !Pump Control Type
   ;                         !Pump Flow Rate Schedule Name
Pump:VariableSpeed,
   CW Circ Pump,                         !Pump Name
   CW Supply Inlet Node,                         !Inlet_Node
   CW Pump Outlet Node,                         !Outlet_Node
   autosize,                         !Rated Volumetric Flow Rate
   179352,                         !Rated Pump Head
   autosize,                         !Rated Power Consumption
   0.9,                         !Motor Efficiency
   0,                         !Fraction of Motor Inefficiencies to Fluid Stream
   0,                         !Coefficient1 of the Part Load Performance Curve
   1,                         !Coefficient2 of the Part Load Performance Curve
   0,                         !Coefficient3 of the Part Load Performance Curve
   0,                         !Coefficient4 of the Part Load Performance Curve
   0,                         !Min Flow Rate while operating in variable flow capacity
   INTERMITTENT,                         !Pump Control Type
   CoolingPumpAvailSched;                         !Pump Flow Rate Schedule Name
Boiler:HotWater,
   Central Boiler,                         !Name
   NaturalGas,                         !Fuel Type
   autosize,                         !Nominal Capacity
   0.8,                         !Nominal Thermal Efficiency
   ,                         !Normalized Boiler Efficiency Curve Name
   81,                         !Design Water Outlet Temperature
   autosize,                         !Design Water Flow Rate
   0.0,                         !Minimum Part Load Ratio
   1.2,                         !Maximum Part Load Ratio
   1.0,                         !Optimum Part Load Ratio
   Central Boiler Inlet Node,                         !Boiler Water Inlet Node Name
   Central Boiler Outlet Node,                         !Boiler Water Outlet Node Name
   100,                         !Water Outlet Upper Temperature Limit
   VariableFlow,                         !Boiler Flow Mode
   ,                         !Parasitic Electric Load
   1.0;                         !Sizing Factor
CHILLER:ELECTRIC,
   Central Chiller,                         !Chiller Name
   WaterCooled,                         !Condenser Type
   autosize,                         !Nominal Capacity
   3.2,                         !COP
   Central Chiller Inlet Node,                         !Plant_Side_Inlet_Node
   Central Chiller Outlet Node,                         !Plant_Side_Outlet_Node
   Central Chiller Condenser Inlet Node,                         !Condenser_Side_Inlet_Node
   Central Chiller Condenser Outlet Node,                         !Condenser_Side_Outlet_Node
   0,                         !Minimum Part Load Ratio
   1,                         !Maximum Part Load Ratio
   0.65,                         !Opt Part Load Ratio
   29.44,                         !Temp Design Condenser Inlet
   2.682759,                         !Temp Rise Coefficient
   6.667,                         !Temp Design Evaporator Outlet
   autosize,                         !Design Evaporator Volumetric Water Flow Rate
   autosize,                         !Design Condenser Volumetric Water Flow Rate
   .944836,                         !Coefficient1 of the capacity ratio curve
   -.0570088,                         !Coefficient2 of the capacity ratio curve
   -.00185486,                         !Coefficient3 of the capacity ratio curve
   1.907846,                         !Coefficient1 of the power ratio curve
   -1.204987,                         !Coefficient2 of the power ratio curve
   .2634623,                         !Coefficient3 of the power ratio curve
   .03303,                         !Coefficient1 of the full load ratio curve
   .6852,                         !Coefficient2 of the full load ratio curve
   .2818,                         !Coefficient3 of the full load ratio curve
   5,                         !Temp Lower Limit Evaporator Outlet
   VariableFlow,                         !Chiller Flow Mode
   0.0,                         !Design heat recovery water flow rate
   ,                         !Heat_Recovery_Side_Inlet_Node
   ,                         !Heat_Recovery_Side_Outlet_Node
   1.0,                         !Sizing Factor
   0.0,                         !Basin Heater Capacity
   2.0,                         !Basin Heater Setpoint Temperature
   ;                         !Basin Heater Operating Schedule Name
COOLINGTOWER:SINGLESPEED,
   Central Tower,                         !Tower Name
   Condenser Tower Inlet Node,                         !Water Inlet Node Name
   Condenser Tower Outlet Node,                         !Water Outlet Node Name
   autosize,                         !Design Water Flow Rate
   autosize,                         !Design Air Flow Rate
   autosize,                         !Fan Power at Design Air Flow Rate
   autosize,                         !Tower UA Value at Design Air Flow Rate
   0.0,                         !Air Flow Rate in Free Convection Regime
   0.0,                         !Tower UA Value at Free Convection Air Flow Rate
   UFactorTimesAreaAndDesignWaterFlowRate,                         !Tower Performance Input Method
   ,                         !Tower Nominal Capacity
   ,                         !Tower Free Convection Capacity
   0.0,                         !Basin Heater Capacity
   2.0,                         !Basin Heater Setpoint Temperature
   ,                         !Basin Heater Operating Schedule Name
   ,                         !Evaporation Loss Mode
   0.2,                         !Evaporation Loss Factor
   0.008,                         !Drift Loss Percent
   ,                         !Blowdown Calculation Mode
   3.0,                         !Blowdown Concentration Ratio
   ,                         !Schedule Name for Makeup Water Usage due to Blowdown 
   ,                         !Name of Water Storage Tank for Supply
   ,                         !Outdoor Air Inlet Node Name
   FanCycling,                         !Capacity Control
   ,                         !Number of Cells
   MinimalCell,                         !Cell Control
   ,                         !Cell Minimum  Water Flow Rate Fraction
   ,                         !Cell Maximum Water Flow Rate Fraction
   ;                         !Sizing Factor
Pipe:Adiabatic,
   Heating Supply Side Bypass,                         !Name
   Heating Supply Bypass Inlet Node,                         !Inlet Node Name
   Heating Supply Bypass Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Heating Supply Outlet,                         !Name
   Heating Supply Exit Pipe Inlet Node,                         !Inlet Node Name
   HW Supply Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Heating Demand Inlet Pipe,                         !Name
   HW Demand Inlet Node,                         !Inlet Node Name
   HW Demand Entrance Pipe Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Heating Demand Outlet Pipe,                         !Name
   HW Demand Exit Pipe Inlet Node,                         !Inlet Node Name
   HW Demand Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Heating Demand Bypass,                         !Name
   Heating Demand Bypass Inlet Node,                         !Inlet Node Name
   Heating Demand Bypass Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Cooling Demand Side Inlet Pipe,                         !Name
   CW Demand Inlet Node,                         !Inlet Node Name
   CW Demand Entrance Pipe Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Cooling Demand Side Bypass,                         !Name
   CW Demand Bypass Inlet Node,                         !Inlet Node Name
   CW Demand Bypass Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   CW Demand Side Outlet Pipe,                         !Name
   CW Demand Exit Pipe Inlet Node,                         !Inlet Node Name
   CW Demand Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Supply Side Outlet Pipe,                         !Name
   Supply Side Exit Pipe Inlet Node,                         !Inlet Node Name
   CW Supply Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Supply Side Bypass,                         !Name
   CW Supply Bypass Inlet Node,                         !Inlet Node Name
   CW Supply Bypass Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Condenser Supply Side Bypass,                         !Name
   Cond Supply Bypass Inlet Node,                         !Inlet Node Name
   Cond Supply Bypass Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Condenser Supply Outlet,                         !Name
   Condenser Supply Exit Pipe Inlet Node,                         !Inlet Node Name
   Condenser Supply Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Condenser Demand Inlet Pipe,                         !Name
   Condenser Demand Inlet Node,                         !Inlet Node Name
   Condenser Demand Entrance Pipe Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Condenser Demand Side Bypass,                         !Name
   Cond Demand Bypass Inlet Node,                         !Inlet Node Name
   Cond Demand Bypass Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Condenser Demand Outlet Pipe,                         !Name
   Condenser Demand Exit Pipe Inlet Node,                         !Inlet Node Name
   Condenser Demand Outlet Node;                         !Outlet Node Name
Pump:VariableSpeed,
   Cond Circ Pump,                         !Pump Name
   Condenser Supply Inlet Node,                         !Inlet_Node
   Condenser Pump Outlet Node,                         !Outlet_Node
   autosize,                         !Rated Volumetric Flow Rate
   179352,                         !Rated Pump Head
   autosize,                         !Rated Power Consumption
   0.9,                         !Motor Efficiency
   0,                         !Fraction of Motor Inefficiencies to Fluid Stream
   0,                         !Coefficient1 of the Part Load Performance Curve
   1,                         !Coefficient2 of the Part Load Performance Curve
   0,                         !Coefficient3 of the Part Load Performance Curve
   0,                         !Coefficient4 of the Part Load Performance Curve
   0,                         !Min Flow Rate while operating in variable flow capacity
   INTERMITTENT,                         !Pump Control Type
   CoolingPumpAvailSched;                         !Pump Flow Rate Schedule Name
AirLoopHVAC:ZoneSplitter,
   Zone Supply Air Splitter 1,                         !Splitter Name
   Zone Eq In Node,                         !Inlet_Node
   SPACE1-1_SPACE1-1 ATU In Node,                         !Outlet_Node_1
   SPACE2-1_SPACE2-1 ATU In Node,                         !Outlet_Node_2
   SPACE3-1_SPACE5-1 ATU In Node,                         !Outlet_Node_3
   SPACE4-1_SPACE4-1 ATU In Node,                         !Outlet_Node_4
   SPACE5-1_SPACE5-1 ATU In Node;                         !Outlet_Node_5
AirLoopHVAC:ReturnPlenum,
   Return-Plenum-1,                         !Zone Plenum Name
   PLENUM-1,                         !Zone Name
   PLENUM-1 Node,                         !Zone Node Name
   Plenum-1 Outlet Node,                         !Outlet_Node
   SPACE1-1_SPACE1-1 Out Node,                         !Inlet_Node_1
   SPACE2-1_SPACE2-1 Out Node,                         !Inlet_Node_2
   SPACE3-1_SPACE3-1 Out Node,                         !Inlet_Node_3
   SPACE4-1_SPACE4-1 Out Node,                         !Inlet_Node_4
   SPACE5-1_SPACE5-1 Out Node;                         !Inlet_Node_5
Connector:Splitter,
   Heating Demand Splitter,                         !SplitterName
   Heating Demand Inlet Branch,                         !Inlet Branch Name
   SPACE1-1_SPACE1-1 Reheat Branch,                         !Outlet Branch Name 1
   SPACE2-1_SPACE2-1 Baseboard Branch,                         !Outlet Branch Name 2
   SPACE3-1_SPACE3-1 Reheat Branch,                         !Outlet Branch Name 3
   SPACE4-1_SPACE4-1 Baseboard Branch,                         !Outlet Branch Name 4
   SPACE5-1_SPACE5-1 Reheat Branch,                         !Outlet Branch Name 5
   Main Heating Coil 1 Branch,                         !Outlet Branch Name 6
   Heating Demand Bypass Branch;                         !Outlet Branch Name 7
Connector:Splitter,
   Heating Supply Splitter,                         !SplitterName
   Heating Supply Inlet Branch,                         !Inlet Branch Name
   Central Boiler Branch,                         !Outlet Branch Name 1
   Heating Supply Bypass Branch;                         !Outlet Branch Name 2
Connector:Splitter,
   CW Loop Splitter,                         !SplitterName
   CW Pump Branch,                         !Inlet Branch Name
   Central Chiller Branch,                         !Outlet Branch Name 1
   Cooling Supply Bypass Branch;                         !Outlet Branch Name 2
Connector:Splitter,
   CW Demand Splitter,                         !SplitterName
   Cooling Demand Inlet,                         !Inlet Branch Name
   Cooling Coil Branch,                         !Outlet Branch Name 1
   Cooling Demand Bypass Branch;                         !Outlet Branch Name 2
Connector:Splitter,
   Condenser Demand Splitter,                         !SplitterName
   Condenser Demand Inlet Branch,                         !Inlet Branch Name
   Central Chiller Condenser Branch,                         !Outlet Branch Name 1
   Condenser Demand Bypass Branch;                         !Outlet Branch Name 2
Connector:Splitter,
   Condenser Supply Splitter,                         !SplitterName
   Condenser Supply Inlet Branch,                         !Inlet Branch Name
   Condenser Supply Tower Branch,                         !Outlet Branch Name 1
   Condenser Supply Bypass Branch;                         !Outlet Branch Name 2
Connector:Mixer,
   Heating Demand Mixer,                         !MixerName
   Heating Demand Outlet Branch,                         !Outlet Branch Name
   SPACE1-1_SPACE1-1 Reheat Branch,                         !Inlet Branch Name 1
   SPACE2-1_SPACE2-1 Baseboard Branch,                         !Inlet Branch Name 2
   SPACE3-1_SPACE3-1 Reheat Branch,                         !Inlet Branch Name 3
   SPACE4-1_SPACE4-1 Baseboard Branch,                         !Inlet Branch Name 4
   SPACE5-1_SPACE5-1 Reheat Branch,                         !Inlet Branch Name 5
   Main Heating Coil 1 Branch,                         !Inlet Branch Name 6
   Heating Demand Bypass Branch;                         !Inlet Branch Name 7
Connector:Mixer,
   Heating Supply Mixer,                         !MixerName
   Heating Supply Outlet Branch,                         !Outlet Branch Name
   Central Boiler Branch,                         !Inlet Branch Name 1
   Heating Supply Bypass Branch;                         !Inlet Branch Name 2
Connector:Mixer,
   CW Loop Mixer,                         !MixerName
   Cooling Supply Outlet,                         !Outlet Branch Name
   Central Chiller Branch,                         !Inlet Branch Name 1
   Cooling Supply Bypass Branch;                         !Inlet Branch Name 2
Connector:Mixer,
   CW Demand Mixer,                         !MixerName
   Cooling Demand Outlet,                         !Outlet Branch Name
   Cooling Coil Branch,                         !Inlet Branch Name 1
   Cooling Demand Bypass Branch;                         !Inlet Branch Name 2
Connector:Mixer,
   Condenser Demand Mixer,                         !MixerName
   Condenser Demand Outlet Branch,                         !Outlet Branch Name
   Central Chiller Condenser Branch,                         !Inlet Branch Name 1
   Condenser Demand Bypass Branch;                         !Inlet Branch Name 2
Connector:Mixer,
   Condenser Supply Mixer,                         !MixerName
   Condenser Supply Outlet Branch,                         !Outlet Branch Name
   Condenser Supply Tower Branch,                         !Inlet Branch Name 1
   Condenser Supply Bypass Branch;                         !Inlet Branch Name 2

