ScheduleTypeLimits,
   Any Number,                         !ScheduleType Name
   ,                         !Lower Limit Value
   ,                         !Upper Limit Value
   ,                         !Numeric Type
   ;                         !Unit Type
Schedule:Compact,
   System Availability Schedule,                         !Name
   Any Number,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Alldays,                         !Complex Field #2
   Until:24:00,1;                         !Complex Field #3
Schedule:Compact,
   Fan Availability Schedule,                         !Name
   Any Number,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Alldays,                         !Complex Field #2
   Until:12:00,1,                         !Complex Field #3
   Until:24:00,0;                         !Complex Field #4
Schedule:Compact,
   Zone Control Type Sched,                         !Name
   Any Number,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Alldays,                         !Complex Field #2
   Until:24:00,1;                         !Complex Field #3
Schedule:Compact,
   Heating Setpoint Schedule,                         !Name
   Any Number,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Alldays,                         !Complex Field #2
   Until:24:00,20;                         !Complex Field #3
NodeList,
   Main Zone_Main Zone_Inlet Nodelist,                      !Node List Name
   Main Zone_Main Zone Inlet Node;                      !Node_ID_1
BranchList,
   Air Loop Branches,                         !Branch List Name
   Air Loop Main Branch;                         !Branch Name 1
AirLoopHVAC,
   Evap Cooler System,                         !Primary Air Loop Name
   ,                         !Name: Controller List
   Evap Cooler Availability List,                         !Name: System Availability Manager List
   2,                         !Primary air design volumetric flow rate
   Air Loop Branches,                         !Air Loop Branch List Name
   ,                         !Air Loop Connector List Name
   Supply Inlet Node,                         !ReturnAir AirLoop Inlet Node
   Zone Equipment Outlet Node,                         !ZoneEquipGroup Outlet Node
   Zone Equipment Inlet Node,                         !SupplyAirPath ZoneEquipGroup Inlet Nodes
   Supply Outlet Node;                         !AirLoop Outlet Nodes
AirLoopHVAC:SupplyPath,
   Zone Supply Air Path,                         !Name
   Zone Equipment Inlet Node,                         !Supply Air Path Inlet Node Name
   AirLoopHVAC:ZoneSplitter,                         !Component 1 Object Type
   Zone Supply Air Splitter;                         !Component 1 Name
AirLoopHVAC:ReturnPath,
   Zone Return Air Path,                         !Name
   Zone Equipment Outlet Node,                         !Return Air Path Outlet Node Name
   AirLoopHVAC:ZoneMixer,                         !Component 1 Object Type
   Zone Return Air Mixer;                         !Component 1 Name
Branch,
   Air Loop Main Branch,                         !Branch Name
   2,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   AirLoopHVAC:OutdoorAirSystem,                         !Comp1 Type
   Outside Air System,                         !Comp1 Name
   Supply Inlet Node,                         !Comp1 Inlet Node Name
   Fan Inlet Node,                         !Comp1 Outlet Node Name
   PASSIVE,                         !Comp1 Branch Control Type
   Fan:ConstantVolume,                         !Comp2 Type
   Supply Fan,                         !Comp2 Name
   Fan Inlet Node,                         !Comp2 Inlet Node Name
   Evap Cooler Inlet Node,                         !Comp2 Outlet Node Name
   ACTIVE,                         !Comp2 Branch Control Type
   EvaporativeCooler:Direct:CelDekPad,                         !Comp3 Type
   Evaporative Cooler,                         !Comp3 Name
   Evap Cooler Inlet Node,                         !Comp3 Inlet Node Name
   Supply Outlet Node,                         !Comp3 Outlet Node Name
   PASSIVE;                         !Comp3 Branch Control Type
ZoneHVAC:EquipmentList,
   Main Zone_Main Zone Equipment,                      !Name
   AirTerminal:SingleDuct:Uncontrolled,                      !KEY--Zone Equipment Type 1
   Main Zone_Main Zone Direct Air,                      !Type Name 1
   1,                      !Cooling Priority 1
   2,                      !Heating Priority 1
   ZoneHVAC:Baseboard:Convective:Electric,                      !KEY--Zone Equipment Type 2
   Main Zone_Main Zone Baseboard,                      !Type Name 2
   2,                      !Cooling Priority 2
   ;                      !Heating Priority 2
AirLoopHVAC:OutdoorAirSystem:EquipmentList,
   Outside Air System Equipment,                         !Name
   OutdoorAir:Mixer,                         !KEY--System Component 1
   Outside Air Mixing Box;                         !Component Name 1
AirLoopHVAC:ControllerList,
   Outside Air System Controllers,                         !Name
   Controller:OutdoorAir,                         !Controller Type 1
   Outside Air Controller;                         !Controller Name 1
Controller:OutdoorAir,
   Outside Air Controller,                         !Name
   Relief Air Outlet Node,                         !Relief Air Outlet Node Name
   Supply Inlet Node,                         !Return Air Node Name
   Fan Inlet Node,                         !Mixed Air Node Name
   Outside Air Inlet Node,                         !Actuator Node Name
   2,                         !Minimum Outdoor Air Flow Rate
   2,                         !Maximum Outdoor Air Flow Rate
   NoEconomizer,                         !Economizer Control Type
   ModulateFlow,                         !Economizer Control Action Type
   ,                         !Economizer Maximum Limit Dry-Bulb Temperature
   ,                         !Economizer Maximum Limit Enthalpy
   ,                         !Economizer Maximum Limit Dewpoint Temperature
   ,                         !Electronic Enthalpy Limit Curve Name
   ,                         !Economizer Minimum Limit Dry-Bulb Temperature
   NoLockout,                         !Lockout Type
   FixedMinimum,                         !Minimum Limit Type
   ,                         !Minimum Outdoor Air Schedule Name
   ,                         !Minimum Fraction of Outdoor Air Schedule Name
   ,                         !Maximum Fraction of Outdoor Air Schedule Name
   ,                         !Mechanical Ventilation Controller Name
   ,                         !Time of Day Economizer Control Schedule Name
   ,                         !High Humidity Control
   ,                         !Humidistat Control Zone Name
   ,                         !High Humidity Outdoor Air Flow Ratio
   ,                         !Control High Indoor Humidity Based on Outdoor Humidity Ratio
   ;                         !Heat Recovery Bypass Control Type
AvailabilityManagerAssignmentList,
   Evap Cooler Availability List,                         !Name
   AvailabilityManager:HighTemperatureTurnOn,                         !System Availability Manager Type 1
   High Temperature Turn On Availability Manager,                         !System Availability Manager Name 1
   AvailabilityManager:LowTemperatureTurnOff,                         !System Availability Manager Type 2
   Low Temperature Turn Off Availability Manager;                         !System Availability Manager Name 2
AvailabilityManager:HighTemperatureTurnOn,
   High Temperature Turn On Availability Manager,                         !Name
   Main Zone_Main Zone Outlet Node,                         !Sensor Node
   27;                         !Temperature
AvailabilityManager:LowTemperatureTurnOff,
   Low Temperature Turn Off Availability Manager,                         !Name
   Main Zone_Main Zone Outlet Node,                         !Sensor Node
   23,                         !Temperature
   ;                         !Applicability schedule name
OutdoorAir:Node,
   Outside Air Inlet Node,                         !Node Name
   ;                         !Height Above Ground
ThermostatSetpoint:SingleHeating,
   Heating Setpoint,                         !Name
   Heating Setpoint Schedule;                         !Setpoint Temperature SCHEDULE Name
ZoneControl:Thermostat,
   Main Zone Thermostat,                         !Thermostat Name
   Main Zone,                         !Zone Name
   Zone Control Type Sched,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:SingleHeating,                         !Control Type #1
   Heating Setpoint;                         !Control Type Name #1
ZoneHVAC:Baseboard:Convective:Electric,
   Main Zone_Main Zone Baseboard,                      !Name
   System Availability Schedule,                      !Available Schedule Name 
   8000,                      !Nominal Capacity
   0.97;                      !Efficiency
AirTerminal:SingleDuct:Uncontrolled,
   Main Zone_Main Zone Direct Air,                      !Direct Air Name
   System Availability Schedule,                      !Schedule name for on/off schedule
   Main Zone_Main Zone Inlet Node,                      !Zone Supply Air Node Name
   1.5;                      !Maximum air flow rate
Fan:ConstantVolume,
   Supply Fan,                         !Fan Name
   Fan Availability Schedule,                         !Available Schedule
   0.7,                         !Fan Total Efficiency
   600,                         !Delta Pressure
   2,                         !Max Flow Rate
   0.9,                         !Motor Efficiency
   1,                         !Motor In Airstream Fraction
   Fan Inlet Node,                         !Fan_Inlet_Node
   Evap Cooler Inlet Node,                         !Fan_Outlet_Node
   General;                         !End-Use Subcategory
EvaporativeCooler:Direct:CelDekPad,
   Evaporative Cooler,                         !EvapCooler Name
   System Availability Schedule,                         !Available Schedule
   0.6,                         !Direct Pad Area
   0.2,                         !Direct Pad Depth
   225,                         !Recirc Water Pump Power Consumption
   Evap Cooler Inlet Node,                         !Evap_Air_Inlet_Node
   Supply Outlet Node,                         !Evap_Air_Outlet_Node
   CONSTANT,                         !Control Type
   ;                         !Name of Water Supply Storage Tank
OutdoorAir:Mixer,
   Outside Air Mixing Box,                         !Name
   Fan Inlet Node,                         !Mixed_Air_Node
   Outside Air Inlet Node,                         !Outside_Air_Stream_Node
   Relief Air Outlet Node,                         !Relief_Air_Stream_Node
   Supply Inlet Node;                         !Return_Air_Stream_Node
AirLoopHVAC:OutdoorAirSystem,
   Outside Air System,                         !Name
   Outside Air System Controllers,                         !Name: Controller List
   Outside Air System Equipment,                         !Name of an Air Loop Equipment List
   Evap Cooler Availability List;                         !Name of a System Availability Manager List
ZoneHVAC:EquipmentConnections,
   Main Zone,                      !Zone Name
   Main Zone_Main Zone Equipment,                      !List Name: Zone Equipment
   Main Zone_Main Zone_Inlet Nodelist,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   Main Zone_Main Zone Node,                      !Zone Air Node Name
   Main Zone_Main Zone Outlet Node;                      !Zone Return Air Node Name
AirLoopHVAC:ZoneSplitter,
   Zone Supply Air Splitter,                         !Splitter Name
   Zone Equipment Inlet Node,                         !Inlet_Node
   Main Zone_Main Zone Inlet Node;                         !Outlet_Node_1
AirLoopHVAC:ZoneMixer,
   Zone Return Air Mixer,                         !Mixer Name
   Zone Equipment Outlet Node,                         !Outlet_Node
   Main Zone_Main Zone Outlet Node;                         !Inlet_Node_1

