ScheduleTypeLimits,
   AnyNumber,                         !ScheduleType Name
   ,                         !Lower Limit Value
   ,                         !Upper Limit Value
   ,                         !Numeric Type
   ;                         !Unit Type
ScheduleTypeLimits,
   Contorl Type,                         !ScheduleType Name
   0,                         !Lower Limit Value
   4,                         !Upper Limit Value
   DISCRETE,                         !Numeric Type
   ;                         !Unit Type
ScheduleTypeLimits,
   Temperature,                         !ScheduleType Name
   -60,                         !Lower Limit Value
   200,                         !Upper Limit Value
   CONTINUOUS,                         !Numeric Type
   Temperature;                         !Unit Type
Schedule:Compact,
   OCC-SCHED,                         !Name
   AnyNumber,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Weekdays SummerDesignDay CustomDay1 CustomDay2,                         !Complex Field #2
   Until:7:00,0,                         !Complex Field #3
   Until:8:00,0.33333333,                         !Complex Field #4
   Until:9:00,0.6666667,                         !Complex Field #5
   Until:17:00,1,                         !Complex Field #6
   Until:18:00,0.5,                         !Complex Field #7
   Until:24:00,0,                         !Complex Field #8
   For: Weekends Holidays WinterDesignDay,                         !Complex Field #9
   Until:7:00,0,                         !Complex Field #10
   Until:8:00,0.6666667,                         !Complex Field #11
   Until:9:00,0.13333333,                         !Complex Field #12
   Until:12:00,0.2,                         !Complex Field #13
   Until:13:00,0.1,                         !Complex Field #14
   Until:24:00,0;                         !Complex Field #15
Schedule:Compact,
   LIT-SCHED,                         !Name
   AnyNumber,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Weekdays SummerDesignDay CustomDay1 CustomDay2,                         !Complex Field #2
   Until:7:00,0.3,                         !Complex Field #3
   Until:17:00,0.9,                         !Complex Field #4
   Until:24:00,0.3,                         !Complex Field #5
   For: Weekends Holidays WinterDesignDay,                         !Complex Field #6
   Until:7:00,0.3,                         !Complex Field #7
   Until:12:00,0.4,                         !Complex Field #8
   Until:24:00,0.3;                         !Complex Field #9
Schedule:Compact,
   INF-SCHED,                         !Name
   AnyNumber,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Weekdays CustomDay1 CustomDay2 SummerDesignDay,                         !Complex Field #2
   Until:6:00,1,                         !Complex Field #3
   Until:18:00,0,                         !Complex Field #4
   Until:24:00,1,                         !Complex Field #5
   For: Weekends Holidays WinterDesignDay,                         !Complex Field #6
   Until:6:00,1,                         !Complex Field #7
   Until:13:00,0,                         !Complex Field #8
   Until:24:00,1;                         !Complex Field #9
Schedule:Compact,
   PER-1T-ACTSCHD,                         !Name
   AnyNumber,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Alldays,                         !Complex Field #2
   Until:24:00,149.48;                         !Complex Field #3
Schedule:Compact,
   EQP-SCHED,                         !Name
   AnyNumber,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Weekdays SummerDesignDay CustomDay1 CustomDay2,                         !Complex Field #2
   Until:7:00,0.17,                         !Complex Field #3
   Until:17:00,1,                         !Complex Field #4
   Until:24:00,0.17,                         !Complex Field #5
   For: Weekends Holidays WinterDesignDay,                         !Complex Field #6
   Until:24:00,0.17;                         !Complex Field #7
Schedule:Compact,
   ALWAYSON,                         !Name
   AnyNumber,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Alldays,                         !Complex Field #2
   Until:24:00,1;                         !Complex Field #3
Schedule:Compact,
   DUAL CONTROL,                         !Name
   Contorl Type,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Alldays,                         !Complex Field #2
   Until:24:00,4;                         !Complex Field #3
Schedule:Compact,
   HEAT1,                         !Name
   AnyNumber,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Weekdays CustomDay1 CustomDay2,                         !Complex Field #2
   Until:6:00,12.8,                         !Complex Field #3
   Until:18:00,21.1,                         !Complex Field #4
   Until:24:00,12.8,                         !Complex Field #5
   For: Weekends Holidays,                         !Complex Field #6
   Until:6:00,12.8,                         !Complex Field #7
   Until:13:00,21.1,                         !Complex Field #8
   Until:24:00,12.8,                         !Complex Field #9
   For: SummerDesignDay,                         !Complex Field #10
   Until:24:00,12.8,                         !Complex Field #11
   For: WinterDesignDay,                         !Complex Field #12
   Until:24:00,21.1;                         !Complex Field #13
Schedule:Compact,
   COOL1,                         !Name
   AnyNumber,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Weekdays CustomDay1 CustomDay2,                         !Complex Field #2
   Until:6:00,32.2,                         !Complex Field #3
   Until:18:00,23.9,                         !Complex Field #4
   Until:24:00,32.2,                         !Complex Field #5
   For: Weekends Holidays,                         !Complex Field #6
   Until:6:00,32.2,                         !Complex Field #7
   Until:13:00,23.9,                         !Complex Field #8
   Until:24:00,32.2,                         !Complex Field #9
   For: SummerDesignDay,                         !Complex Field #10
   Until:24:00,23.9,                         !Complex Field #11
   For: WinterDesignDay,                         !Complex Field #12
   Until:24:00,32.2;                         !Complex Field #13
Schedule:Compact,
   AIRSYSAVAILSCHED,                         !Name
   AnyNumber,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Weekdays SummerDesignDay WinterDesignDay CustomDay1 CustomDay2,                         !Complex Field #2
   Until:6:00,0,                         !Complex Field #3
   Until:18:00,1,                         !Complex Field #4
   Until:24:00,0,                         !Complex Field #5
   For: Weekends Holidays,                         !Complex Field #6
   Until:6:00,0,                         !Complex Field #7
   Until:13:00,1,                         !Complex Field #8
   Until:24:00,0;                         !Complex Field #9
Schedule:Compact,
   HEATINGAVAILSCHED,                         !Name
   AnyNumber,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Weekdays SummerDesignDay WinterDesignDay CustomDay1 CustomDay2,                         !Complex Field #2
   Until:6:00,0,                         !Complex Field #3
   Until:18:00,1,                         !Complex Field #4
   Until:24:00,0,                         !Complex Field #5
   For: Weekends Holidays,                         !Complex Field #6
   Until:6:00,0,                         !Complex Field #7
   Until:13:00,1,                         !Complex Field #8
   Until:24:00,0;                         !Complex Field #9
Schedule:Compact,
   COOLINGAVAILSCHED,                         !Name
   AnyNumber,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Weekdays SummerDesignDay WinterDesignDay CustomDay1 CustomDay2,                         !Complex Field #2
   Until:6:00,0,                         !Complex Field #3
   Until:18:00,1,                         !Complex Field #4
   Until:24:00,0,                         !Complex Field #5
   For: Weekends Holidays,                         !Complex Field #6
   Until:6:00,0,                         !Complex Field #7
   Until:13:00,1,                         !Complex Field #8
   Until:24:00,0;                         !Complex Field #9
Schedule:Compact,
   CW TEMP SCHEDULE,                         !Name
   AnyNumber,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Alldays,                         !Complex Field #2
   Until:24:00,6.67;                         !Complex Field #3
Schedule:Compact,
   HW LOOP TEMP SCHEDULE,                         !Name
   AnyNumber,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Alldays,                         !Complex Field #2
   Until:24:00,60;                         !Complex Field #3
Schedule:Compact,
   CONDENSER TEMP SCHEDULE,                         !Name
   AnyNumber,                         !ScheduleType
   Through:12/31,                         !Complex Field #1
   For: Alldays,                         !Complex Field #2
   Until:24:00,29.5;                         !Complex Field #3
Schedule:Compact,
   SEASONAL RESET SUPPLY AIR TEMP SCH,                         !Name
   Temperature,                         !ScheduleType
   Through:3/31,                         !Complex Field #1
   For: Alldays,                         !Complex Field #2
   Until:24:00,16,                         !Complex Field #3
   Through:9/30,                         !Complex Field #4
   For: Weekdays,                         !Complex Field #5
   Until:24:00,13,                         !Complex Field #6
   Through:12/31,                         !Complex Field #7
   For: Alldays,                         !Complex Field #8
   Until:24:00,16;                         !Complex Field #9
NodeList,
   PER-1T_P Zone Inlet,                      !Node List Name
   PER-1T_P Zone Inlet Node;                      !Node_ID_1
NodeList,
   PER-2T_P Zone Inlet,                      !Node List Name
   PER-2T_P Zone Inlet Node;                      !Node_ID_1
NodeList,
   PER-3T_P Zone Inlet,                      !Node List Name
   PER-3T_P Zone Inlet Node;                      !Node_ID_1
NodeList,
   PER-4T_P Zone Inlet,                      !Node List Name
   PER-4T_P Zone Inlet Node;                      !Node_ID_1
NodeList,
   PER-1F_P Zone Inlet,                      !Node List Name
   PER-1F_P Zone Inlet Node;                      !Node_ID_1
NodeList,
   PER-2F_P Zone Inlet,                      !Node List Name
   PER-2F_P Zone Inlet Node;                      !Node_ID_1
NodeList,
   PER-3F_P Zone Inlet,                      !Node List Name
   PER-3F_P Zone Inlet Node;                      !Node_ID_1
NodeList,
   PER-4F_P Zone Inlet,                      !Node List Name
   PER-4F_P Zone Inlet Node;                      !Node_ID_1
NodeList,
   PER-1I_P Zone Inlet,                      !Node List Name
   PER-1I_P Zone Inlet Node;                      !Node_ID_1
NodeList,
   PER-2I_P Zone Inlet,                      !Node List Name
   PER-2I_P Zone Inlet Node;                      !Node_ID_1
NodeList,
   PER-3I_P Zone Inlet,                      !Node List Name
   PER-3I_P Zone Inlet Node;                      !Node_ID_1
NodeList,
   PER-4I_P Zone Inlet,                      !Node List Name
   PER-4I_P Zone Inlet Node;                      !Node_ID_1
NodeList,
   COR-T_C Zone Inlet,                      !Node List Name
   COR-T_C Zone Inlet Node;                      !Node_ID_1
NodeList,
   COR-F_C Zone Inlet,                      !Node List Name
   COR-F_C Zone Inlet Node;                      !Node_ID_1
NodeList,
   COR-I_C Zone Inlet,                      !Node List Name
   COR-I_C Zone Inlet Node;                      !Node_ID_1
NodeList,
   Mixed OA Node 1,                         !Node List Name
   Mixed Air Node 1;                         !Node_ID_1
NodeList,
   OA Inlet Node 1,                         !Node List Name
   OAMixer1_OutsideAirStreamNode;                         !Node_ID_1
NodeList,
   Supply Air Temp Node,                         !Node List Name
   Simple Cooling Coil_AirOutletNode;                         !Node_ID_1
NodeList,
   Chilled Water Loop Setpoint Node List,                         !Node List Name
   CW Supply Outlet Node;                         !Node_ID_1
NodeList,
   Hot Water Loop Setpoint Node List,                         !Node List Name
   HW Supply Outlet Node;                         !Node_ID_1
NodeList,
   Chilled Water Condenser Loop Setpoint Node List,                         !Node List Name
   Condenser Supply Outlet Node;                         !Node_ID_1
BranchList,
   VAV Sys 1 Branches,                         !Branch List Name
   VAV Sys 1 Main Branch;                         !Branch Name 1
BranchList,
   Cooling Supply Side Branches,                         !Branch List Name
   CW Pump Branch,                         !Branch Name 1
   Chiller Branch,                         !Branch Name 2
   CW Supply Bypass Branch,                         !Branch Name 3
   Cooling Supply Outlet;                         !Branch Name 4
BranchList,
   Cooling Demand Side Branches,                         !Branch List Name
   Cooling Demand Inlet,                         !Branch Name 1
   Cooling Coil Branch,                         !Branch Name 2
   Demand Bypass Branch,                         !Branch Name 3
   Cooling Demand Outlet;                         !Branch Name 4
BranchList,
   Condenser Supply Side Branches,                         !Branch List Name
   Condenser Supply Inlet Branch,                         !Branch Name 1
   Condenser Supply Tower Branch,                         !Branch Name 2
   Condenser Supply Bypass Branch,                         !Branch Name 3
   Condenser Supply Outlet Branch;                         !Branch Name 4
BranchList,
   Condenser Demand Side Branche,                         !Branch List Name
   Condenser Demand Inlet Branch,                         !Branch Name 1
   Chiller Condenser Branch,                         !Branch Name 2
   Condenser Demand Bypass Branch,                         !Branch Name 3
   Condenser Demand Outlet Branch;                         !Branch Name 4
BranchList,
   Heating Supply Side Branches,                         !Branch List Name
   Heating Supply Inlet Branch,                         !Branch Name 1
   Boiler Branch,                         !Branch Name 2
   Heating Supply Bypass Branch,                         !Branch Name 3
   Heating Supply Outlet Branch;                         !Branch Name 4
BranchList,
   Heating Demand Side Branches,                         !Branch List Name
   Reheat Inlet Branch,                         !Branch Name 1
   PER-1T_P Zone Branch,                         !Branch Name 2
   PER-2T_P Zone Branch,                         !Branch Name 2
   PER-3T_P Zone Branch,                         !Branch Name 2
   PER-4T_P Zone Branch,                         !Branch Name 2
   PER-1F_P Zone Branch,                         !Branch Name 2
   PER-2F_P Zone Branch,                         !Branch Name 2
   PER-3F_P Zone Branch,                         !Branch Name 2
   PER-4F_P Zone Branch,                         !Branch Name 2
   PER-1I_P Zone Branch,                         !Branch Name 2
   PER-2I_P Zone Branch,                         !Branch Name 2
   PER-3I_P Zone Branch,                         !Branch Name 2
   PER-4I_P Zone Branch,                         !Branch Name 2
   COR-T_C  Zone Branch,                         !Branch Name 3
   COR-F_C  Zone Branch,                         !Branch Name 3
   COR-I_C  Zone Branch,                         !Branch Name 3
   Reheat Bypass Branch,                         !Branch Name 4
   Reheat Outlet Branch;                         !Branch Name 5
AirLoopHVAC,
   VAV Sys 1,                         !Primary Air Loop Name
   VAV Sys 1 Controllers,                         !Name: Controller List
   VAV Sys 1 Avail List,                         !Name: System Availability Manager List
   autosize,                         !Primary air design volumetric flow rate
   VAV Sys 1 Branches,                         !Air Loop Branch List Name
   ,                         !Air Loop Connector List Name
   OAMixer1_ReturnAirStreamNode,                         !ReturnAir AirLoop Inlet Node
   ZoneMixer1_OutletNode,                         !ZoneEquipGroup Outlet Node
   ZoneSplitter1_InletNode,                         !SupplyAirPath ZoneEquipGroup Inlet Nodes
   Simple Cooling Coil_AirOutletNode;                         !AirLoop Outlet Nodes
CondenserLoop,
   Chilled Water Condenser Loop,                         !Condenser Loop Name
   Water,                         !Fluid Type
   Tower Loop Operation,                         !Condenser Operation Scheme List Name
   Condenser Supply Outlet Node,                         !Condenser Loop Temperature Setpoint Node or reference
   80,                         !Maximum Loop Temperature
   5,                         !Minimum Loop Temperature
   autosize,                         !Maximum Loop Volumetric Flow Rate
   0,                         !Minimum Loop Volumetric Flow Rate
   autocalculate,                         !volume of the condenser loop
   Condenser Supply Inlet Node,                         !Condenser Side Inlet Node Name
   Condenser Supply Outlet Node,                         !Condenser Side Outlet Node Name
   Condenser Supply Side Branches,                         !Condenser Side Branch List Name
   Condenser Supply Side Connectors,                         !Condenser Side Connector List Name
   Condenser Demand Inlet Node,                         !Demand Side Inlet Node Name
   Condenser Demand Outlet Node,                         !Demand Side Outlet Nodes Name
   Condenser Demand Side Branche,                         !Condenser Demand Side Branch List Name
   Condenser Demand Side Connectors,                         !Condenser Demand Side Connector List Name
   Sequential,                         !Load Distribution Scheme
   ;                         !Pressure Simulation Type
PlantLoop,
   Chilled Water Loop,                         !Plant Loop Name
   Water,                         !Fluid Type
   CW Loop Operation,                         !Plant Operation Scheme List Name
   CW Supply Outlet Node,                         !Loop Temperature Setpoint Node Name
   98,                         !Maximum Loop Temperature
   5,                         !Minimum Loop Temperature
   autosize,                         !Maximum Loop Volumetric Flow Rate
   0,                         !Minimum Loop Volumetric Flow Rate
   autocalculate,                         !volume of the plant loop
   CW Supply Inlet Node,                         !Plant Side Inlet Node Name
   CW Supply Outlet Node,                         !Plant Side Outlet Node Name
   Cooling Supply Side Branches,                         !Plant Side Branch List Name
   Cooling Supply Side Connectors,                         !Plant Side Connector List Name
   CW Demand Inlet Node,                         !Demand Side Inlet Node Name
   CW Demand Outlet Node,                         !Demand Side Outlet Nodes Name
   Cooling Demand Side Branches,                         !Demand Side Branch List Name
   Cooling Demand Side Connectors,                         !Demand Side Connector List Name
   SEQUENTIAL,                         !Load Distribution Scheme
   ,                         !System Availability Manager List
   ,                         !Plant Loop Demand Calculation Scheme
   ,                         !Common Pipe Simulation
   ;                         !Pressure Simulation Type
PlantLoop,
   Hot Water Loop,                         !Plant Loop Name
   Water,                         !Fluid Type
   Hot Loop Operation,                         !Plant Operation Scheme List Name
   HW Supply Outlet Node,                         !Loop Temperature Setpoint Node Name
   100,                         !Maximum Loop Temperature
   5,                         !Minimum Loop Temperature
   autosize,                         !Maximum Loop Volumetric Flow Rate
   0,                         !Minimum Loop Volumetric Flow Rate
   autocalculate,                         !volume of the plant loop
   HW Supply Inlet Node,                         !Plant Side Inlet Node Name
   HW Supply Outlet Node,                         !Plant Side Outlet Node Name
   Heating Supply Side Branches,                         !Plant Side Branch List Name
   Heating Supply Side Connectors,                         !Plant Side Connector List Name
   HW Demand Inlet Node,                         !Demand Side Inlet Node Name
   HW Demand Outlet Node,                         !Demand Side Outlet Nodes Name
   Heating Demand Side Branches,                         !Demand Side Branch List Name
   Heating Demand Side Connectors,                         !Demand Side Connector List Name
   ,                         !Load Distribution Scheme
   ,                         !System Availability Manager List
   ,                         !Plant Loop Demand Calculation Scheme
   ,                         !Common Pipe Simulation
   ;                         !Pressure Simulation Type
AirLoopHVAC:ReturnPath,
   Zone Return Air Path 1,                         !Name
   ZoneMixer1_OutletNode,                         !Return Air Path Outlet Node Name
   AirLoopHVAC:ZoneMixer,                         !Component 1 Object Type
   ZoneMixer1;                         !Component 1 Name
AirLoopHVAC:SupplyPath,
   Zone Supply Air Path 1,                         !Name
   ZoneSplitter1_InletNode,                         !Supply Air Path Inlet Node Name
   AirLoopHVAC:ZoneSplitter,                         !Component 1 Object Type
   ZoneSplitter1;                         !Component 1 Name
Branch,
   VAV Sys 1 Main Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   AirLoopHVAC:OutdoorAirSystem,                         !Comp1 Type
   OA System 1,                         !Comp1 Name
   OAMixer1_ReturnAirStreamNode,                         !Comp1 Inlet Node Name
   Mixed Air Node 1,                         !Comp1 Outlet Node Name
   PASSIVE,                         !Comp1 Branch Control Type
   Fan:VariableVolume,                         !Comp2 Type
   Supply Fan 1,                         !Comp2 Name
   Mixed Air Node 1,                         !Comp2 Inlet Node Name
   Supply Fan 1_FanOutletNode,                         !Comp2 Outlet Node Name
   ACTIVE,                         !Comp2 Branch Control Type
   COIL:Cooling:Water,                         !Comp3 Type
   Simple Cooling Coil,                         !Comp3 Name
   Supply Fan 1_FanOutletNode,                         !Comp3 Inlet Node Name
   Simple Cooling Coil_AirOutletNode,                         !Comp3 Outlet Node Name
   PASSIVE;                         !Comp3 Branch Control Type
Branch,
   CW Pump Branch,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pump:VariableSpeed,                         !Comp1 Type
   CW Circ Pump,                         !Comp1 Name
   CW Supply Inlet Node,                         !Comp1 Inlet Node Name
   CW Pump Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Chiller Branch,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   CHILLER:ELECTRIC,                         !Comp1 Type
   Chiller 1,                         !Comp1 Name
   Central Chiller Inlet Node,                         !Comp1 Inlet Node Name
   Central Chiller Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   CW Supply Bypass Branch,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Supply Side Bypass,                         !Comp1 Name
   CW Supply Bypass Inlet Node,                         !Comp1 Inlet Node Name
   CW Supply Bypass Outlet Node,                         !Comp1 Outlet Node Name
   BYPASS;                         !Comp1 Branch Control Type
Branch,
   Cooling Supply Outlet,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Supply Side Outlet Pipe,                         !Comp1 Name
   Supply Side Exit Pipe Inlet Node,                         !Comp1 Inlet Node Name
   CW Supply Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Cooling Demand Inlet,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Demand Side Inlet Pipe,                         !Comp1 Name
   CW Demand Inlet Node,                         !Comp1 Inlet Node Name
   CW Demand Entrance Pipe Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Cooling Coil Branch,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   COIL:Cooling:Water,                         !Comp1 Type
   Simple Cooling Coil,                         !Comp1 Name
   Simple Cooling Coil_WaterInletNode,                         !Comp1 Inlet Node Name
   Simple Cooling Coil_WaterOutletNode,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Demand Bypass Branch,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Demand Side Bypass,                         !Comp1 Name
   CW Demand Bypass Inlet Node,                         !Comp1 Inlet Node Name
   CW Demand Bypass Outlet Node,                         !Comp1 Outlet Node Name
   BYPASS;                         !Comp1 Branch Control Type
Branch,
   Cooling Demand Outlet,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Demand Side Outlet Pipe,                         !Comp1 Name
   CW Demand Exit Pipe Inlet Node,                         !Comp1 Inlet Node Name
   CW Demand Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Condenser Supply Inlet Branch,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pump:VariableSpeed,                         !Comp1 Type
   Cond Circ Pump,                         !Comp1 Name
   Condenser Supply Inlet Node,                         !Comp1 Inlet Node Name
   Condenser Pump Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Condenser Supply Tower Branch,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   COOLINGTOWER:SINGLESPEED,                         !Comp1 Type
   Big Tower,                         !Comp1 Name
   Condenser Tower Inlet Node,                         !Comp1 Inlet Node Name
   Condenser Tower Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Condenser Supply Bypass Branch,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Condenser Supply Side Bypass,                         !Comp1 Name
   Cond Supply Bypass Inlet Node,                         !Comp1 Inlet Node Name
   Cond Supply Bypass Outlet Node,                         !Comp1 Outlet Node Name
   BYPASS;                         !Comp1 Branch Control Type
Branch,
   Condenser Supply Outlet Branch,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Condenser Supply Outlet,                         !Comp1 Name
   Condenser Supply Exit Pipe Inlet Node,                         !Comp1 Inlet Node Name
   Condenser Supply Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Condenser Demand Inlet Branch,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Condenser Demand Inlet Pipe,                         !Comp1 Name
   Condenser Demand Inlet Node,                         !Comp1 Inlet Node Name
   Condenser Demand Inpipe Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Chiller Condenser Branch,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   CHILLER:ELECTRIC,                         !Comp1 Type
   Chiller 1,                         !Comp1 Name
   Central Chiller Condenser Inlet Node,                         !Comp1 Inlet Node Name
   Central Chiller Condenser Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Condenser Demand Bypass Branch,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Condenser Demand Side Bypass,                         !Comp1 Name
   Cond Demand Bypass Inlet Node,                         !Comp1 Inlet Node Name
   Cond Demand Bypass Outlet Node,                         !Comp1 Outlet Node Name
   BYPASS;                         !Comp1 Branch Control Type
Branch,
   Condenser Demand Outlet Branch,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Condenser Demand Outlet Pipe,                         !Comp1 Name
   Condenser Demand Exit Pipe Inlet Node,                         !Comp1 Inlet Node Name
   Condenser Demand Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Heating Supply Inlet Branch,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pump:VariableSpeed,                         !Comp1 Type
   HW Circ Pump,                         !Comp1 Name
   HW Supply Inlet Node,                         !Comp1 Inlet Node Name
   HW Pump Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Boiler Branch,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Boiler:HotWater,                         !Comp1 Type
   Central Boiler,                         !Comp1 Name
   Central Boiler Inlet Node,                         !Comp1 Inlet Node Name
   Central Boiler Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Heating Supply Bypass Branch,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Heating Supply Side Bypass,                         !Comp1 Name
   Heating Supply Bypass Inlet Node,                         !Comp1 Inlet Node Name
   Heating Supply Bypass Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Heating Supply Outlet Branch,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Heating Supply Outlet,                         !Comp1 Name
   Heating Supply Exit Pipe Inlet Node,                         !Comp1 Inlet Node Name
   HW Supply Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Reheat Outlet Branch,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Reheat Outlet Pipe,                         !Comp1 Name
   HW Demand Exit Pipe Inlet Node,                         !Comp1 Inlet Node Name
   HW Demand Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Reheat Inlet Branch,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Reheat Inlet Pipe,                         !Comp1 Name
   HW Demand Inlet Node,                         !Comp1 Inlet Node Name
   HW Demand Entrance Pipe Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Reheat Bypass Branch,                         !Branch Name
   0,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Reheat Bypass,                         !Comp1 Name
   Reheat Bypass Inlet Node,                         !Comp1 Inlet Node Name
   Reheat Bypass Outlet Node,                         !Comp1 Outlet Node Name
   BYPASS;                         !Comp1 Branch Control Type
Branch,
   PER-1T_P Zone Branch,                      !Branch Name
   0,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   Coil:Heating:Water,                      !Comp1 Type
   PER-1T_P  VAV system_Coil,                      !Comp1 Name
   PER-1T_P  VAV system_CoilWaterInletNode,                      !Comp1 Inlet Node Name
   PER-1T_P  VAV system_CoilWaterOutletNode,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   PER-2T_P Zone Branch,                      !Branch Name
   0,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   Coil:Heating:Water,                      !Comp1 Type
   PER-2T_P  VAV system_Coil,                      !Comp1 Name
   PER-2T_P  VAV system_CoilWaterInletNode,                      !Comp1 Inlet Node Name
   PER-2T_P  VAV system_CoilWaterOutletNode,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   PER-3T_P Zone Branch,                      !Branch Name
   0,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   Coil:Heating:Water,                      !Comp1 Type
   PER-3T_P  VAV system_Coil,                      !Comp1 Name
   PER-3T_P  VAV system_CoilWaterInletNode,                      !Comp1 Inlet Node Name
   PER-3T_P  VAV system_CoilWaterOutletNode,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   PER-4T_P Zone Branch,                      !Branch Name
   0,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   Coil:Heating:Water,                      !Comp1 Type
   PER-4T_P  VAV system_Coil,                      !Comp1 Name
   PER-4T_P  VAV system_CoilWaterInletNode,                      !Comp1 Inlet Node Name
   PER-4T_P  VAV system_CoilWaterOutletNode,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   PER-1F_P Zone Branch,                      !Branch Name
   0,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   Coil:Heating:Water,                      !Comp1 Type
   PER-1F_P  VAV system_Coil,                      !Comp1 Name
   PER-1F_P  VAV system_CoilWaterInletNode,                      !Comp1 Inlet Node Name
   PER-1F_P  VAV system_CoilWaterOutletNode,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   PER-2F_P Zone Branch,                      !Branch Name
   0,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   Coil:Heating:Water,                      !Comp1 Type
   PER-2F_P  VAV system_Coil,                      !Comp1 Name
   PER-2F_P  VAV system_CoilWaterInletNode,                      !Comp1 Inlet Node Name
   PER-2F_P  VAV system_CoilWaterOutletNode,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   PER-3F_P Zone Branch,                      !Branch Name
   0,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   Coil:Heating:Water,                      !Comp1 Type
   PER-3F_P  VAV system_Coil,                      !Comp1 Name
   PER-3F_P  VAV system_CoilWaterInletNode,                      !Comp1 Inlet Node Name
   PER-3F_P  VAV system_CoilWaterOutletNode,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   PER-4F_P Zone Branch,                      !Branch Name
   0,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   Coil:Heating:Water,                      !Comp1 Type
   PER-4F_P  VAV system_Coil,                      !Comp1 Name
   PER-4F_P  VAV system_CoilWaterInletNode,                      !Comp1 Inlet Node Name
   PER-4F_P  VAV system_CoilWaterOutletNode,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   PER-1I_P Zone Branch,                      !Branch Name
   0,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   Coil:Heating:Water,                      !Comp1 Type
   PER-1I_P  VAV system_Coil,                      !Comp1 Name
   PER-1I_P  VAV system_CoilWaterInletNode,                      !Comp1 Inlet Node Name
   PER-1I_P  VAV system_CoilWaterOutletNode,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   PER-2I_P Zone Branch,                      !Branch Name
   0,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   Coil:Heating:Water,                      !Comp1 Type
   PER-2I_P  VAV system_Coil,                      !Comp1 Name
   PER-2I_P  VAV system_CoilWaterInletNode,                      !Comp1 Inlet Node Name
   PER-2I_P  VAV system_CoilWaterOutletNode,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   PER-3I_P Zone Branch,                      !Branch Name
   0,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   Coil:Heating:Water,                      !Comp1 Type
   PER-3I_P  VAV system_Coil,                      !Comp1 Name
   PER-3I_P  VAV system_CoilWaterInletNode,                      !Comp1 Inlet Node Name
   PER-3I_P  VAV system_CoilWaterOutletNode,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   PER-4I_P Zone Branch,                      !Branch Name
   0,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   Coil:Heating:Water,                      !Comp1 Type
   PER-4I_P  VAV system_Coil,                      !Comp1 Name
   PER-4I_P  VAV system_CoilWaterInletNode,                      !Comp1 Inlet Node Name
   PER-4I_P  VAV system_CoilWaterOutletNode,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   COR-T_C  Zone Branch,                      !Branch Name
   0,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   Coil:Heating:Water,                      !Comp1 Type
   COR-T_C  VAV system_Coil,                      !Comp1 Name
   COR-T_C  VAV system_CoilWaterInletNode,                      !Comp1 Inlet Node Name
   COR-T_C  VAV system_CoilWaterOutletNode,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   COR-F_C  Zone Branch,                      !Branch Name
   0,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   Coil:Heating:Water,                      !Comp1 Type
   COR-F_C  VAV system_Coil,                      !Comp1 Name
   COR-F_C  VAV system_CoilWaterInletNode,                      !Comp1 Inlet Node Name
   COR-F_C  VAV system_CoilWaterOutletNode,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   COR-I_C  Zone Branch,                      !Branch Name
   0,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   Coil:Heating:Water,                      !Comp1 Type
   COR-I_C  VAV system_Coil,                      !Comp1 Name
   COR-I_C  VAV system_CoilWaterInletNode,                      !Comp1 Inlet Node Name
   COR-I_C  VAV system_CoilWaterOutletNode,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
ConnectorList,
   Cooling Supply Side Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   CW Loop Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   CW Loop Mixer;                         !Name of Connector 2
ConnectorList,
   Cooling Demand Side Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   CW Demand Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   CW Demand Mixer;                         !Name of Connector 2
ConnectorList,
   Condenser Supply Side Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   Condenser Supply Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   Condenser Supply Mixer;                         !Name of Connector 2
ConnectorList,
   Condenser Demand Side Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   Condenser Demand Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   Condenser Demand Mixer;                         !Name of Connector 2
ConnectorList,
   Heating Supply Side Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   Heating Supply Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   Heating Supply Mixer;                         !Name of Connector 2
ConnectorList,
   Heating Demand Side Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   Reheat Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   Reheat Mixer;                         !Name of Connector 2
PlantEquipmentOperationSchemes,
   CW Loop Operation,                         !PlantOperationSchemeName
   PlantEquipmentOperation:CoolingLoad,                         !KEY--Control Scheme 1
   Chiller operation,                         !Control Scheme Name 1
   ALWAYSON;                         !Control Scheme Schedule 1
PlantEquipmentOperationSchemes,
   Hot Loop Operation,                         !PlantOperationSchemeName
   PlantEquipmentOperation:HeatingLoad,                         !KEY--Control Scheme 1
   Boiler operation,                         !Control Scheme Name 1
   ALWAYSON;                         !Control Scheme Schedule 1
CondenserEquipmentOperationSchemes,
   Tower Loop Operation,                         !CondenserOperationSchemeName
   PlantEquipmentOperation:CoolingLoad,                         !KEY--Control Scheme 1
   Year Round Tower Operation,                         !Control Scheme Name 1
   ALWAYSON;                         !Control Scheme Schedule 1
PlantEquipmentOperation:CoolingLoad,
   Chiller operation,                         !Name
   0,                         !Load Range Lower Limit 1
   4000000,                         !Load Range Upper Limit 1
   All Chillers;                         !Priority Control Equip List Name 1
PlantEquipmentOperation:CoolingLoad,
   Year Round Tower Operation,                         !Name
   0,                         !Load Range Lower Limit 1
   90000000,                         !Load Range Upper Limit 1
   All Towers;                         !Priority Control Equip List Name 1
PlantEquipmentOperation:HeatingLoad,
   Boiler operation,                         !Name
   0,                         !Load Range Lower Limit 1
   10000000,                         !Load Range Upper Limit 1
   heating plant;                         !Priority Control Equip List Name 1
ZoneHVAC:EquipmentList,
   PER-1T_P Zone EquipList,                      !Name
   ZoneHVAC:AirDistributionUnit,                      !KEY--Zone Equipment Type 1
   PER-1T_P  VAV system_AHU,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   PER-2T_P Zone EquipList,                      !Name
   ZoneHVAC:AirDistributionUnit,                      !KEY--Zone Equipment Type 1
   PER-2T_P  VAV system_AHU,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   PER-3T_P Zone EquipList,                      !Name
   ZoneHVAC:AirDistributionUnit,                      !KEY--Zone Equipment Type 1
   PER-3T_P  VAV system_AHU,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   PER-4T_P Zone EquipList,                      !Name
   ZoneHVAC:AirDistributionUnit,                      !KEY--Zone Equipment Type 1
   PER-4T_P  VAV system_AHU,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   PER-1F_P Zone EquipList,                      !Name
   ZoneHVAC:AirDistributionUnit,                      !KEY--Zone Equipment Type 1
   PER-1F_P  VAV system_AHU,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   PER-2F_P Zone EquipList,                      !Name
   ZoneHVAC:AirDistributionUnit,                      !KEY--Zone Equipment Type 1
   PER-2F_P  VAV system_AHU,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   PER-3F_P Zone EquipList,                      !Name
   ZoneHVAC:AirDistributionUnit,                      !KEY--Zone Equipment Type 1
   PER-3F_P  VAV system_AHU,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   PER-4F_P Zone EquipList,                      !Name
   ZoneHVAC:AirDistributionUnit,                      !KEY--Zone Equipment Type 1
   PER-4F_P  VAV system_AHU,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   PER-1I_P Zone EquipList,                      !Name
   ZoneHVAC:AirDistributionUnit,                      !KEY--Zone Equipment Type 1
   PER-1I_P  VAV system_AHU,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   PER-2I_P Zone EquipList,                      !Name
   ZoneHVAC:AirDistributionUnit,                      !KEY--Zone Equipment Type 1
   PER-2I_P  VAV system_AHU,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   PER-3I_P Zone EquipList,                      !Name
   ZoneHVAC:AirDistributionUnit,                      !KEY--Zone Equipment Type 1
   PER-3I_P  VAV system_AHU,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   PER-4I_P Zone EquipList,                      !Name
   ZoneHVAC:AirDistributionUnit,                      !KEY--Zone Equipment Type 1
   PER-4I_P  VAV system_AHU,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   COR-T_C Zone EquipList,                      !Name
   ZoneHVAC:AirDistributionUnit,                      !KEY--Zone Equipment Type 1
   COR-T_C  VAV system_AHU,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   COR-F_C Zone EquipList,                      !Name
   ZoneHVAC:AirDistributionUnit,                      !KEY--Zone Equipment Type 1
   COR-F_C  VAV system_AHU,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   COR-I_C Zone EquipList,                      !Name
   ZoneHVAC:AirDistributionUnit,                      !KEY--Zone Equipment Type 1
   COR-I_C  VAV system_AHU,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
AirLoopHVAC:OutdoorAirSystem:EquipmentList,
   OA System 1 Equipment,                         !Name
   OutdoorAir:Mixer,                         !KEY--System Component 1
   OA Mixing Box 1;                         !Component Name 1
PlantEquipmentList,
   All Chillers,                         !Equip List Name
   CHILLER:ELECTRIC,                         !KEY--Plant Equip 1
   Chiller 1;                         !Equip Name 1
PlantEquipmentList,
   heating plant,                         !Equip List Name
   Boiler:HotWater,                         !KEY--Plant Equip 1
   Central Boiler;                         !Equip Name 1
CondenserEquipmentList,
   All Towers,                         !Equip List Name
   COOLINGTOWER:SINGLESPEED,                         !KEY--Condenser Equip 1
   Big Tower;                         !Equip Name 1
AirLoopHVAC:ControllerList,
   OA System 1 Controller,                         !Name
   Controller:OutdoorAir,                         !Controller Type 1
   Controller_OA1;                         !Controller Name 1
AirLoopHVAC:ControllerList,
   VAV Sys 1 Controllers,                         !Name
   CONTROLLER:WaterCoil,                         !Controller Type 1
   Main Cooling Coil Controller;                         !Controller Name 1
CONTROLLER:WaterCoil,
   Main Cooling Coil Controller,                         !Name
   Temperature,                         !Control variable
   REVERSE,                         !Action
   Flow,                         !Actuator variable
   Simple Cooling Coil_AirOutletNode,                         !Control_Node
   Simple Cooling Coil_WaterInletNode,                         !Actuator_Node
   ,                         !Controller Convergence Tolerance
   autosize,                         !Max Actuated Flow
   0;                         !Min Actuated Flow
Controller:OutdoorAir,
   Controller_OA1,                         !Name
   OAMixer1_ReliefAirStreamNode,                         !Relief Air Outlet Node Name
   OAMixer1_ReturnAirStreamNode,                         !Return Air Node Name
   Mixed Air Node 1,                         !Mixed Air Node Name
   OAMixer1_OutsideAirStreamNode,                         !Actuator Node Name
   autosize,                         !Minimum Outdoor Air Flow Rate
   autosize,                         !Maximum Outdoor Air Flow Rate
   NoEconomizer,                         !Economizer Control Type
   ModulateFlow,                         !Economizer Control Action Type
   19,                         !Economizer Maximum Limit Dry-Bulb Temperature
   ,                         !Economizer Maximum Limit Enthalpy
   ,                         !Economizer Maximum Limit Dewpoint Temperature
   ,                         !Electronic Enthalpy Limit Curve Name
   4,                         !Economizer Minimum Limit Dry-Bulb Temperature
   NoLockout,                         !Lockout Type
   ProportionalMinimum,                         !Minimum Limit Type
   ,                         !Minimum Outdoor Air Schedule Name
   ,                         !Minimum Fraction of Outdoor Air Schedule Name
   ,                         !Maximum Fraction of Outdoor Air Schedule Name
   ,                         !Mechanical Ventilation Controller Name
   ,                         !Time of Day Economizer Control Schedule Name
   ,                         !High Humidity Control
   ,                         !Humidistat Control Zone Name
   ,                         !High Humidity Outdoor Air Flow Ratio
   ,                         !Control High Indoor Humidity Based on Outdoor Humidity Ratio
   ;                         !Heat Recovery Bypass Control Type
AvailabilityManagerAssignmentList,
   VAV Sys 1 Avail List,                         !Name
   AvailabilityManager:Scheduled,                         !System Availability Manager Type 1
   VAV Sys 1 Avail;                         !System Availability Manager Name 1
AvailabilityManager:Scheduled,
   VAV Sys 1 Avail,                         !Name
   AIRSYSAVAILSCHED;                         !Schedule name
SetpointManager:Scheduled,
   Chilled Water Loop Setpoint Manager,                         !Name
   Temperature,                         !Control variable
   CW TEMP SCHEDULE,                         !Schedule Name
   Chilled Water Loop Setpoint Node List;                         !Name of the set point Node or Node List
SetpointManager:Scheduled,
   Hot Water Loop Setpoint Manager,                         !Name
   Temperature,                         !Control variable
   HW LOOP TEMP SCHEDULE,                         !Schedule Name
   Hot Water Loop Setpoint Node List;                         !Name of the set point Node or Node List
SetpointManager:Scheduled,
   Chilled Water Condenser Loop Setpoint Manager,                         !Name
   Temperature,                         !Control variable
   CONDENSER TEMP SCHEDULE,                         !Schedule Name
   Chilled Water Condenser Loop Setpoint Node List;                         !Name of the set point Node or Node List
SetpointManager:Scheduled,
   Supply Air temp Manager,                         !Name
   Temperature,                         !Control variable
   SEASONAL RESET SUPPLY AIR TEMP SCH,                         !Schedule Name
   Supply Air Temp Node;                         !Name of the set point Node or Node List
OutdoorAir:NodeList,
   OAMixer1_OutsideAirStreamNode;                         !1st Node name or node list name
ThermostatSetpoint:DualSetpoint,
   DualSetPoint,                         !Name
   HEAT1,                         !Heating Setpoint Temperature SCHEDULE Name
   COOL1;                         !Cooling Setpoint Temperature SCHEDULE Name
SIZING:PARAMETERS,
   1,                         !Cooling Sizing Factor
   1,                         !Heating sizing factor
   ;                         !time steps in averaging window
Sizing:Plant,
   Hot Water Loop,                         !name of a PLANT LOOP or CONDENSER LOOP object
   Heating,                         !loop type
   60,                         !Design loop exit temperature
   11;                         !Design loop delta T
Sizing:Plant,
   Chilled Water Loop,                         !name of a PLANT LOOP or CONDENSER LOOP object
   Cooling,                         !loop type
   6.67,                         !Design loop exit temperature
   6.67;                         !Design loop delta T
Sizing:Plant,
   Chilled Water Condenser Loop,                         !name of a PLANT LOOP or CONDENSER LOOP object
   Condenser,                         !loop type
   29.5,                         !Design loop exit temperature
   5.6;                         !Design loop delta T
Sizing:System,
   VAV Sys 1,                         !name of an AIR PRIMARY LOOP object
   sensible,                         !type of load to size on
   autosize,                         !Design (minimum) outside air volumetric flow rate
   0.3,                         !minimum system air flow ratio
   0.7,                         !Preheat design temperature
   0.008,                         !Preheat design humidity ratio
   11,                         !Precool design temperature
   0.008,                         !Precool design humidity ratio
   13,                         !Central cooling design supply air temperature
   16,                         !Central heating design supply air temperature
   noncoincident,                         !Sizing Option
   no,                         !Cooling 100% Outside Air
   no,                         !Heating 100% Outside Air
   0.008,                         !Central cooling design supply air humidity ratio
   0.008,                         !Central heating design supply air humidity ratio
   DesignDay,                         !Central heating design supply air humidity ratio
   0,                         !cooling design air flow rate
   DesignDay,                         !heating design air flow method
   0;                         !heating design air flow rate
Sizing:Zone,
   PER-1T,                         !Name of a zone
   14,                         !Zone cooling design supply air temperature
   50,                         !Zone heating design supply air temperature
   0.009,                         !Zone cooling design supply air humidity ratio
   0.004,                         !Zone heating design supply air humidity ratio
   flow/person,                         !outside air method
   0.00944,                         !outside air flow per person
   0,                         !outside air flow per zone area
   0,                         !outside air flow per zone
   0,                         !zone heating sizing factor
   0,                         !zone cooling sizing factor
   DesignDay,                         !cooling design air flow method
   0,                         !cooling design air flow rate
   ,                         !cooling min air flow per zone area
   ,                         !cooling min air flow
   ,                         !cooling min air flow fraction
   DesignDay,                         !heating design air flow method
   0,                         !heating design air flow rate
   ,                         !heating max air flow per zone area
   ,                         !heating max air flow
   ;                         !heating max air flow fraction
Sizing:Zone,
   PER-4F,                         !Name of a zone
   14,                         !Zone cooling design supply air temperature
   50,                         !Zone heating design supply air temperature
   0.009,                         !Zone cooling design supply air humidity ratio
   0.004,                         !Zone heating design supply air humidity ratio
   flow/person,                         !outside air method
   0.00944,                         !outside air flow per person
   0,                         !outside air flow per zone area
   0,                         !outside air flow per zone
   0.8,                         !zone heating sizing factor
   0.8,                         !zone cooling sizing factor
   DesignDay,                         !cooling design air flow method
   0,                         !cooling design air flow rate
   ,                         !cooling min air flow per zone area
   ,                         !cooling min air flow
   ,                         !cooling min air flow fraction
   DesignDay,                         !heating design air flow method
   0,                         !heating design air flow rate
   ,                         !heating max air flow per zone area
   ,                         !heating max air flow
   ;                         !heating max air flow fraction
Sizing:Zone,
   COR-I,                         !Name of a zone
   14,                         !Zone cooling design supply air temperature
   50,                         !Zone heating design supply air temperature
   0.009,                         !Zone cooling design supply air humidity ratio
   0.004,                         !Zone heating design supply air humidity ratio
   flow/person,                         !outside air method
   0.00944,                         !outside air flow per person
   0,                         !outside air flow per zone area
   0,                         !outside air flow per zone
   1.1,                         !zone heating sizing factor
   1.1,                         !zone cooling sizing factor
   DesignDay,                         !cooling design air flow method
   0,                         !cooling design air flow rate
   ,                         !cooling min air flow per zone area
   ,                         !cooling min air flow
   ,                         !cooling min air flow fraction
   DesignDay,                         !heating design air flow method
   0,                         !heating design air flow rate
   ,                         !heating max air flow per zone area
   ,                         !heating max air flow
   ;                         !heating max air flow fraction
ZoneControl:Thermostat,
   P1T Thermostat,                         !Thermostat Name
   PER-1T,                         !Zone Name
   DUAL CONTROL,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:DualSetpoint,                         !Control Type #1
   DualSetPoint;                         !Control Type Name #1
ZoneControl:Thermostat,
   P2T Thermostat,                         !Thermostat Name
   PER-2T,                         !Zone Name
   DUAL CONTROL,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:DualSetpoint,                         !Control Type #1
   DualSetPoint;                         !Control Type Name #1
ZoneControl:Thermostat,
   P3T Thermostat,                         !Thermostat Name
   PER-3T,                         !Zone Name
   DUAL CONTROL,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:DualSetpoint,                         !Control Type #1
   DualSetPoint;                         !Control Type Name #1
ZoneControl:Thermostat,
   P4T Thermostat,                         !Thermostat Name
   PER-4T,                         !Zone Name
   DUAL CONTROL,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:DualSetpoint,                         !Control Type #1
   DualSetPoint;                         !Control Type Name #1
ZoneControl:Thermostat,
   C1T Thermostat,                         !Thermostat Name
   COR-T,                         !Zone Name
   DUAL CONTROL,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:DualSetpoint,                         !Control Type #1
   DualSetPoint;                         !Control Type Name #1
ZoneControl:Thermostat,
   P1F Thermostat,                         !Thermostat Name
   PER-1F,                         !Zone Name
   DUAL CONTROL,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:DualSetpoint,                         !Control Type #1
   DualSetPoint;                         !Control Type Name #1
ZoneControl:Thermostat,
   P2F Thermostat,                         !Thermostat Name
   PER-2F,                         !Zone Name
   DUAL CONTROL,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:DualSetpoint,                         !Control Type #1
   DualSetPoint;                         !Control Type Name #1
ZoneControl:Thermostat,
   P3F Thermostat,                         !Thermostat Name
   PER-3F,                         !Zone Name
   DUAL CONTROL,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:DualSetpoint,                         !Control Type #1
   DualSetPoint;                         !Control Type Name #1
ZoneControl:Thermostat,
   P4F Thermostat,                         !Thermostat Name
   PER-4F,                         !Zone Name
   DUAL CONTROL,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:DualSetpoint,                         !Control Type #1
   DualSetPoint;                         !Control Type Name #1
ZoneControl:Thermostat,
   C1F Thermostat,                         !Thermostat Name
   COR-F,                         !Zone Name
   DUAL CONTROL,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:DualSetpoint,                         !Control Type #1
   DualSetPoint;                         !Control Type Name #1
ZoneControl:Thermostat,
   P1I Thermostat,                         !Thermostat Name
   PER-1I,                         !Zone Name
   DUAL CONTROL,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:DualSetpoint,                         !Control Type #1
   DualSetPoint;                         !Control Type Name #1
ZoneControl:Thermostat,
   P2I Thermostat,                         !Thermostat Name
   PER-2I,                         !Zone Name
   DUAL CONTROL,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:DualSetpoint,                         !Control Type #1
   DualSetPoint;                         !Control Type Name #1
ZoneControl:Thermostat,
   P3I Thermostat,                         !Thermostat Name
   PER-3I,                         !Zone Name
   DUAL CONTROL,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:DualSetpoint,                         !Control Type #1
   DualSetPoint;                         !Control Type Name #1
ZoneControl:Thermostat,
   P4I Thermostat,                         !Thermostat Name
   PER-4I,                         !Zone Name
   DUAL CONTROL,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:DualSetpoint,                         !Control Type #1
   DualSetPoint;                         !Control Type Name #1
CURVE:QUADRATIC,
   BoilerEfficiency,                         !Name
   1,                         !Coeff1 Constant
   0,                         !Coeff2 x
   0,                         !Coeff3 x**2
   0,                         !minimum value of x
   1,                         !maximum value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
AirTerminal:SingleDuct:VAV:Reheat,
   PER-1T_P  VAV system,                      !Name of System
   AIRSYSAVAILSCHED,                      !System Availability schedule
   PER-1T_P  VAV system_CoilAirInletNode,                      !DAMPER Air Outlet Node
   PER-1T_P  VAV system_UnitAirInletNode,                      !UNIT Air Inlet Node
   autosize,                      !Maximum air flow rate
   Constant,                      !Zone Minimum Air Flow Input Method
   0.3,                      !Constant Minimum Air Flow Fraction
   ,                      !Fixed Minimum Air Flow Rate
   ,                      !Minimum Air Flow Fraction Schedule Name
   COIL:Heating:Water,                      !Reheat Component Object
   PER-1T_P  VAV system_Coil,                      !Name of Reheat Component
   autosize,                      !Max Reheat Water Flow
   0,                      !Min Reheat Water Flow
   PER-1T_P Zone Inlet Node,                      !UNIT Air Outlet Node
   0.00025,                      !Convergence Tolerance
   NORMAL,                      !Damper Heating Action
   ,                      !Maximum Flow per Zone Floor Area During Reheat
   ,                      !Maximum Flow Fraction During Reheat
   ,                      !Maximum Reheat Air Temperature
   ;                      !Design Specification Outdoor Air Object Name
COIL:Heating:Water,
   PER-1T_P  VAV system_Coil,                      !Coil Name
   HEATINGAVAILSCHED,                      !Available Schedule
   autosize,                      !UA of the Coil
   autosize,                      !Max Water Flow Rate of Coil
   PER-1T_P  VAV system_CoilWaterInletNode,                      !Coil_Water_Inlet_Node
   PER-1T_P  VAV system_CoilWaterOutletNode,                      !Coil_Water_Outlet_Node
   PER-1T_P  VAV system_CoilAirInletNode,                      !Coil_Air_Inlet_Node
   PER-1T_P Zone Inlet Node,                      !Coil_Air_Outlet_Node
   UFactorTimesAreaAndDesignWaterFlowRate,                      !Coil Performance Input Method
   autosize,                      !Nominal Capacity
   82.2,                      !Design Inlet Water Temperature
   16.6,                      !Design Inlet Air Temperature
   71.1,                      !Design Outlet Water Temperature
   32.2,                      !Design Outlet Air Temperature
   ;                      !Rated Ratio for Air and Water Convection
ZoneHVAC:AirDistributionUnit,
   PER-1T_P  VAV system_AHU,                      !Air Distribution Unit Name
   PER-1T_P Zone Inlet Node,                      !Air Dist Unit Outlet Node Name
   AirTerminal:SingleDuct:VAV:Reheat,                      !KEY--System Component Type
   PER-1T_P  VAV system,                      !Component Name
   ,                      !upstream nominal leakage fraction
   ;                      !downstream constant leakage fraction
AirTerminal:SingleDuct:VAV:Reheat,
   PER-2T_P  VAV system,                      !Name of System
   AIRSYSAVAILSCHED,                      !System Availability schedule
   PER-2T_P  VAV system_CoilAirInletNode,                      !DAMPER Air Outlet Node
   PER-2T_P  VAV system_UnitAirInletNode,                      !UNIT Air Inlet Node
   autosize,                      !Maximum air flow rate
   Constant,                      !Zone Minimum Air Flow Input Method
   0.3,                      !Constant Minimum Air Flow Fraction
   ,                      !Fixed Minimum Air Flow Rate
   ,                      !Minimum Air Flow Fraction Schedule Name
   COIL:Heating:Water,                      !Reheat Component Object
   PER-2T_P  VAV system_Coil,                      !Name of Reheat Component
   autosize,                      !Max Reheat Water Flow
   0,                      !Min Reheat Water Flow
   PER-2T_P Zone Inlet Node,                      !UNIT Air Outlet Node
   0.00025,                      !Convergence Tolerance
   NORMAL,                      !Damper Heating Action
   ,                      !Maximum Flow per Zone Floor Area During Reheat
   ,                      !Maximum Flow Fraction During Reheat
   ,                      !Maximum Reheat Air Temperature
   ;                      !Design Specification Outdoor Air Object Name
COIL:Heating:Water,
   PER-2T_P  VAV system_Coil,                      !Coil Name
   HEATINGAVAILSCHED,                      !Available Schedule
   autosize,                      !UA of the Coil
   autosize,                      !Max Water Flow Rate of Coil
   PER-2T_P  VAV system_CoilWaterInletNode,                      !Coil_Water_Inlet_Node
   PER-2T_P  VAV system_CoilWaterOutletNode,                      !Coil_Water_Outlet_Node
   PER-2T_P  VAV system_CoilAirInletNode,                      !Coil_Air_Inlet_Node
   PER-2T_P Zone Inlet Node,                      !Coil_Air_Outlet_Node
   UFactorTimesAreaAndDesignWaterFlowRate,                      !Coil Performance Input Method
   autosize,                      !Nominal Capacity
   82.2,                      !Design Inlet Water Temperature
   16.6,                      !Design Inlet Air Temperature
   71.1,                      !Design Outlet Water Temperature
   32.2,                      !Design Outlet Air Temperature
   ;                      !Rated Ratio for Air and Water Convection
ZoneHVAC:AirDistributionUnit,
   PER-2T_P  VAV system_AHU,                      !Air Distribution Unit Name
   PER-2T_P Zone Inlet Node,                      !Air Dist Unit Outlet Node Name
   AirTerminal:SingleDuct:VAV:Reheat,                      !KEY--System Component Type
   PER-2T_P  VAV system,                      !Component Name
   ,                      !upstream nominal leakage fraction
   ;                      !downstream constant leakage fraction
AirTerminal:SingleDuct:VAV:Reheat,
   PER-3T_P  VAV system,                      !Name of System
   AIRSYSAVAILSCHED,                      !System Availability schedule
   PER-3T_P  VAV system_CoilAirInletNode,                      !DAMPER Air Outlet Node
   PER-3T_P  VAV system_UnitAirInletNode,                      !UNIT Air Inlet Node
   autosize,                      !Maximum air flow rate
   Constant,                      !Zone Minimum Air Flow Input Method
   0.3,                      !Constant Minimum Air Flow Fraction
   ,                      !Fixed Minimum Air Flow Rate
   ,                      !Minimum Air Flow Fraction Schedule Name
   COIL:Heating:Water,                      !Reheat Component Object
   PER-3T_P  VAV system_Coil,                      !Name of Reheat Component
   autosize,                      !Max Reheat Water Flow
   0,                      !Min Reheat Water Flow
   PER-3T_P Zone Inlet Node,                      !UNIT Air Outlet Node
   0.00025,                      !Convergence Tolerance
   NORMAL,                      !Damper Heating Action
   ,                      !Maximum Flow per Zone Floor Area During Reheat
   ,                      !Maximum Flow Fraction During Reheat
   ,                      !Maximum Reheat Air Temperature
   ;                      !Design Specification Outdoor Air Object Name
COIL:Heating:Water,
   PER-3T_P  VAV system_Coil,                      !Coil Name
   HEATINGAVAILSCHED,                      !Available Schedule
   autosize,                      !UA of the Coil
   autosize,                      !Max Water Flow Rate of Coil
   PER-3T_P  VAV system_CoilWaterInletNode,                      !Coil_Water_Inlet_Node
   PER-3T_P  VAV system_CoilWaterOutletNode,                      !Coil_Water_Outlet_Node
   PER-3T_P  VAV system_CoilAirInletNode,                      !Coil_Air_Inlet_Node
   PER-3T_P Zone Inlet Node,                      !Coil_Air_Outlet_Node
   UFactorTimesAreaAndDesignWaterFlowRate,                      !Coil Performance Input Method
   autosize,                      !Nominal Capacity
   82.2,                      !Design Inlet Water Temperature
   16.6,                      !Design Inlet Air Temperature
   71.1,                      !Design Outlet Water Temperature
   32.2,                      !Design Outlet Air Temperature
   ;                      !Rated Ratio for Air and Water Convection
ZoneHVAC:AirDistributionUnit,
   PER-3T_P  VAV system_AHU,                      !Air Distribution Unit Name
   PER-3T_P Zone Inlet Node,                      !Air Dist Unit Outlet Node Name
   AirTerminal:SingleDuct:VAV:Reheat,                      !KEY--System Component Type
   PER-3T_P  VAV system,                      !Component Name
   ,                      !upstream nominal leakage fraction
   ;                      !downstream constant leakage fraction
AirTerminal:SingleDuct:VAV:Reheat,
   PER-4T_P  VAV system,                      !Name of System
   AIRSYSAVAILSCHED,                      !System Availability schedule
   PER-4T_P  VAV system_CoilAirInletNode,                      !DAMPER Air Outlet Node
   PER-4T_P  VAV system_UnitAirInletNode,                      !UNIT Air Inlet Node
   autosize,                      !Maximum air flow rate
   Constant,                      !Zone Minimum Air Flow Input Method
   0.3,                      !Constant Minimum Air Flow Fraction
   ,                      !Fixed Minimum Air Flow Rate
   ,                      !Minimum Air Flow Fraction Schedule Name
   COIL:Heating:Water,                      !Reheat Component Object
   PER-4T_P  VAV system_Coil,                      !Name of Reheat Component
   autosize,                      !Max Reheat Water Flow
   0,                      !Min Reheat Water Flow
   PER-4T_P Zone Inlet Node,                      !UNIT Air Outlet Node
   0.00025,                      !Convergence Tolerance
   NORMAL,                      !Damper Heating Action
   ,                      !Maximum Flow per Zone Floor Area During Reheat
   ,                      !Maximum Flow Fraction During Reheat
   ,                      !Maximum Reheat Air Temperature
   ;                      !Design Specification Outdoor Air Object Name
COIL:Heating:Water,
   PER-4T_P  VAV system_Coil,                      !Coil Name
   HEATINGAVAILSCHED,                      !Available Schedule
   autosize,                      !UA of the Coil
   autosize,                      !Max Water Flow Rate of Coil
   PER-4T_P  VAV system_CoilWaterInletNode,                      !Coil_Water_Inlet_Node
   PER-4T_P  VAV system_CoilWaterOutletNode,                      !Coil_Water_Outlet_Node
   PER-4T_P  VAV system_CoilAirInletNode,                      !Coil_Air_Inlet_Node
   PER-4T_P Zone Inlet Node,                      !Coil_Air_Outlet_Node
   UFactorTimesAreaAndDesignWaterFlowRate,                      !Coil Performance Input Method
   autosize,                      !Nominal Capacity
   82.2,                      !Design Inlet Water Temperature
   16.6,                      !Design Inlet Air Temperature
   71.1,                      !Design Outlet Water Temperature
   32.2,                      !Design Outlet Air Temperature
   ;                      !Rated Ratio for Air and Water Convection
ZoneHVAC:AirDistributionUnit,
   PER-4T_P  VAV system_AHU,                      !Air Distribution Unit Name
   PER-4T_P Zone Inlet Node,                      !Air Dist Unit Outlet Node Name
   AirTerminal:SingleDuct:VAV:Reheat,                      !KEY--System Component Type
   PER-4T_P  VAV system,                      !Component Name
   ,                      !upstream nominal leakage fraction
   ;                      !downstream constant leakage fraction
AirTerminal:SingleDuct:VAV:Reheat,
   PER-1F_P  VAV system,                      !Name of System
   AIRSYSAVAILSCHED,                      !System Availability schedule
   PER-1F_P  VAV system_CoilAirInletNode,                      !DAMPER Air Outlet Node
   PER-1F_P  VAV system_UnitAirInletNode,                      !UNIT Air Inlet Node
   autosize,                      !Maximum air flow rate
   Constant,                      !Zone Minimum Air Flow Input Method
   0.3,                      !Constant Minimum Air Flow Fraction
   ,                      !Fixed Minimum Air Flow Rate
   ,                      !Minimum Air Flow Fraction Schedule Name
   COIL:Heating:Water,                      !Reheat Component Object
   PER-1F_P  VAV system_Coil,                      !Name of Reheat Component
   autosize,                      !Max Reheat Water Flow
   0,                      !Min Reheat Water Flow
   PER-1F_P Zone Inlet Node,                      !UNIT Air Outlet Node
   0.00025,                      !Convergence Tolerance
   NORMAL,                      !Damper Heating Action
   ,                      !Maximum Flow per Zone Floor Area During Reheat
   ,                      !Maximum Flow Fraction During Reheat
   ,                      !Maximum Reheat Air Temperature
   ;                      !Design Specification Outdoor Air Object Name
COIL:Heating:Water,
   PER-1F_P  VAV system_Coil,                      !Coil Name
   HEATINGAVAILSCHED,                      !Available Schedule
   autosize,                      !UA of the Coil
   autosize,                      !Max Water Flow Rate of Coil
   PER-1F_P  VAV system_CoilWaterInletNode,                      !Coil_Water_Inlet_Node
   PER-1F_P  VAV system_CoilWaterOutletNode,                      !Coil_Water_Outlet_Node
   PER-1F_P  VAV system_CoilAirInletNode,                      !Coil_Air_Inlet_Node
   PER-1F_P Zone Inlet Node,                      !Coil_Air_Outlet_Node
   UFactorTimesAreaAndDesignWaterFlowRate,                      !Coil Performance Input Method
   autosize,                      !Nominal Capacity
   82.2,                      !Design Inlet Water Temperature
   16.6,                      !Design Inlet Air Temperature
   71.1,                      !Design Outlet Water Temperature
   32.2,                      !Design Outlet Air Temperature
   ;                      !Rated Ratio for Air and Water Convection
ZoneHVAC:AirDistributionUnit,
   PER-1F_P  VAV system_AHU,                      !Air Distribution Unit Name
   PER-1F_P Zone Inlet Node,                      !Air Dist Unit Outlet Node Name
   AirTerminal:SingleDuct:VAV:Reheat,                      !KEY--System Component Type
   PER-1F_P  VAV system,                      !Component Name
   ,                      !upstream nominal leakage fraction
   ;                      !downstream constant leakage fraction
AirTerminal:SingleDuct:VAV:Reheat,
   PER-2F_P  VAV system,                      !Name of System
   AIRSYSAVAILSCHED,                      !System Availability schedule
   PER-2F_P  VAV system_CoilAirInletNode,                      !DAMPER Air Outlet Node
   PER-2F_P  VAV system_UnitAirInletNode,                      !UNIT Air Inlet Node
   autosize,                      !Maximum air flow rate
   Constant,                      !Zone Minimum Air Flow Input Method
   0.3,                      !Constant Minimum Air Flow Fraction
   ,                      !Fixed Minimum Air Flow Rate
   ,                      !Minimum Air Flow Fraction Schedule Name
   COIL:Heating:Water,                      !Reheat Component Object
   PER-2F_P  VAV system_Coil,                      !Name of Reheat Component
   autosize,                      !Max Reheat Water Flow
   0,                      !Min Reheat Water Flow
   PER-2F_P Zone Inlet Node,                      !UNIT Air Outlet Node
   0.00025,                      !Convergence Tolerance
   NORMAL,                      !Damper Heating Action
   ,                      !Maximum Flow per Zone Floor Area During Reheat
   ,                      !Maximum Flow Fraction During Reheat
   ,                      !Maximum Reheat Air Temperature
   ;                      !Design Specification Outdoor Air Object Name
COIL:Heating:Water,
   PER-2F_P  VAV system_Coil,                      !Coil Name
   HEATINGAVAILSCHED,                      !Available Schedule
   autosize,                      !UA of the Coil
   autosize,                      !Max Water Flow Rate of Coil
   PER-2F_P  VAV system_CoilWaterInletNode,                      !Coil_Water_Inlet_Node
   PER-2F_P  VAV system_CoilWaterOutletNode,                      !Coil_Water_Outlet_Node
   PER-2F_P  VAV system_CoilAirInletNode,                      !Coil_Air_Inlet_Node
   PER-2F_P Zone Inlet Node,                      !Coil_Air_Outlet_Node
   UFactorTimesAreaAndDesignWaterFlowRate,                      !Coil Performance Input Method
   autosize,                      !Nominal Capacity
   82.2,                      !Design Inlet Water Temperature
   16.6,                      !Design Inlet Air Temperature
   71.1,                      !Design Outlet Water Temperature
   32.2,                      !Design Outlet Air Temperature
   ;                      !Rated Ratio for Air and Water Convection
ZoneHVAC:AirDistributionUnit,
   PER-2F_P  VAV system_AHU,                      !Air Distribution Unit Name
   PER-2F_P Zone Inlet Node,                      !Air Dist Unit Outlet Node Name
   AirTerminal:SingleDuct:VAV:Reheat,                      !KEY--System Component Type
   PER-2F_P  VAV system,                      !Component Name
   ,                      !upstream nominal leakage fraction
   ;                      !downstream constant leakage fraction
AirTerminal:SingleDuct:VAV:Reheat,
   PER-3F_P  VAV system,                      !Name of System
   AIRSYSAVAILSCHED,                      !System Availability schedule
   PER-3F_P  VAV system_CoilAirInletNode,                      !DAMPER Air Outlet Node
   PER-3F_P  VAV system_UnitAirInletNode,                      !UNIT Air Inlet Node
   autosize,                      !Maximum air flow rate
   Constant,                      !Zone Minimum Air Flow Input Method
   0.3,                      !Constant Minimum Air Flow Fraction
   ,                      !Fixed Minimum Air Flow Rate
   ,                      !Minimum Air Flow Fraction Schedule Name
   COIL:Heating:Water,                      !Reheat Component Object
   PER-3F_P  VAV system_Coil,                      !Name of Reheat Component
   autosize,                      !Max Reheat Water Flow
   0,                      !Min Reheat Water Flow
   PER-3F_P Zone Inlet Node,                      !UNIT Air Outlet Node
   0.00025,                      !Convergence Tolerance
   NORMAL,                      !Damper Heating Action
   ,                      !Maximum Flow per Zone Floor Area During Reheat
   ,                      !Maximum Flow Fraction During Reheat
   ,                      !Maximum Reheat Air Temperature
   ;                      !Design Specification Outdoor Air Object Name
COIL:Heating:Water,
   PER-3F_P  VAV system_Coil,                      !Coil Name
   HEATINGAVAILSCHED,                      !Available Schedule
   autosize,                      !UA of the Coil
   autosize,                      !Max Water Flow Rate of Coil
   PER-3F_P  VAV system_CoilWaterInletNode,                      !Coil_Water_Inlet_Node
   PER-3F_P  VAV system_CoilWaterOutletNode,                      !Coil_Water_Outlet_Node
   PER-3F_P  VAV system_CoilAirInletNode,                      !Coil_Air_Inlet_Node
   PER-3F_P Zone Inlet Node,                      !Coil_Air_Outlet_Node
   UFactorTimesAreaAndDesignWaterFlowRate,                      !Coil Performance Input Method
   autosize,                      !Nominal Capacity
   82.2,                      !Design Inlet Water Temperature
   16.6,                      !Design Inlet Air Temperature
   71.1,                      !Design Outlet Water Temperature
   32.2,                      !Design Outlet Air Temperature
   ;                      !Rated Ratio for Air and Water Convection
ZoneHVAC:AirDistributionUnit,
   PER-3F_P  VAV system_AHU,                      !Air Distribution Unit Name
   PER-3F_P Zone Inlet Node,                      !Air Dist Unit Outlet Node Name
   AirTerminal:SingleDuct:VAV:Reheat,                      !KEY--System Component Type
   PER-3F_P  VAV system,                      !Component Name
   ,                      !upstream nominal leakage fraction
   ;                      !downstream constant leakage fraction
AirTerminal:SingleDuct:VAV:Reheat,
   PER-4F_P  VAV system,                      !Name of System
   AIRSYSAVAILSCHED,                      !System Availability schedule
   PER-4F_P  VAV system_CoilAirInletNode,                      !DAMPER Air Outlet Node
   PER-4F_P  VAV system_UnitAirInletNode,                      !UNIT Air Inlet Node
   autosize,                      !Maximum air flow rate
   Constant,                      !Zone Minimum Air Flow Input Method
   0.3,                      !Constant Minimum Air Flow Fraction
   ,                      !Fixed Minimum Air Flow Rate
   ,                      !Minimum Air Flow Fraction Schedule Name
   COIL:Heating:Water,                      !Reheat Component Object
   PER-4F_P  VAV system_Coil,                      !Name of Reheat Component
   autosize,                      !Max Reheat Water Flow
   0,                      !Min Reheat Water Flow
   PER-4F_P Zone Inlet Node,                      !UNIT Air Outlet Node
   0.00025,                      !Convergence Tolerance
   NORMAL,                      !Damper Heating Action
   ,                      !Maximum Flow per Zone Floor Area During Reheat
   ,                      !Maximum Flow Fraction During Reheat
   ,                      !Maximum Reheat Air Temperature
   ;                      !Design Specification Outdoor Air Object Name
COIL:Heating:Water,
   PER-4F_P  VAV system_Coil,                      !Coil Name
   HEATINGAVAILSCHED,                      !Available Schedule
   autosize,                      !UA of the Coil
   autosize,                      !Max Water Flow Rate of Coil
   PER-4F_P  VAV system_CoilWaterInletNode,                      !Coil_Water_Inlet_Node
   PER-4F_P  VAV system_CoilWaterOutletNode,                      !Coil_Water_Outlet_Node
   PER-4F_P  VAV system_CoilAirInletNode,                      !Coil_Air_Inlet_Node
   PER-4F_P Zone Inlet Node,                      !Coil_Air_Outlet_Node
   UFactorTimesAreaAndDesignWaterFlowRate,                      !Coil Performance Input Method
   autosize,                      !Nominal Capacity
   82.2,                      !Design Inlet Water Temperature
   16.6,                      !Design Inlet Air Temperature
   71.1,                      !Design Outlet Water Temperature
   32.2,                      !Design Outlet Air Temperature
   ;                      !Rated Ratio for Air and Water Convection
ZoneHVAC:AirDistributionUnit,
   PER-4F_P  VAV system_AHU,                      !Air Distribution Unit Name
   PER-4F_P Zone Inlet Node,                      !Air Dist Unit Outlet Node Name
   AirTerminal:SingleDuct:VAV:Reheat,                      !KEY--System Component Type
   PER-4F_P  VAV system,                      !Component Name
   ,                      !upstream nominal leakage fraction
   ;                      !downstream constant leakage fraction
AirTerminal:SingleDuct:VAV:Reheat,
   PER-1I_P  VAV system,                      !Name of System
   AIRSYSAVAILSCHED,                      !System Availability schedule
   PER-1I_P  VAV system_CoilAirInletNode,                      !DAMPER Air Outlet Node
   PER-1I_P  VAV system_UnitAirInletNode,                      !UNIT Air Inlet Node
   autosize,                      !Maximum air flow rate
   Constant,                      !Zone Minimum Air Flow Input Method
   0.3,                      !Constant Minimum Air Flow Fraction
   ,                      !Fixed Minimum Air Flow Rate
   ,                      !Minimum Air Flow Fraction Schedule Name
   COIL:Heating:Water,                      !Reheat Component Object
   PER-1I_P  VAV system_Coil,                      !Name of Reheat Component
   autosize,                      !Max Reheat Water Flow
   0,                      !Min Reheat Water Flow
   PER-1I_P Zone Inlet Node,                      !UNIT Air Outlet Node
   0.00025,                      !Convergence Tolerance
   NORMAL,                      !Damper Heating Action
   ,                      !Maximum Flow per Zone Floor Area During Reheat
   ,                      !Maximum Flow Fraction During Reheat
   ,                      !Maximum Reheat Air Temperature
   ;                      !Design Specification Outdoor Air Object Name
COIL:Heating:Water,
   PER-1I_P  VAV system_Coil,                      !Coil Name
   HEATINGAVAILSCHED,                      !Available Schedule
   autosize,                      !UA of the Coil
   autosize,                      !Max Water Flow Rate of Coil
   PER-1I_P  VAV system_CoilWaterInletNode,                      !Coil_Water_Inlet_Node
   PER-1I_P  VAV system_CoilWaterOutletNode,                      !Coil_Water_Outlet_Node
   PER-1I_P  VAV system_CoilAirInletNode,                      !Coil_Air_Inlet_Node
   PER-1I_P Zone Inlet Node,                      !Coil_Air_Outlet_Node
   UFactorTimesAreaAndDesignWaterFlowRate,                      !Coil Performance Input Method
   autosize,                      !Nominal Capacity
   82.2,                      !Design Inlet Water Temperature
   16.6,                      !Design Inlet Air Temperature
   71.1,                      !Design Outlet Water Temperature
   32.2,                      !Design Outlet Air Temperature
   ;                      !Rated Ratio for Air and Water Convection
ZoneHVAC:AirDistributionUnit,
   PER-1I_P  VAV system_AHU,                      !Air Distribution Unit Name
   PER-1I_P Zone Inlet Node,                      !Air Dist Unit Outlet Node Name
   AirTerminal:SingleDuct:VAV:Reheat,                      !KEY--System Component Type
   PER-1I_P  VAV system,                      !Component Name
   ,                      !upstream nominal leakage fraction
   ;                      !downstream constant leakage fraction
AirTerminal:SingleDuct:VAV:Reheat,
   PER-2I_P  VAV system,                      !Name of System
   AIRSYSAVAILSCHED,                      !System Availability schedule
   PER-2I_P  VAV system_CoilAirInletNode,                      !DAMPER Air Outlet Node
   PER-2I_P  VAV system_UnitAirInletNode,                      !UNIT Air Inlet Node
   autosize,                      !Maximum air flow rate
   Constant,                      !Zone Minimum Air Flow Input Method
   0.3,                      !Constant Minimum Air Flow Fraction
   ,                      !Fixed Minimum Air Flow Rate
   ,                      !Minimum Air Flow Fraction Schedule Name
   COIL:Heating:Water,                      !Reheat Component Object
   PER-2I_P  VAV system_Coil,                      !Name of Reheat Component
   autosize,                      !Max Reheat Water Flow
   0,                      !Min Reheat Water Flow
   PER-2I_P Zone Inlet Node,                      !UNIT Air Outlet Node
   0.00025,                      !Convergence Tolerance
   NORMAL,                      !Damper Heating Action
   ,                      !Maximum Flow per Zone Floor Area During Reheat
   ,                      !Maximum Flow Fraction During Reheat
   ,                      !Maximum Reheat Air Temperature
   ;                      !Design Specification Outdoor Air Object Name
COIL:Heating:Water,
   PER-2I_P  VAV system_Coil,                      !Coil Name
   HEATINGAVAILSCHED,                      !Available Schedule
   autosize,                      !UA of the Coil
   autosize,                      !Max Water Flow Rate of Coil
   PER-2I_P  VAV system_CoilWaterInletNode,                      !Coil_Water_Inlet_Node
   PER-2I_P  VAV system_CoilWaterOutletNode,                      !Coil_Water_Outlet_Node
   PER-2I_P  VAV system_CoilAirInletNode,                      !Coil_Air_Inlet_Node
   PER-2I_P Zone Inlet Node,                      !Coil_Air_Outlet_Node
   UFactorTimesAreaAndDesignWaterFlowRate,                      !Coil Performance Input Method
   autosize,                      !Nominal Capacity
   82.2,                      !Design Inlet Water Temperature
   16.6,                      !Design Inlet Air Temperature
   71.1,                      !Design Outlet Water Temperature
   32.2,                      !Design Outlet Air Temperature
   ;                      !Rated Ratio for Air and Water Convection
ZoneHVAC:AirDistributionUnit,
   PER-2I_P  VAV system_AHU,                      !Air Distribution Unit Name
   PER-2I_P Zone Inlet Node,                      !Air Dist Unit Outlet Node Name
   AirTerminal:SingleDuct:VAV:Reheat,                      !KEY--System Component Type
   PER-2I_P  VAV system,                      !Component Name
   ,                      !upstream nominal leakage fraction
   ;                      !downstream constant leakage fraction
AirTerminal:SingleDuct:VAV:Reheat,
   PER-3I_P  VAV system,                      !Name of System
   AIRSYSAVAILSCHED,                      !System Availability schedule
   PER-3I_P  VAV system_CoilAirInletNode,                      !DAMPER Air Outlet Node
   PER-3I_P  VAV system_UnitAirInletNode,                      !UNIT Air Inlet Node
   autosize,                      !Maximum air flow rate
   Constant,                      !Zone Minimum Air Flow Input Method
   0.3,                      !Constant Minimum Air Flow Fraction
   ,                      !Fixed Minimum Air Flow Rate
   ,                      !Minimum Air Flow Fraction Schedule Name
   COIL:Heating:Water,                      !Reheat Component Object
   PER-3I_P  VAV system_Coil,                      !Name of Reheat Component
   autosize,                      !Max Reheat Water Flow
   0,                      !Min Reheat Water Flow
   PER-3I_P Zone Inlet Node,                      !UNIT Air Outlet Node
   0.00025,                      !Convergence Tolerance
   NORMAL,                      !Damper Heating Action
   ,                      !Maximum Flow per Zone Floor Area During Reheat
   ,                      !Maximum Flow Fraction During Reheat
   ,                      !Maximum Reheat Air Temperature
   ;                      !Design Specification Outdoor Air Object Name
COIL:Heating:Water,
   PER-3I_P  VAV system_Coil,                      !Coil Name
   HEATINGAVAILSCHED,                      !Available Schedule
   autosize,                      !UA of the Coil
   autosize,                      !Max Water Flow Rate of Coil
   PER-3I_P  VAV system_CoilWaterInletNode,                      !Coil_Water_Inlet_Node
   PER-3I_P  VAV system_CoilWaterOutletNode,                      !Coil_Water_Outlet_Node
   PER-3I_P  VAV system_CoilAirInletNode,                      !Coil_Air_Inlet_Node
   PER-3I_P Zone Inlet Node,                      !Coil_Air_Outlet_Node
   UFactorTimesAreaAndDesignWaterFlowRate,                      !Coil Performance Input Method
   autosize,                      !Nominal Capacity
   82.2,                      !Design Inlet Water Temperature
   16.6,                      !Design Inlet Air Temperature
   71.1,                      !Design Outlet Water Temperature
   32.2,                      !Design Outlet Air Temperature
   ;                      !Rated Ratio for Air and Water Convection
ZoneHVAC:AirDistributionUnit,
   PER-3I_P  VAV system_AHU,                      !Air Distribution Unit Name
   PER-3I_P Zone Inlet Node,                      !Air Dist Unit Outlet Node Name
   AirTerminal:SingleDuct:VAV:Reheat,                      !KEY--System Component Type
   PER-3I_P  VAV system,                      !Component Name
   ,                      !upstream nominal leakage fraction
   ;                      !downstream constant leakage fraction
AirTerminal:SingleDuct:VAV:Reheat,
   PER-4I_P  VAV system,                      !Name of System
   AIRSYSAVAILSCHED,                      !System Availability schedule
   PER-4I_P  VAV system_CoilAirInletNode,                      !DAMPER Air Outlet Node
   PER-4I_P  VAV system_UnitAirInletNode,                      !UNIT Air Inlet Node
   autosize,                      !Maximum air flow rate
   Constant,                      !Zone Minimum Air Flow Input Method
   0.3,                      !Constant Minimum Air Flow Fraction
   ,                      !Fixed Minimum Air Flow Rate
   ,                      !Minimum Air Flow Fraction Schedule Name
   COIL:Heating:Water,                      !Reheat Component Object
   PER-4I_P  VAV system_Coil,                      !Name of Reheat Component
   autosize,                      !Max Reheat Water Flow
   0,                      !Min Reheat Water Flow
   PER-4I_P Zone Inlet Node,                      !UNIT Air Outlet Node
   0.00025,                      !Convergence Tolerance
   NORMAL,                      !Damper Heating Action
   ,                      !Maximum Flow per Zone Floor Area During Reheat
   ,                      !Maximum Flow Fraction During Reheat
   ,                      !Maximum Reheat Air Temperature
   ;                      !Design Specification Outdoor Air Object Name
COIL:Heating:Water,
   PER-4I_P  VAV system_Coil,                      !Coil Name
   HEATINGAVAILSCHED,                      !Available Schedule
   autosize,                      !UA of the Coil
   autosize,                      !Max Water Flow Rate of Coil
   PER-4I_P  VAV system_CoilWaterInletNode,                      !Coil_Water_Inlet_Node
   PER-4I_P  VAV system_CoilWaterOutletNode,                      !Coil_Water_Outlet_Node
   PER-4I_P  VAV system_CoilAirInletNode,                      !Coil_Air_Inlet_Node
   PER-4I_P Zone Inlet Node,                      !Coil_Air_Outlet_Node
   UFactorTimesAreaAndDesignWaterFlowRate,                      !Coil Performance Input Method
   autosize,                      !Nominal Capacity
   82.2,                      !Design Inlet Water Temperature
   16.6,                      !Design Inlet Air Temperature
   71.1,                      !Design Outlet Water Temperature
   32.2,                      !Design Outlet Air Temperature
   ;                      !Rated Ratio for Air and Water Convection
ZoneHVAC:AirDistributionUnit,
   PER-4I_P  VAV system_AHU,                      !Air Distribution Unit Name
   PER-4I_P Zone Inlet Node,                      !Air Dist Unit Outlet Node Name
   AirTerminal:SingleDuct:VAV:Reheat,                      !KEY--System Component Type
   PER-4I_P  VAV system,                      !Component Name
   ,                      !upstream nominal leakage fraction
   ;                      !downstream constant leakage fraction
AirTerminal:SingleDuct:VAV:Reheat,
   COR-T_C  VAV system,                      !Name of System
   AIRSYSAVAILSCHED,                      !System Availability schedule
   COR-T_C  VAV system_CoilAirInletNode,                      !DAMPER Air Outlet Node
   COR-T_C  VAV system_UnitAirInletNode,                      !UNIT Air Inlet Node
   autosize,                      !Maximum air flow rate
   Constant,                      !Zone Minimum Air Flow Input Method
   0.5,                      !Constant Minimum Air Flow Fraction
   ,                      !Fixed Minimum Air Flow Rate
   ,                      !Minimum Air Flow Fraction Schedule Name
   COIL:Heating:Water,                      !Reheat Component Object
   COR-T_C  VAV system_Coil,                      !Name of Reheat Component
   autosize,                      !Max Reheat Water Flow
   0,                      !Min Reheat Water Flow
   COR-T_C Zone Inlet Node,                      !UNIT Air Outlet Node
   0.00025,                      !Convergence Tolerance
   NORMAL,                      !Damper Heating Action
   ,                      !Maximum Flow per Zone Floor Area During Reheat
   ,                      !Maximum Flow Fraction During Reheat
   ,                      !Maximum Reheat Air Temperature
   ;                      !Design Specification Outdoor Air Object Name
COIL:Heating:Water,
   COR-T_C  VAV system_Coil,                      !Coil Name
   HEATINGAVAILSCHED,                      !Available Schedule
   autosize,                      !UA of the Coil
   autosize,                      !Max Water Flow Rate of Coil
   COR-T_C  VAV system_CoilWaterInletNode,                      !Coil_Water_Inlet_Node
   COR-T_C  VAV system_CoilWaterOutletNode,                      !Coil_Water_Outlet_Node
   COR-T_C  VAV system_CoilAirInletNode,                      !Coil_Air_Inlet_Node
   COR-T_C Zone Inlet Node,                      !Coil_Air_Outlet_Node
   UFactorTimesAreaAndDesignWaterFlowRate,                      !Coil Performance Input Method
   autosize,                      !Nominal Capacity
   82.2,                      !Design Inlet Water Temperature
   16.6,                      !Design Inlet Air Temperature
   71.1,                      !Design Outlet Water Temperature
   32.2,                      !Design Outlet Air Temperature
   ;                      !Rated Ratio for Air and Water Convection
ZoneHVAC:AirDistributionUnit,
   COR-T_C  VAV system_AHU,                      !Air Distribution Unit Name
   COR-T_C Zone Inlet Node,                      !Air Dist Unit Outlet Node Name
   AirTerminal:SingleDuct:VAV:Reheat,                      !KEY--System Component Type
   COR-T_C  VAV system,                      !Component Name
   ,                      !upstream nominal leakage fraction
   ;                      !downstream constant leakage fraction
AirTerminal:SingleDuct:VAV:Reheat,
   COR-F_C  VAV system,                      !Name of System
   AIRSYSAVAILSCHED,                      !System Availability schedule
   COR-F_C  VAV system_CoilAirInletNode,                      !DAMPER Air Outlet Node
   COR-F_C  VAV system_UnitAirInletNode,                      !UNIT Air Inlet Node
   autosize,                      !Maximum air flow rate
   Constant,                      !Zone Minimum Air Flow Input Method
   0.5,                      !Constant Minimum Air Flow Fraction
   ,                      !Fixed Minimum Air Flow Rate
   ,                      !Minimum Air Flow Fraction Schedule Name
   COIL:Heating:Water,                      !Reheat Component Object
   COR-F_C  VAV system_Coil,                      !Name of Reheat Component
   autosize,                      !Max Reheat Water Flow
   0,                      !Min Reheat Water Flow
   COR-F_C Zone Inlet Node,                      !UNIT Air Outlet Node
   0.00025,                      !Convergence Tolerance
   NORMAL,                      !Damper Heating Action
   ,                      !Maximum Flow per Zone Floor Area During Reheat
   ,                      !Maximum Flow Fraction During Reheat
   ,                      !Maximum Reheat Air Temperature
   ;                      !Design Specification Outdoor Air Object Name
COIL:Heating:Water,
   COR-F_C  VAV system_Coil,                      !Coil Name
   HEATINGAVAILSCHED,                      !Available Schedule
   autosize,                      !UA of the Coil
   autosize,                      !Max Water Flow Rate of Coil
   COR-F_C  VAV system_CoilWaterInletNode,                      !Coil_Water_Inlet_Node
   COR-F_C  VAV system_CoilWaterOutletNode,                      !Coil_Water_Outlet_Node
   COR-F_C  VAV system_CoilAirInletNode,                      !Coil_Air_Inlet_Node
   COR-F_C Zone Inlet Node,                      !Coil_Air_Outlet_Node
   UFactorTimesAreaAndDesignWaterFlowRate,                      !Coil Performance Input Method
   autosize,                      !Nominal Capacity
   82.2,                      !Design Inlet Water Temperature
   16.6,                      !Design Inlet Air Temperature
   71.1,                      !Design Outlet Water Temperature
   32.2,                      !Design Outlet Air Temperature
   ;                      !Rated Ratio for Air and Water Convection
ZoneHVAC:AirDistributionUnit,
   COR-F_C  VAV system_AHU,                      !Air Distribution Unit Name
   COR-F_C Zone Inlet Node,                      !Air Dist Unit Outlet Node Name
   AirTerminal:SingleDuct:VAV:Reheat,                      !KEY--System Component Type
   COR-F_C  VAV system,                      !Component Name
   ,                      !upstream nominal leakage fraction
   ;                      !downstream constant leakage fraction
AirTerminal:SingleDuct:VAV:Reheat,
   COR-I_C  VAV system,                      !Name of System
   AIRSYSAVAILSCHED,                      !System Availability schedule
   COR-I_C  VAV system_CoilAirInletNode,                      !DAMPER Air Outlet Node
   COR-I_C  VAV system_UnitAirInletNode,                      !UNIT Air Inlet Node
   autosize,                      !Maximum air flow rate
   Constant,                      !Zone Minimum Air Flow Input Method
   0.5,                      !Constant Minimum Air Flow Fraction
   ,                      !Fixed Minimum Air Flow Rate
   ,                      !Minimum Air Flow Fraction Schedule Name
   COIL:Heating:Water,                      !Reheat Component Object
   COR-I_C  VAV system_Coil,                      !Name of Reheat Component
   autosize,                      !Max Reheat Water Flow
   0,                      !Min Reheat Water Flow
   COR-I_C Zone Inlet Node,                      !UNIT Air Outlet Node
   0.00025,                      !Convergence Tolerance
   NORMAL,                      !Damper Heating Action
   ,                      !Maximum Flow per Zone Floor Area During Reheat
   ,                      !Maximum Flow Fraction During Reheat
   ,                      !Maximum Reheat Air Temperature
   ;                      !Design Specification Outdoor Air Object Name
COIL:Heating:Water,
   COR-I_C  VAV system_Coil,                      !Coil Name
   HEATINGAVAILSCHED,                      !Available Schedule
   autosize,                      !UA of the Coil
   autosize,                      !Max Water Flow Rate of Coil
   COR-I_C  VAV system_CoilWaterInletNode,                      !Coil_Water_Inlet_Node
   COR-I_C  VAV system_CoilWaterOutletNode,                      !Coil_Water_Outlet_Node
   COR-I_C  VAV system_CoilAirInletNode,                      !Coil_Air_Inlet_Node
   COR-I_C Zone Inlet Node,                      !Coil_Air_Outlet_Node
   UFactorTimesAreaAndDesignWaterFlowRate,                      !Coil Performance Input Method
   autosize,                      !Nominal Capacity
   82.2,                      !Design Inlet Water Temperature
   16.6,                      !Design Inlet Air Temperature
   71.1,                      !Design Outlet Water Temperature
   32.2,                      !Design Outlet Air Temperature
   ;                      !Rated Ratio for Air and Water Convection
ZoneHVAC:AirDistributionUnit,
   COR-I_C  VAV system_AHU,                      !Air Distribution Unit Name
   COR-I_C Zone Inlet Node,                      !Air Dist Unit Outlet Node Name
   AirTerminal:SingleDuct:VAV:Reheat,                      !KEY--System Component Type
   COR-I_C  VAV system,                      !Component Name
   ,                      !upstream nominal leakage fraction
   ;                      !downstream constant leakage fraction
ZoneHVAC:EquipmentConnections,
   PER-1T,                      !Zone Name
   PER-1T_P Zone EquipList,                      !List Name: Zone Equipment
   PER-1T_P Zone Inlet Node,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   PER-1T_P ZoneGroup_ZoneAirNodeName,                      !Zone Air Node Name
   PER-1T_P ZoneGroup_ZoneReturnAirNodeName;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   PER-2T,                      !Zone Name
   PER-2T_P Zone EquipList,                      !List Name: Zone Equipment
   PER-2T_P Zone Inlet Node,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   PER-2T_P ZoneGroup_ZoneAirNodeName,                      !Zone Air Node Name
   PER-2T_P ZoneGroup_ZoneReturnAirNodeName;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   PER-3T,                      !Zone Name
   PER-3T_P Zone EquipList,                      !List Name: Zone Equipment
   PER-3T_P Zone Inlet Node,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   PER-3T_P ZoneGroup_ZoneAirNodeName,                      !Zone Air Node Name
   PER-3T_P ZoneGroup_ZoneReturnAirNodeName;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   PER-4T,                      !Zone Name
   PER-4T_P Zone EquipList,                      !List Name: Zone Equipment
   PER-4T_P Zone Inlet Node,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   PER-4T_P ZoneGroup_ZoneAirNodeName,                      !Zone Air Node Name
   PER-4T_P ZoneGroup_ZoneReturnAirNodeName;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   PER-1F,                      !Zone Name
   PER-1F_P Zone EquipList,                      !List Name: Zone Equipment
   PER-1F_P Zone Inlet Node,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   PER-1F_P ZoneGroup_ZoneAirNodeName,                      !Zone Air Node Name
   PER-1F_P ZoneGroup_ZoneReturnAirNodeName;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   PER-2F,                      !Zone Name
   PER-2F_P Zone EquipList,                      !List Name: Zone Equipment
   PER-2F_P Zone Inlet Node,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   PER-2F_P ZoneGroup_ZoneAirNodeName,                      !Zone Air Node Name
   PER-2F_P ZoneGroup_ZoneReturnAirNodeName;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   PER-3F,                      !Zone Name
   PER-3F_P Zone EquipList,                      !List Name: Zone Equipment
   PER-3F_P Zone Inlet Node,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   PER-3F_P ZoneGroup_ZoneAirNodeName,                      !Zone Air Node Name
   PER-3F_P ZoneGroup_ZoneReturnAirNodeName;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   PER-4F,                      !Zone Name
   PER-4F_P Zone EquipList,                      !List Name: Zone Equipment
   PER-4F_P Zone Inlet Node,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   PER-4F_P ZoneGroup_ZoneAirNodeName,                      !Zone Air Node Name
   PER-4F_P ZoneGroup_ZoneReturnAirNodeName;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   PER-1I,                      !Zone Name
   PER-1I_P Zone EquipList,                      !List Name: Zone Equipment
   PER-1I_P Zone Inlet Node,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   PER-1I_P ZoneGroup_ZoneAirNodeName,                      !Zone Air Node Name
   PER-1I_P ZoneGroup_ZoneReturnAirNodeName;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   PER-2I,                      !Zone Name
   PER-2I_P Zone EquipList,                      !List Name: Zone Equipment
   PER-2I_P Zone Inlet Node,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   PER-2I_P ZoneGroup_ZoneAirNodeName,                      !Zone Air Node Name
   PER-2I_P ZoneGroup_ZoneReturnAirNodeName;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   PER-3I,                      !Zone Name
   PER-3I_P Zone EquipList,                      !List Name: Zone Equipment
   PER-3I_P Zone Inlet Node,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   PER-3I_P ZoneGroup_ZoneAirNodeName,                      !Zone Air Node Name
   PER-3I_P ZoneGroup_ZoneReturnAirNodeName;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   PER-4I,                      !Zone Name
   PER-4I_P Zone EquipList,                      !List Name: Zone Equipment
   PER-4I_P Zone Inlet Node,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   PER-4I_P ZoneGroup_ZoneAirNodeName,                      !Zone Air Node Name
   PER-4I_P ZoneGroup_ZoneReturnAirNodeName;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   COR-T,                      !Zone Name
   COR-T_C Zone EquipList,                      !List Name: Zone Equipment
   COR-T_C Zone Inlet Node,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   COR-T_C ZoneGroup_ZoneAirNodeName,                      !Zone Air Node Name
   COR-T_C ZoneGroup_ZoneReturnAirNodeName;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   COR-F,                      !Zone Name
   COR-F_C Zone EquipList,                      !List Name: Zone Equipment
   COR-F_C Zone Inlet Node,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   COR-F_C ZoneGroup_ZoneAirNodeName,                      !Zone Air Node Name
   COR-F_C ZoneGroup_ZoneReturnAirNodeName;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   COR-I,                      !Zone Name
   COR-I_C Zone EquipList,                      !List Name: Zone Equipment
   COR-I_C Zone Inlet Node,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   COR-I_C ZoneGroup_ZoneAirNodeName,                      !Zone Air Node Name
   COR-I_C ZoneGroup_ZoneReturnAirNodeName;                      !Zone Return Air Node Name
Fan:VariableVolume,
   Supply Fan 1,                         !Fan Name
   AIRSYSAVAILSCHED,                         !Available Schedule
   0.7,                         !Fan Total Efficiency
   1000,                         !Delta Pressure
   autosize,                         !Max Flow Rate
   Fraction,                         !Fan Power Minimum Flow Rate Input Method
   0.25,                         !Fan Power Minimum Flow Fraction
   ,                         !Fan Power Minimum Air Flow Rate
   0.9,                         !Motor Efficiency
   1.0,                         !Motor In Airstream Fraction
   0.35071223,                         !FanCoefficient 1
   0.30850,                         !FanCoefficient 2
   0.54137,                         !FanCoefficient 3
   0.87199,                         !FanCoefficient 4
   0,                         !FanCoefficient 5
   Mixed Air Node 1,                         !Fan_Inlet_Node
   Supply Fan 1_FanOutletNode,                         !Fan_Outlet_Node
   General;                         !End-Use Subcategory
COIL:Cooling:Water,
   Simple Cooling Coil,                         !Coil Name
   COOLINGAVAILSCHED,                         !Available Schedule
   autosize,                         !Design Water Flow Rate of Coil
   autosize,                         !Design Air Volume Flow Rate
   autosize,                         !Design Inlet Water Temperature
   autosize,                         !Design Inlet Air Temperature
   autosize,                         !Design Outlet Air Temperature
   autosize,                         !Design Inlet Air Humidity Ratio 
   autosize,                         !Design Outlet Air Humidity Ratio
   Simple Cooling Coil_WaterInletNode,                         !Coil_Water_Inlet_Node
   Simple Cooling Coil_WaterOutletNode,                         !Coil_Water_Outlet_Node
   Supply Fan 1_FanOutletNode,                         !Coil_Air_Inlet_Node
   Simple Cooling Coil_AirOutletNode,                         !Coil_Air_Outlet_Node
   SimpleAnalysis,                         !Type of Analysis
   CrossFlow,                         !Heat Exchanger Configuration
   ;                         !Name of Water Storage Tank for Condensate Collection
OutdoorAir:Mixer,
   OA Mixing Box 1,                         !Name
   Mixed Air Node 1,                         !Mixed_Air_Node
   OAMixer1_OutsideAirStreamNode,                         !Outside_Air_Stream_Node
   OAMixer1_ReliefAirStreamNode,                         !Relief_Air_Stream_Node
   OAMixer1_ReturnAirStreamNode;                         !Return_Air_Stream_Node
AirLoopHVAC:OutdoorAirSystem,
   OA System 1,                         !Name
   OA System 1 Controller,                         !Name: Controller List
   OA System 1 Equipment,                         !Name of an Air Loop Equipment List
   VAV Sys 1 Avail List;                         !Name of a System Availability Manager List
Pump:VariableSpeed,
   Cond Circ Pump,                         !Pump Name
   Condenser Supply Inlet Node,                         !Inlet_Node
   Condenser Pump Outlet Node,                         !Outlet_Node
   autosize,                         !Rated Volumetric Flow Rate
   179352,                         !Rated Pump Head
   autosize,                         !Rated Power Consumption
   0.9,                         !Motor Efficiency
   0,                         !Fraction of Motor Inefficiencies to Fluid Stream
   0,                         !Coefficient1 of the Part Load Performance Curve
   1,                         !Coefficient2 of the Part Load Performance Curve
   0,                         !Coefficient3 of the Part Load Performance Curve
   0,                         !Coefficient4 of the Part Load Performance Curve
   0,                         !Min Flow Rate while operating in variable flow capacity
   INTERMITTENT,                         !Pump Control Type
   COOLINGAVAILSCHED;                         !Pump Flow Rate Schedule Name
Pump:VariableSpeed,
   HW Circ Pump,                         !Pump Name
   HW Supply Inlet Node,                         !Inlet_Node
   HW Pump Outlet Node,                         !Outlet_Node
   autosize,                         !Rated Volumetric Flow Rate
   179352,                         !Rated Pump Head
   autosize,                         !Rated Power Consumption
   0.9,                         !Motor Efficiency
   0,                         !Fraction of Motor Inefficiencies to Fluid Stream
   0,                         !Coefficient1 of the Part Load Performance Curve
   1,                         !Coefficient2 of the Part Load Performance Curve
   0,                         !Coefficient3 of the Part Load Performance Curve
   0,                         !Coefficient4 of the Part Load Performance Curve
   0,                         !Min Flow Rate while operating in variable flow capacity
   INTERMITTENT,                         !Pump Control Type
   ;                         !Pump Flow Rate Schedule Name
Pump:VariableSpeed,
   CW Circ Pump,                         !Pump Name
   CW Supply Inlet Node,                         !Inlet_Node
   CW Pump Outlet Node,                         !Outlet_Node
   autosize,                         !Rated Volumetric Flow Rate
   179352,                         !Rated Pump Head
   autosize,                         !Rated Power Consumption
   0.9,                         !Motor Efficiency
   0,                         !Fraction of Motor Inefficiencies to Fluid Stream
   0,                         !Coefficient1 of the Part Load Performance Curve
   1,                         !Coefficient2 of the Part Load Performance Curve
   0,                         !Coefficient3 of the Part Load Performance Curve
   0,                         !Coefficient4 of the Part Load Performance Curve
   0,                         !Min Flow Rate while operating in variable flow capacity
   INTERMITTENT,                         !Pump Control Type
   COOLINGAVAILSCHED;                         !Pump Flow Rate Schedule Name
Boiler:HotWater,
   Central Boiler,                         !Name
   NaturalGas,                         !Fuel Type
   autosize,                         !Nominal Capacity
   0.8,                         !Nominal Thermal Efficiency
   BoilerEfficiency,                         !Normalized Boiler Efficiency Curve Name
   81,                         !Design Water Outlet Temperature
   autosize,                         !Design Water Flow Rate
   0.0,                         !Minimum Part Load Ratio
   1.2,                         !Maximum Part Load Ratio
   1.0,                         !Optimum Part Load Ratio
   Central Boiler Inlet Node,                         !Boiler Water Inlet Node Name
   Central Boiler Outlet Node,                         !Boiler Water Outlet Node Name
   100,                         !Water Outlet Upper Temperature Limit
   VariableFlow,                         !Boiler Flow Mode
   ,                         !Parasitic Electric Load
   ;                         !Sizing Factor
CHILLER:ELECTRIC,
   Chiller 1,                         !Chiller Name
   WaterCooled,                         !Condenser Type
   autosize,                         !Nominal Capacity
   3.2,                         !COP
   Central Chiller Inlet Node,                         !Plant_Side_Inlet_Node
   Central Chiller Outlet Node,                         !Plant_Side_Outlet_Node
   Central Chiller Condenser Inlet Node,                         !Condenser_Side_Inlet_Node
   Central Chiller Condenser Outlet Node,                         !Condenser_Side_Outlet_Node
   0,                         !Minimum Part Load Ratio
   1,                         !Maximum Part Load Ratio
   0.65,                         !Opt Part Load Ratio
   29.44,                         !Temp Design Condenser Inlet
   2.6828,                         !Temp Rise Coefficient
   6.667,                         !Temp Design Evaporator Outlet
   autosize,                         !Design Evaporator Volumetric Water Flow Rate
   autosize,                         !Design Condenser Volumetric Water Flow Rate
   0.944836,                         !Coefficient1 of the capacity ratio curve
   -0.0570088,                         !Coefficient2 of the capacity ratio curve
   -0.00185486,                         !Coefficient3 of the capacity ratio curve
   1.907846,                         !Coefficient1 of the power ratio curve
   -1.204987,                         !Coefficient2 of the power ratio curve
   0.2634623,                         !Coefficient3 of the power ratio curve
   0.03303,                         !Coefficient1 of the full load ratio curve
   0.6852,                         !Coefficient2 of the full load ratio curve
   0.2818,                         !Coefficient3 of the full load ratio curve
   5,                         !Temp Lower Limit Evaporator Outlet
   VariableFlow,                         !Chiller Flow Mode
   ,                         !Design heat recovery water flow rate
   ,                         !Heat_Recovery_Side_Inlet_Node
   ,                         !Heat_Recovery_Side_Outlet_Node
   ,                         !Sizing Factor
   ,                         !Basin Heater Capacity
   ,                         !Basin Heater Setpoint Temperature
   ;                         !Basin Heater Operating Schedule Name
COOLINGTOWER:SINGLESPEED,
   Big Tower,                         !Tower Name
   Condenser Tower Inlet Node,                         !Water Inlet Node Name
   Condenser Tower Outlet Node,                         !Water Outlet Node Name
   autosize,                         !Design Water Flow Rate
   autosize,                         !Design Air Flow Rate
   autosize,                         !Fan Power at Design Air Flow Rate
   autosize,                         !Tower UA Value at Design Air Flow Rate
   0.0,                         !Air Flow Rate in Free Convection Regime
   0.0,                         !Tower UA Value at Free Convection Air Flow Rate
   UFactorTimesAreaAndDesignWaterFlowRate,                         !Tower Performance Input Method
   ,                         !Tower Nominal Capacity
   ,                         !Tower Free Convection Capacity
   ,                         !Basin Heater Capacity
   ,                         !Basin Heater Setpoint Temperature
   ,                         !Basin Heater Operating Schedule Name
   ,                         !Evaporation Loss Mode
   ,                         !Evaporation Loss Factor
   ,                         !Drift Loss Percent
   ,                         !Blowdown Calculation Mode
   ,                         !Blowdown Concentration Ratio
   ,                         !Schedule Name for Makeup Water Usage due to Blowdown 
   ,                         !Name of Water Storage Tank for Supply
   ,                         !Outdoor Air Inlet Node Name
   ,                         !Capacity Control
   ,                         !Number of Cells
   ,                         !Cell Control
   ,                         !Cell Minimum  Water Flow Rate Fraction
   ,                         !Cell Maximum Water Flow Rate Fraction
   ;                         !Sizing Factor
Pipe:Adiabatic,
   Supply Side Bypass,                         !Name
   CW Supply Bypass Inlet Node,                         !Inlet Node Name
   CW Supply Bypass Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Supply Side Outlet Pipe,                         !Name
   Supply Side Exit Pipe Inlet Node,                         !Inlet Node Name
   CW Supply Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Demand Side Inlet Pipe,                         !Name
   CW Demand Inlet Node,                         !Inlet Node Name
   CW Demand Entrance Pipe Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Demand Side Outlet Pipe,                         !Name
   CW Demand Exit Pipe Inlet Node,                         !Inlet Node Name
   CW Demand Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Demand Side Bypass,                         !Name
   CW Demand Bypass Inlet Node,                         !Inlet Node Name
   CW Demand Bypass Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Condenser Supply Side Bypass,                         !Name
   Cond Supply Bypass Inlet Node,                         !Inlet Node Name
   Cond Supply Bypass Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Condenser Supply Outlet,                         !Name
   Condenser Supply Exit Pipe Inlet Node,                         !Inlet Node Name
   Condenser Supply Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Condenser Demand Inlet Pipe,                         !Name
   Condenser Demand Inlet Node,                         !Inlet Node Name
   Condenser Demand Inpipe Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Condenser Demand Side Bypass,                         !Name
   Cond Demand Bypass Inlet Node,                         !Inlet Node Name
   Cond Demand Bypass Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Condenser Demand Outlet Pipe,                         !Name
   Condenser Demand Exit Pipe Inlet Node,                         !Inlet Node Name
   Condenser Demand Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Heating Supply Side Bypass,                         !Name
   Heating Supply Bypass Inlet Node,                         !Inlet Node Name
   Heating Supply Bypass Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Heating Supply Outlet,                         !Name
   Heating Supply Exit Pipe Inlet Node,                         !Inlet Node Name
   HW Supply Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Reheat Inlet Pipe,                         !Name
   HW Demand Inlet Node,                         !Inlet Node Name
   HW Demand Entrance Pipe Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Reheat Outlet Pipe,                         !Name
   HW Demand Exit Pipe Inlet Node,                         !Inlet Node Name
   HW Demand Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Reheat Bypass,                         !Name
   Reheat Bypass Inlet Node,                         !Inlet Node Name
   Reheat Bypass Outlet Node;                         !Outlet Node Name
AirLoopHVAC:ZoneSplitter,
   ZoneSplitter1,                         !Splitter Name
   ZoneSplitter1_InletNode,                         !Inlet_Node
   PER-1T_P  VAV system_UnitAirInletNode,                         !Outlet_Node_1
   PER-2T_P  VAV system_UnitAirInletNode,                         !Outlet_Node_1
   PER-3T_P  VAV system_UnitAirInletNode,                         !Outlet_Node_1
   PER-4T_P  VAV system_UnitAirInletNode,                         !Outlet_Node_1
   PER-1F_P  VAV system_UnitAirInletNode,                         !Outlet_Node_1
   PER-2F_P  VAV system_UnitAirInletNode,                         !Outlet_Node_1
   PER-3F_P  VAV system_UnitAirInletNode,                         !Outlet_Node_1
   PER-4F_P  VAV system_UnitAirInletNode,                         !Outlet_Node_1
   PER-1I_P  VAV system_UnitAirInletNode,                         !Outlet_Node_1
   PER-2I_P  VAV system_UnitAirInletNode,                         !Outlet_Node_1
   PER-3I_P  VAV system_UnitAirInletNode,                         !Outlet_Node_1
   PER-4I_P  VAV system_UnitAirInletNode,                         !Outlet_Node_1
   COR-T_C  VAV system_UnitAirInletNode,                         !Outlet_Node_2
   COR-F_C  VAV system_UnitAirInletNode,                         !Outlet_Node_2
   COR-I_C  VAV system_UnitAirInletNode;                         !Outlet_Node_2
AirLoopHVAC:ZoneMixer,
   ZoneMixer1,                         !Mixer Name
   ZoneMixer1_OutletNode,                         !Outlet_Node
   PER-1T_P ZoneGroup_ZoneReturnAirNodeName,                         !Inlet_Node_1
   PER-2T_P ZoneGroup_ZoneReturnAirNodeName,                         !Inlet_Node_1
   PER-3T_P ZoneGroup_ZoneReturnAirNodeName,                         !Inlet_Node_1
   PER-4T_P ZoneGroup_ZoneReturnAirNodeName,                         !Inlet_Node_1
   PER-1F_P ZoneGroup_ZoneReturnAirNodeName,                         !Inlet_Node_1
   PER-2F_P ZoneGroup_ZoneReturnAirNodeName,                         !Inlet_Node_1
   PER-3F_P ZoneGroup_ZoneReturnAirNodeName,                         !Inlet_Node_1
   PER-4F_P ZoneGroup_ZoneReturnAirNodeName,                         !Inlet_Node_1
   PER-1I_P ZoneGroup_ZoneReturnAirNodeName,                         !Inlet_Node_1
   PER-2I_P ZoneGroup_ZoneReturnAirNodeName,                         !Inlet_Node_1
   PER-3I_P ZoneGroup_ZoneReturnAirNodeName,                         !Inlet_Node_1
   PER-4I_P ZoneGroup_ZoneReturnAirNodeName,                         !Inlet_Node_1
   COR-T_C ZoneGroup_ZoneReturnAirNodeName,                         !Inlet_Node_2
   COR-F_C ZoneGroup_ZoneReturnAirNodeName,                         !Inlet_Node_2
   COR-I_C ZoneGroup_ZoneReturnAirNodeName;                         !Inlet_Node_2
Connector:Splitter,
   CW Loop Splitter,                         !SplitterName
   CW Pump Branch,                         !Inlet Branch Name
   CW Supply Bypass Branch,                         !Outlet Branch Name 1
   Chiller Branch;                         !Outlet Branch Name 2
Connector:Splitter,
   CW Demand Splitter,                         !SplitterName
   Cooling Demand Inlet,                         !Inlet Branch Name
   Cooling Coil Branch,                         !Outlet Branch Name 1
   Demand Bypass Branch;                         !Outlet Branch Name 2
Connector:Splitter,
   Condenser Demand Splitter,                         !SplitterName
   Condenser Demand Inlet Branch,                         !Inlet Branch Name
   Chiller Condenser Branch,                         !Outlet Branch Name 1
   Condenser Demand Bypass Branch;                         !Outlet Branch Name 2
Connector:Splitter,
   Condenser Supply Splitter,                         !SplitterName
   Condenser Supply Inlet Branch,                         !Inlet Branch Name
   Condenser Supply Tower Branch,                         !Outlet Branch Name 1
   Condenser Supply Bypass Branch;                         !Outlet Branch Name 2
Connector:Splitter,
   Reheat Splitter,                         !SplitterName
   Reheat Inlet Branch,                         !Inlet Branch Name
   COR-T_C  Zone Branch,                         !Outlet Branch Name 1
   COR-F_C  Zone Branch,                         !Outlet Branch Name 1
   COR-I_C  Zone Branch,                         !Outlet Branch Name 1
   PER-1T_P Zone Branch,                         !Outlet Branch Name 2
   PER-2T_P Zone Branch,                         !Outlet Branch Name 2
   PER-3T_P Zone Branch,                         !Outlet Branch Name 2
   PER-4T_P Zone Branch,                         !Outlet Branch Name 2
   PER-1F_P Zone Branch,                         !Outlet Branch Name 2
   PER-2F_P Zone Branch,                         !Outlet Branch Name 2
   PER-3F_P Zone Branch,                         !Outlet Branch Name 2
   PER-4F_P Zone Branch,                         !Outlet Branch Name 2
   PER-1I_P Zone Branch,                         !Outlet Branch Name 2
   PER-2I_P Zone Branch,                         !Outlet Branch Name 2
   PER-3I_P Zone Branch,                         !Outlet Branch Name 2
   PER-4I_P Zone Branch,                         !Outlet Branch Name 2
   Reheat Bypass Branch;                         !Outlet Branch Name 3
Connector:Splitter,
   Heating Supply Splitter,                         !SplitterName
   Heating Supply Inlet Branch,                         !Inlet Branch Name
   Boiler Branch,                         !Outlet Branch Name 1
   Heating Supply Bypass Branch;                         !Outlet Branch Name 2
Connector:Mixer,
   CW Loop Mixer,                         !MixerName
   Cooling Supply Outlet,                         !Outlet Branch Name
   CW Supply Bypass Branch,                         !Inlet Branch Name 1
   Chiller Branch;                         !Inlet Branch Name 2
Connector:Mixer,
   CW Demand Mixer,                         !MixerName
   Cooling Demand Outlet,                         !Outlet Branch Name
   Demand Bypass Branch,                         !Inlet Branch Name 1
   Cooling Coil Branch;                         !Inlet Branch Name 2
Connector:Mixer,
   Condenser Demand Mixer,                         !MixerName
   Condenser Demand Outlet Branch,                         !Outlet Branch Name
   Chiller Condenser Branch,                         !Inlet Branch Name 1
   Condenser Demand Bypass Branch;                         !Inlet Branch Name 2
Connector:Mixer,
   Condenser Supply Mixer,                         !MixerName
   Condenser Supply Outlet Branch,                         !Outlet Branch Name
   Condenser Supply Tower Branch,                         !Inlet Branch Name 1
   Condenser Supply Bypass Branch;                         !Inlet Branch Name 2
Connector:Mixer,
   Reheat Mixer,                         !MixerName
   Reheat Outlet Branch,                         !Outlet Branch Name
   Reheat Bypass Branch,                         !Inlet Branch Name 1
   COR-T_C  Zone Branch,                         !Inlet Branch Name 2
   COR-F_C  Zone Branch,                         !Inlet Branch Name 2
   COR-I_C  Zone Branch,                         !Inlet Branch Name 2
   PER-1T_P Zone Branch,                         !Inlet Branch Name 3
   PER-2T_P Zone Branch,                         !Inlet Branch Name 3
   PER-3T_P Zone Branch,                         !Inlet Branch Name 3
   PER-4T_P Zone Branch,                         !Inlet Branch Name 3
   PER-1F_P Zone Branch,                         !Inlet Branch Name 3
   PER-2F_P Zone Branch,                         !Inlet Branch Name 3
   PER-3F_P Zone Branch,                         !Inlet Branch Name 3
   PER-4F_P Zone Branch,                         !Inlet Branch Name 3
   PER-1I_P Zone Branch,                         !Inlet Branch Name 3
   PER-2I_P Zone Branch,                         !Inlet Branch Name 3
   PER-3I_P Zone Branch,                         !Inlet Branch Name 3
   PER-4I_P Zone Branch;                         !Inlet Branch Name 3
Connector:Mixer,
   Heating Supply Mixer,                         !MixerName
   Heating Supply Outlet Branch,                         !Outlet Branch Name
   Boiler Branch,                         !Inlet Branch Name 1
   Heating Supply Bypass Branch;                         !Inlet Branch Name 2

