Schedule:Compact,
   Zone Control Type Sched,                         !Name
   Control Type,                         !ScheduleType
   Through: 3/31,                         !Complex Field #1
   For: AllDays,                         !Complex Field #2
   Until:24:00,1,                         !Complex Field #3
   Through: 9/30,                         !Complex Field #4
   For: AllDays,                         !Complex Field #5
   Until:24:00,2,                         !Complex Field #6
   Through: 12/31,                         !Complex Field #7
   For: AllDays,                         !Complex Field #8
   Until:24:00,1;                         !Complex Field #9
NodeList,
   WEST ZONE_Zone1Inlets,                      !Node List Name
   WEST ZONE_Zone1PTACAirOutletNode;                      !Node_ID_1
NodeList,
   EAST ZONE_Zone2Inlets,                      !Node List Name
   EAST ZONE_Zone2PTACAirOutletNode;                      !Node_ID_1
NodeList,
   EAST ZONE_Zone2Exhausts,                      !Node List Name
   EAST ZONE_Zone 2 Outlet Node;                      !Node_ID_1
NodeList,
   NORTH ZONE_Zone3Inlets,                      !Node List Name
   NORTH ZONE_Zone3PTACAIROutletNode;                      !Node_ID_1
NodeList,
   NORTH ZONE_Zone3Exhausts,                      !Node List Name
   NORTH ZONE_Zone 3 Outlet Node;                      !Node_ID_1
NodeList,
   EAST ZONE_zone1outllets,                      !Node List Name
   EAST ZONE_Zone 2 Outlet Node;                      !Node_ID_1
BranchList,
   Steam Demand 1 Steam Demand Side Branches,                         !Branch List Name
   Steam Demand 1 Steam Inlet Branch,                         !Branch Name 1
   NORTH ZONE_Zone3 Steam-Branch,                         !Branch Name 2
   Steam Coil Bypass Branch,                         !Branch Name 3
   Steam Demand 1 Steam Outlet Branch;                         !Branch Name 4
BranchList,
   Steam Boiler Plant Steam Supply Side Branches,                         !Branch List Name
   Steam Boiler Plant Steam Supply Inlet Branch,                         !Branch Name 1
   waterboiler,                         !Branch Name 2
   Steam Boiler Bypass Branch,                         !Branch Name 3
   Steam Boiler Plant Steam Supply Outlet Branch;                         !Branch Name 4
PlantLoop,
   Steam Boiler Plant,                         !Plant Loop Name
   Water,                         !Fluid Type
   Steam Boiler Plant Operation,                         !Plant Operation Scheme List Name
   Steam Boiler Plant Steam Supply Outlet Node,                         !Loop Temperature Setpoint Node Name
   110,                         !Maximum Loop Temperature
   10,                         !Minimum Loop Temperature
   .05,                         !Maximum Loop Volumetric Flow Rate
   0,                         !Minimum Loop Volumetric Flow Rate
   autocalculate,                         !volume of the plant loop
   Pump_VS1_InletNode,                         !Plant Side Inlet Node Name
   Steam Boiler Plant Steam Supply Outlet Node,                         !Plant Side Outlet Node Name
   Steam Boiler Plant Steam Supply Side Branches,                         !Plant Side Branch List Name
   Steam Boiler Plant Steam Supply Side Connectors,                         !Plant Side Connector List Name
   Steam Demand 1 Steam Demand Inlet Node,                         !Demand Side Inlet Node Name
   Steam Demand 1 Steam Demand Outlet Node,                         !Demand Side Outlet Nodes Name
   Steam Demand 1 Steam Demand Side Branches,                         !Demand Side Branch List Name
   Steam Demand 1 Steam Demand Side Connectors,                         !Demand Side Connector List Name
   OPTIMAL,                         !Load Distribution Scheme
   ,                         !System Availability Manager List
   ,                         !Plant Loop Demand Calculation Scheme
   ,                         !Common Pipe Simulation
   ;                         !Pressure Simulation Type
Branch,
   Steam Coil Bypass Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Steam Boiler Demand Bypass Pipe,                         !Comp1 Name
   Steam Boiler Demand Bypass Pipe Inlet Node,                         !Comp1 Inlet Node Name
   Steam Boiler Demand Bypass Pipe Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   NORTH ZONE_Zone3 Steam-Branch,                      !Branch Name
   ,                      !Maximum Branch Flow Rate
   ,                      !Pressure Drop Curve Name
   Coil:Heating:Water,                      !Comp1 Type
   NORTH ZONE_Zone3PTACHeater,                      !Comp1 Name
   NORTH ZONE_Zone3 Steam Coil Inlet Node,                      !Comp1 Inlet Node Name
   NORTH ZONE_Zone3 Steam Coil Outlet Node,                      !Comp1 Outlet Node Name
   ACTIVE;                      !Comp1 Branch Control Type
Branch,
   Steam Demand 1 Steam Inlet Branch,                         !Branch Name
   ,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Steam Demand 1 Steam Inlet Pipe,                         !Comp1 Name
   Steam Demand 1 Steam Demand Inlet Node,                         !Comp1 Inlet Node Name
   Steam Demand 1 Steam Demand Entrance Pipe Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Steam Demand 1 Steam Outlet Branch,                         !Branch Name
   ,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Steam Demand 1 Steam Outlet Pipe,                         !Comp1 Name
   Steam Demand 1 Steam Demand Exit Pipe Inlet Node,                         !Comp1 Inlet Node Name
   Steam Demand 1 Steam Demand Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Steam Boiler Bypass Branch,                         !Branch Name
   ,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Steam Boiler Bypass Pipe,                         !Comp1 Name
   Steam Boiler Bypass Pipe Inlet Node,                         !Comp1 Inlet Node Name
   Steam Boiler Bypass Pipe Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Steam Boiler Plant Steam Supply Outlet Branch,                         !Branch Name
   ,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Steam Boiler Plant Steam Supply Outlet,                         !Comp1 Name
   Steam Boiler Plant Steam Supply Exit Pipe Inlet Node,                         !Comp1 Inlet Node Name
   Steam Boiler Plant Steam Supply Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Steam Boiler Plant Steam Supply Inlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pump:VariableSpeed,                         !Comp1 Type
   Steam Boiler Plant Steam Circ Pump,                         !Comp1 Name
   Pump_VS1_InletNode,                         !Comp1 Inlet Node Name
   Pump_VS1_OutletNode,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   waterboiler,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Boiler:HotWater,                         !Comp1 Type
   Boiler_Simple1,                         !Comp1 Name
   Boiler_Simple1_BoilerWaterInletNode,                         !Comp1 Inlet Node Name
   Boiler_Simple1_BoilerWaterOutletNode,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
ConnectorList,
   Steam Demand 1 Steam Demand Side Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   Steam Demand 1 Steam Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   Steam Demand 1 Steam Mixer;                         !Name of Connector 2
ConnectorList,
   Steam Boiler Plant Steam Supply Side Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   Steam Boiler Plant Steam Supply Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   Steam Boiler Plant Steam Supply Mixer;                         !Name of Connector 2
PlantEquipmentOperationSchemes,
   Steam Boiler Plant Operation,                         !PlantOperationSchemeName
   PlantEquipmentOperation:HeatingLoad,                         !KEY--Control Scheme 1
   Steam Boiler Plant Heat Supply,                         !Control Scheme Name 1
   ON;                         !Control Scheme Schedule 1
PlantEquipmentOperation:HeatingLoad,
   Steam Boiler Plant Heat Supply,                         !Name
   0,                         !Load Range Lower Limit 1
   10000000000,                         !Load Range Upper Limit 1
   Steam Boiler Plant heating plant;                         !Priority Control Equip List Name 1
ZoneHVAC:EquipmentList,
   EAST ZONE_Zone2Equipment,                      !Name
   ZoneHVAC:PackagedTerminalAirConditioner,                      !KEY--Zone Equipment Type 1
   EAST ZONE_Zone2PTAC,                      !Type Name 1
   1,                      !Cooling Priority 1
   2;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   WEST ZONE_Zone1Equipment,                      !Name
   ZoneHVAC:PackagedTerminalAirConditioner,                      !KEY--Zone Equipment Type 1
   WEST ZONE_Zone1PTAC,                      !Type Name 1
   1,                      !Cooling Priority 1
   2;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   NORTH ZONE_Zone3Equipment,                      !Name
   ZoneHVAC:PackagedTerminalAirConditioner,                      !KEY--Zone Equipment Type 1
   NORTH ZONE_Zone3PTAC,                      !Type Name 1
   1,                      !Cooling Priority 1
   2;                      !Heating Priority 1
PlantEquipmentList,
   Steam Boiler Plant heating plant,                         !Equip List Name
   Boiler:HotWater,                         !KEY--Plant Equip 1
   Boiler_Simple1;                         !Equip Name 1
SetpointManager:Scheduled,
   Steam Boiler Plant Steam Temp Manager,                         !Name
   Temperature,                         !Control variable
   Steam-Loop-Temp-Schedule,                         !Schedule Name
   Steam Boiler Plant Steam Supply Outlet Node;                         !Name of the set point Node or Node List
OutdoorAir:NodeList,
   WEST ZONE_Zone1PTACOAInNode,                         !1st Node name or node list name
   EAST ZONE_Zone2PTACOAInNode,                         !2nd Node name or node list name
   NORTH ZONE_Zone3PTACOAInNode;                         !3rd Node name or node list name
ThermostatSetpoint:SingleHeating,
   Heating Setpoint,                         !Name
   Heating Setpoints;                         !Setpoint Temperature SCHEDULE Name
ThermostatSetpoint:SingleCooling,
   Cooling Setpoint,                         !Name
   Cooling Setpoints;                         !Setpoint Temperature SCHEDULE Name
ThermostatSetpoint:DualSetpoint,
   DualSetPoint,                         !Name
   Heating Setpoints,                         !Heating Setpoint Temperature SCHEDULE Name
   Cooling Setpoints;                         !Cooling Setpoint Temperature SCHEDULE Name
SIZING:PARAMETERS,
   1.2,                         !Cooling Sizing Factor
   1.2,                         !Heating sizing factor
   ;                         !time steps in averaging window
Sizing:Plant,
   Steam Boiler Plant,                         !name of a PLANT LOOP or CONDENSER LOOP object
   Heating,                         !loop type
   100,                         !Design loop exit temperature
   25;                         !Design loop delta T
Sizing:Zone,
   WEST ZONE,                         !Name of a zone
   12,                         !Zone cooling design supply air temperature
   50,                         !Zone heating design supply air temperature
   0.008,                         !Zone cooling design supply air humidity ratio
   0.008,                         !Zone heating design supply air humidity ratio
   flow/person,                         !outside air method
   0.00944,                         !outside air flow per person
   0,                         !outside air flow per zone area
   0,                         !outside air flow per zone
   0,                         !zone heating sizing factor
   0,                         !zone cooling sizing factor
   designday,                         !cooling design air flow method
   0,                         !cooling design air flow rate
   ,                         !cooling min air flow per zone area
   ,                         !cooling min air flow
   ,                         !cooling min air flow fraction
   designday,                         !heating design air flow method
   0,                         !heating design air flow rate
   ,                         !heating max air flow per zone area
   ,                         !heating max air flow
   ;                         !heating max air flow fraction
Sizing:Zone,
   EAST ZONE,                         !Name of a zone
   12,                         !Zone cooling design supply air temperature
   50,                         !Zone heating design supply air temperature
   0.008,                         !Zone cooling design supply air humidity ratio
   0.008,                         !Zone heating design supply air humidity ratio
   flow/person,                         !outside air method
   0.00944,                         !outside air flow per person
   0,                         !outside air flow per zone area
   0,                         !outside air flow per zone
   0,                         !zone heating sizing factor
   0,                         !zone cooling sizing factor
   designday,                         !cooling design air flow method
   0,                         !cooling design air flow rate
   ,                         !cooling min air flow per zone area
   ,                         !cooling min air flow
   ,                         !cooling min air flow fraction
   designday,                         !heating design air flow method
   0,                         !heating design air flow rate
   ,                         !heating max air flow per zone area
   ,                         !heating max air flow
   ;                         !heating max air flow fraction
Sizing:Zone,
   NORTH ZONE,                         !Name of a zone
   12,                         !Zone cooling design supply air temperature
   50,                         !Zone heating design supply air temperature
   0.008,                         !Zone cooling design supply air humidity ratio
   0.008,                         !Zone heating design supply air humidity ratio
   flow/person,                         !outside air method
   0.00944,                         !outside air flow per person
   0,                         !outside air flow per zone area
   0,                         !outside air flow per zone
   0,                         !zone heating sizing factor
   0,                         !zone cooling sizing factor
   designday,                         !cooling design air flow method
   0,                         !cooling design air flow rate
   ,                         !cooling min air flow per zone area
   ,                         !cooling min air flow
   ,                         !cooling min air flow fraction
   designday,                         !heating design air flow method
   0,                         !heating design air flow rate
   ,                         !heating max air flow per zone area
   ,                         !heating max air flow
   ;                         !heating max air flow fraction
ZoneControl:Thermostat,
   ZoneControl_T1,                         !Thermostat Name
   WEST ZONE,                         !Zone Name
   Zone Control Type Sched,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:SingleHeating,                         !Control Type #1
   Heating Setpoint,                         !Control Type Name #1
   ThermostatSetpoint:SingleCooling,                         !Control Type #2
   Cooling Setpoint;                         !Control Type Name #2
ZoneControl:Thermostat,
   Zone 2 Thermostat,                         !Thermostat Name
   EAST ZONE,                         !Zone Name
   Zone Control Type Sched,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:SingleHeating,                         !Control Type #1
   Heating Setpoint,                         !Control Type Name #1
   ThermostatSetpoint:SingleCooling,                         !Control Type #2
   Cooling Setpoint;                         !Control Type Name #2
ZoneControl:Thermostat,
   Zone 3 Thermostat,                         !Thermostat Name
   NORTH ZONE,                         !Zone Name
   Zone Control Type Sched,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:SingleHeating,                         !Control Type #1
   Heating Setpoint,                         !Control Type Name #1
   ThermostatSetpoint:SingleCooling,                         !Control Type #2
   Cooling Setpoint;                         !Control Type Name #2
CURVE:QUADRATIC,
   HPACCoolCapFFF,                         !Name
   .8,                         !Coeff1 Constant
   .2,                         !Coeff2 x
   0,                         !Coeff3 x**2
   .5,                         !minimum value of x
   1.5,                         !maximum value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Dimensionless,                         !Input Unit Type for X
   Dimensionless;                         !Output Unit Type
CURVE:QUADRATIC,
   HPACEIRFFF,                         !Name
   1.1552,                         !Coeff1 Constant
   -.1808,                         !Coeff2 x
   .0256,                         !Coeff3 x**2
   .5,                         !minimum value of x
   1.5,                         !maximum value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Dimensionless,                         !Input Unit Type for X
   Dimensionless;                         !Output Unit Type
CURVE:QUADRATIC,
   HPACPLFFPLR,                         !Name
   .85,                         !Coeff1 Constant
   .15,                         !Coeff2 x
   0,                         !Coeff3 x**2
   0,                         !minimum value of x
   1,                         !maximum value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Dimensionless,                         !Input Unit Type for X
   Dimensionless;                         !Output Unit Type
CURVE:QUADRATIC,
   HPACHeatEIRFFF,                         !Name
   1.3824,                         !Coeff1 Constant
   -.4336,                         !Coeff2 x
   .0512,                         !Coeff3 x**2
   0,                         !minimum value of x
   1,                         !maximum value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Dimensionless,                         !Input Unit Type for X
   Dimensionless;                         !Output Unit Type
CURVE:QUADRATIC,
   HPACCOOLPLFFPLR,                         !Name
   .75,                         !Coeff1 Constant
   .25,                         !Coeff2 x
   0,                         !Coeff3 x**2
   0,                         !minimum value of x
   1,                         !maximum value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Dimensionless,                         !Input Unit Type for X
   Dimensionless;                         !Output Unit Type
Curve:Cubic,
   HPACHeatCapFT,                         !Name 
   .758746,                         !Coefficient1 Constant
   .027626,                         !Coefficient2 x 
   .000148716,                         !Coefficient3 x**2
   .0000034992,                         !Coefficient4 x**3
   -20,                         !Minimum Value of x 
   20,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Dimensionless;                         !Output Unit Type
Curve:Cubic,
   HPACHeatCapFFF,                         !Name 
   .84,                         !Coefficient1 Constant
   .16,                         !Coefficient2 x 
   0,                         !Coefficient3 x**2
   0,                         !Coefficient4 x**3
   .5,                         !Minimum Value of x 
   1.5,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Dimensionless,                         !Input Unit Type for X
   Dimensionless;                         !Output Unit Type
Curve:Cubic,
   HPACHeatEIRFT,                         !Name 
   1.19248,                         !Coefficient1 Constant
   -.0300438,                         !Coefficient2 x 
   .00103745,                         !Coefficient3 x**2
   -.000023328,                         !Coefficient4 x**3
   -20,                         !Minimum Value of x 
   20,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Dimensionless;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HPACCoolCapFT,                         !Name
   .942587793,                         !Coeff1 Constant
   .009543347,                         !Coeff2 x
   .00068377,                         !Coeff3 x**2
   -.011042676,                         !Coeff4 y
   .000005249,                         !Coeff5 y**2
   -.00000972,                         !Coeff6 x*y
   12.77778,                         !minimum value of x
   23.88889,                         !maximum value of x
   18,                         !minimum value of y
   46.11111,                         !maximum value of y
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HPACEIRFT,                         !Name
   .342414409,                         !Coeff1 Constant
   .034885008,                         !Coeff2 x
   -.0006237,                         !Coeff3 x**2
   .004977216,                         !Coeff4 y
   .000437951,                         !Coeff5 y**2
   -.000728028,                         !Coeff6 x*y
   12.77778,                         !minimum value of x
   23.88889,                         !maximum value of x
   18,                         !minimum value of y
   46.11111,                         !maximum value of y
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
CURVE:QUADRATIC,
   BoilerEfficiency,                         !Name
   1,                         !Coeff1 Constant
   0,                         !Coeff2 x
   0,                         !Coeff3 x**2
   0,                         !minimum value of x
   1,                         !maximum value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Dimensionless,                         !Input Unit Type for X
   Dimensionless;                         !Output Unit Type
Pipe:Adiabatic,
   Steam Boiler Demand Bypass Pipe,                         !Name
   Steam Boiler Demand Bypass Pipe Inlet Node,                         !Inlet Node Name
   Steam Boiler Demand Bypass Pipe Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Steam Boiler Bypass Pipe,                         !Name
   Steam Boiler Bypass Pipe Inlet Node,                         !Inlet Node Name
   Steam Boiler Bypass Pipe Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Steam Demand 1 Steam Outlet Pipe,                         !Name
   Steam Demand 1 Steam Demand Exit Pipe Inlet Node,                         !Inlet Node Name
   Steam Demand 1 Steam Demand Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Steam Boiler Plant Steam Supply Outlet,                         !Name
   Steam Boiler Plant Steam Supply Exit Pipe Inlet Node,                         !Inlet Node Name
   Steam Boiler Plant Steam Supply Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Steam Demand 1 Steam Inlet Pipe,                         !Name
   Steam Demand 1 Steam Demand Inlet Node,                         !Inlet Node Name
   Steam Demand 1 Steam Demand Entrance Pipe Outlet Node;                         !Outlet Node Name
Pump:VariableSpeed,
   Steam Boiler Plant Steam Circ Pump,                         !Pump Name
   Pump_VS1_InletNode,                         !Inlet_Node
   Pump_VS1_OutletNode,                         !Outlet_Node
   .05,                         !Rated Volumetric Flow Rate
   ,                         !Rated Pump Head
   autosize,                         !Rated Power Consumption
   ,                         !Motor Efficiency
   0,                         !Fraction of Motor Inefficiencies to Fluid Stream
   0,                         !Coefficient1 of the Part Load Performance Curve
   1,                         !Coefficient2 of the Part Load Performance Curve
   0,                         !Coefficient3 of the Part Load Performance Curve
   0,                         !Coefficient4 of the Part Load Performance Curve
   0,                         !Min Flow Rate while operating in variable flow capacity
   CONTINUOUS,                         !Pump Control Type
   ;                         !Pump Flow Rate Schedule Name
ZoneHVAC:EquipmentConnections,
   WEST ZONE,                      !Zone Name
   WEST ZONE_Zone1Equipment,                      !List Name: Zone Equipment
   WEST ZONE_Zone1PTACAirOutletNode,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   WEST ZONE_Zone 1 Node,                      !Zone Air Node Name
   WEST ZONE_Zone 1 Outlet Node;                      !Zone Return Air Node Name
ZoneHVAC:PackagedTerminalAirConditioner,
   WEST ZONE_Zone1PTAC,                      !Air conditioner name
   FanAndCoilAvailSched,                      !Availability schedule name
   WEST ZONE_Zone 1 Outlet Node,                      !Air inlet node name
   WEST ZONE_Zone1PTACAirOutletNode,                      !Air outlet node name
   WEST ZONE_Zone1PTACOAMixer,                      !Outside air mixer name
   .5,                      !Supply air volumetric flow rate during cooling operation
   .6,                      !Supply air volumetric flow rate during heating operation
   ,                      !Supply air volumetric flow rate when no cooling or heating is needed
   .028,                      !Outside air volumetric flow rate during cooling operation
   .0233,                      !Outside air volumetric flow rate during heating operation
   .0186,                      !Outside air volumetric flow rate when no cooling or heating is needed
   FAN:ConstantVolume,                      !Supply air fan type
   WEST ZONE_Zone1PTACFan,                      !Supply air fan name
   COIL:Heating:Electric,                      !Heating coil type
   WEST ZONE_Zone1PTACHeater,                      !Heating coil name
   Coil:Cooling:DX:SingleSpeed,                      !Cooling coil type
   WEST ZONE_Zone1PTACDXCoolCoil,                      !Cooling coil name
   blowthrough,                      !Fan placement
   ConstantFanSch;                      !Supply air fan operating mode schedule name
Fan:ConstantVolume,
   WEST ZONE_Zone1PTACFan,                      !Fan Name
   FanAndCoilAvailSched,                      !Available Schedule
   .5,                      !Fan Total Efficiency
   75,                      !Delta Pressure
   .6,                      !Max Flow Rate
   .9,                      !Motor Efficiency
   1,                      !Motor In Airstream Fraction
   WEST ZONE_Zone1PTACOAMixerOutletNode,                      !Fan_Inlet_Node
   WEST ZONE_PTAC_FCVCHE1_FanOutletNode,                      !Fan_Outlet_Node
   General;                      !End-Use Subcategory
Coil:Cooling:DX:SingleSpeed,
   WEST ZONE_Zone1PTACDXCoolCoil,                      !Name
   CoolingCoilAvailSched,                      !Availability Schedule Name
   8750,                      !Rated Total Cooling Capacity
   .75,                      !Rated Sensible Heat Ratio
   3,                      !Rated COP
   .5,                      !Rated Air Flow Rate
   ,                      !Rated Evaporator Fan Power Per Volume Flow Rate
   WEST ZONE_PTAC_FCVCHE1_FanOutletNode,                      !Air Inlet Node Name
   WEST ZONE_PTAC_FCVCHE1_CoolingAirOutletNodeName,                      !Air Outlet Node Name
   HPACCoolCapFT,                      !Total Cooling Capacity Function of Temperature Curve Name
   HPACCoolCapFFF,                      !Total Cooling Capacity Function of Flow Fraction Curve Name
   HPACEIRFT,                      !Energy Input Ratio Function of Temperature Curve Name
   HPACEIRFFF,                      !Energy Input Ratio Function of Flow Fraction Curve Name
   HPACPLFFPLR,                      !Part Load Fraction Correlation Curve Name
   ,                      !Nominal Time for Condensate Removal to Begin
   ,                      !Ratio of Initial Moisture Evaporation Rate and Steady State Latent Capacity
   ,                      !Maximum Cycling Rate
   ,                      !Latent Capacity Time Constant 
   ,                      !Condenser Air Inlet Node Name
   ,                      !Condenser Type
   ,                      !Evaporative Condenser Effectiveness
   ,                      !Evaporative Condenser Air Flow Rate
   ,                      !Evaporative Condenser Pump Rated Power Consumption
   ,                      !Crankcase Heater Capacity
   ,                      !Maximum Outdoor Dry-Bulb Temperature for Crankcase Heater Operation
   ,                      !Supply Water Storage Tank Name
   ,                      !Condensate Collection Water Storage Tank Name
   ,                      !Basin Heater Capacity 
   ,                      !Basin Heater Setpoint Temperature
   ;                      !Basin Heater Operating Schedule Name
COIL:Heating:Electric,
   WEST ZONE_Zone1PTACHeater,                      !Coil Name
   HeatingCoilAvailSched,                      !Available Schedule
   1,                      !Efficiency of the Coil
   autosize,                      !Nominal Capacity of the Coil
   WEST ZONE_PTAC_FCVCHE1_CoolingAirOutletNodeName,                      !Coil_Air_Inlet_Node
   WEST ZONE_Zone1PTACAirOutletNode,                      !Coil_Air_Outlet_Node
   ;                      !Coil_Temp_Setpoint_Node
OutdoorAir:Mixer,
   WEST ZONE_Zone1PTACOAMixer,                      !Name
   WEST ZONE_Zone1PTACOAMixerOutletNode,                      !Mixed_Air_Node
   WEST ZONE_Zone1PTACOAInNode,                      !Outside_Air_Stream_Node
   WEST ZONE_Zone1PTACExhNode,                      !Relief_Air_Stream_Node
   WEST ZONE_Zone 1 Outlet Node;                      !Return_Air_Stream_Node
ZoneHVAC:PackagedTerminalAirConditioner,
   EAST ZONE_Zone2PTAC,                      !Air conditioner name
   FanAndCoilAvailSched,                      !Availability schedule name
   EAST ZONE_Zone 2 Outlet Node,                      !Air inlet node name
   EAST ZONE_Zone2PTACAirOutletNode,                      !Air outlet node name
   EAST ZONE_Zone2PTACOAMixer,                      !Outside air mixer name
   autosize,                      !Supply air volumetric flow rate during cooling operation
   autosize,                      !Supply air volumetric flow rate during heating operation
   autosize,                      !Supply air volumetric flow rate when no cooling or heating is needed
   autosize,                      !Outside air volumetric flow rate during cooling operation
   autosize,                      !Outside air volumetric flow rate during heating operation
   autosize,                      !Outside air volumetric flow rate when no cooling or heating is needed
   Fan:OnOff,                      !Supply air fan type
   EAST ZONE_Zone2PTACFan,                      !Supply air fan name
   COIL:Heating:Electric,                      !Heating coil type
   EAST ZONE_Zone2PTACHeater,                      !Heating coil name
   Coil:Cooling:DX:SingleSpeed,                      !Cooling coil type
   EAST ZONE_Zone2PTACDXCoolCoil,                      !Cooling coil name
   blowthrough,                      !Fan placement
   ConstantFanSch;                      !Supply air fan operating mode schedule name
FAN:OnOff,
   EAST ZONE_Zone2PTACFan,                      !Fan Name
   FanAndCoilAvailSched,                      !Available Schedule
   .5,                      !Fan Total Efficiency
   75,                      !Delta Pressure
   autosize,                      !Max Flow Rate
   .9,                      !Motor Efficiency
   1,                      !Motor In Airstream Fraction
   EAST ZONE_Zone2PTACOAMixerOutletNode,                      !Fan_Inlet_Node
   EAST ZONE_PTAC_FOFCHE1_FanOutletNode,                      !Fan_Outlet_Node
   General;                      !End-Use Subcategory
Coil:Cooling:DX:SingleSpeed,
   EAST ZONE_Zone2PTACDXCoolCoil,                      !Name
   CoolingCoilAvailSched,                      !Availability Schedule Name
   autosize,                      !Rated Total Cooling Capacity
   autosize,                      !Rated Sensible Heat Ratio
   3,                      !Rated COP
   autosize,                      !Rated Air Flow Rate
   ,                      !Rated Evaporator Fan Power Per Volume Flow Rate
   EAST ZONE_PTAC_FOFCHE1_FanOutletNode,                      !Air Inlet Node Name
   EAST ZONE_PTAC_FOFCHE1_CoolingAirOutletNodeName,                      !Air Outlet Node Name
   HPACCoolCapFT,                      !Total Cooling Capacity Function of Temperature Curve Name
   HPACCoolCapFFF,                      !Total Cooling Capacity Function of Flow Fraction Curve Name
   HPACEIRFT,                      !Energy Input Ratio Function of Temperature Curve Name
   HPACEIRFFF,                      !Energy Input Ratio Function of Flow Fraction Curve Name
   HPACPLFFPLR,                      !Part Load Fraction Correlation Curve Name
   ,                      !Nominal Time for Condensate Removal to Begin
   ,                      !Ratio of Initial Moisture Evaporation Rate and Steady State Latent Capacity
   ,                      !Maximum Cycling Rate
   ,                      !Latent Capacity Time Constant 
   ,                      !Condenser Air Inlet Node Name
   ,                      !Condenser Type
   ,                      !Evaporative Condenser Effectiveness
   ,                      !Evaporative Condenser Air Flow Rate
   ,                      !Evaporative Condenser Pump Rated Power Consumption
   ,                      !Crankcase Heater Capacity
   ,                      !Maximum Outdoor Dry-Bulb Temperature for Crankcase Heater Operation
   ,                      !Supply Water Storage Tank Name
   ,                      !Condensate Collection Water Storage Tank Name
   ,                      !Basin Heater Capacity 
   ,                      !Basin Heater Setpoint Temperature
   ;                      !Basin Heater Operating Schedule Name
COIL:Heating:Electric,
   EAST ZONE_Zone2PTACHeater,                      !Coil Name
   HeatingCoilAvailSched,                      !Available Schedule
   1,                      !Efficiency of the Coil
   autosize,                      !Nominal Capacity of the Coil
   EAST ZONE_PTAC_FOFCHE1_CoolingAirOutletNodeName,                      !Coil_Air_Inlet_Node
   EAST ZONE_Zone2PTACAirOutletNode,                      !Coil_Air_Outlet_Node
   ;                      !Coil_Temp_Setpoint_Node
OutdoorAir:Mixer,
   EAST ZONE_Zone2PTACOAMixer,                      !Name
   EAST ZONE_Zone2PTACOAMixerOutletNode,                      !Mixed_Air_Node
   EAST ZONE_Zone2PTACOAInNode,                      !Outside_Air_Stream_Node
   EAST ZONE_Zone2PTACExhNode,                      !Relief_Air_Stream_Node
   EAST ZONE_Zone 2 Outlet Node;                      !Return_Air_Stream_Node
ZoneHVAC:PackagedTerminalAirConditioner,
   NORTH ZONE_Zone3PTAC,                      !Air conditioner name
   FanAndCoilAvailSched,                      !Availability schedule name
   NORTH ZONE_Zone 3 Outlet Node,                      !Air inlet node name
   NORTH ZONE_Zone3PTACAIROutletNode,                      !Air outlet node name
   NORTH ZONE_Zone3PTACOAMixer,                      !Outside air mixer name
   autosize,                      !Supply air volumetric flow rate during cooling operation
   autosize,                      !Supply air volumetric flow rate during heating operation
   autosize,                      !Supply air volumetric flow rate when no cooling or heating is needed
   autosize,                      !Outside air volumetric flow rate during cooling operation
   autosize,                      !Outside air volumetric flow rate during heating operation
   autosize,                      !Outside air volumetric flow rate when no cooling or heating is needed
   Fan:OnOff,                      !Supply air fan type
   NORTH ZONE_Zone3PTACFan,                      !Supply air fan name
   COIL:Heating:Water,                      !Heating coil type
   NORTH ZONE_Zone3PTACHeater,                      !Heating coil name
   Coil:Cooling:DX:SingleSpeed,                      !Cooling coil type
   NORTH ZONE_Zone3PTACDXCoolCoil,                      !Cooling coil name
   blowthrough,                      !Fan placement
   AlternateFanOperationSch;                      !Supply air fan operating mode schedule name
FAN:OnOFF,
   NORTH ZONE_Zone3PTACFan,                      !Fan Name
   FanAndCoilAvailSched,                      !Available Schedule
   .5,                      !Fan Total Efficiency
   75,                      !Delta Pressure
   autosize,                      !Max Flow Rate
   .9,                      !Motor Efficiency
   1,                      !Motor In Airstream Fraction
   NORTH ZONE_Zone3PTACOAMixerOutletNode,                      !Fan_Inlet_Node
   NORTH ZONE_Zone3_FanOutletNode,                      !Fan_Outlet_Node
   General;                      !End-Use Subcategory
Coil:Cooling:DX:SingleSpeed,
   NORTH ZONE_Zone3PTACDXCoolCoil,                      !Name
   CoolingCoilAvailSched,                      !Availability Schedule Name
   autosize,                      !Rated Total Cooling Capacity
   autosize,                      !Rated Sensible Heat Ratio
   3,                      !Rated COP
   autosize,                      !Rated Air Flow Rate
   ,                      !Rated Evaporator Fan Power Per Volume Flow Rate
   NORTH ZONE_Zone3_FanOutletNode,                      !Air Inlet Node Name
   NORTH ZONE_Zone3PTACCoolCoilOutletNode,                      !Air Outlet Node Name
   HPACCoolCapFT,                      !Total Cooling Capacity Function of Temperature Curve Name
   HPACCoolCapFFF,                      !Total Cooling Capacity Function of Flow Fraction Curve Name
   HPACEIRFT,                      !Energy Input Ratio Function of Temperature Curve Name
   HPACEIRFFF,                      !Energy Input Ratio Function of Flow Fraction Curve Name
   HPACPLFFPLR,                      !Part Load Fraction Correlation Curve Name
   ,                      !Nominal Time for Condensate Removal to Begin
   ,                      !Ratio of Initial Moisture Evaporation Rate and Steady State Latent Capacity
   ,                      !Maximum Cycling Rate
   ,                      !Latent Capacity Time Constant 
   ,                      !Condenser Air Inlet Node Name
   ,                      !Condenser Type
   ,                      !Evaporative Condenser Effectiveness
   ,                      !Evaporative Condenser Air Flow Rate
   ,                      !Evaporative Condenser Pump Rated Power Consumption
   ,                      !Crankcase Heater Capacity
   ,                      !Maximum Outdoor Dry-Bulb Temperature for Crankcase Heater Operation
   ,                      !Supply Water Storage Tank Name
   ,                      !Condensate Collection Water Storage Tank Name
   ,                      !Basin Heater Capacity 
   ,                      !Basin Heater Setpoint Temperature
   ;                      !Basin Heater Operating Schedule Name
COIL:Heating:Water,
   NORTH ZONE_Zone3PTACHeater,                      !Coil Name
   HeatingCoilAvailSched,                      !Available Schedule
   ,                      !UA of the Coil
   .05,                      !Max Water Flow Rate of Coil
   NORTH ZONE_Zone3 Steam Coil Inlet Node,                      !Coil_Water_Inlet_Node
   NORTH ZONE_Zone3 Steam Coil Outlet Node,                      !Coil_Water_Outlet_Node
   NORTH ZONE_Zone3PTACCoolCoilOutletNode,                      !Coil_Air_Inlet_Node
   NORTH ZONE_Zone3PTACAIROutletNode,                      !Coil_Air_Outlet_Node
   UFactorTimesAreaAndDesignWaterFlowRate,                      !Coil Performance Input Method
   autosize,                      !Nominal Capacity
   82.2,                      !Design Inlet Water Temperature
   16.6,                      !Design Inlet Air Temperature
   71.1,                      !Design Outlet Water Temperature
   32.2,                      !Design Outlet Air Temperature
   0.5;                      !Rated Ratio for Air and Water Convection
OutdoorAir:Mixer,
   NORTH ZONE_Zone3PTACOAMixer,                      !Name
   NORTH ZONE_Zone3PTACOAMixerOutletNode,                      !Mixed_Air_Node
   NORTH ZONE_Zone3PTACOAInNode,                      !Outside_Air_Stream_Node
   NORTH ZONE_Zone3PTACExhNode,                      !Relief_Air_Stream_Node
   NORTH ZONE_Zone 3 Outlet Node;                      !Return_Air_Stream_Node
ZoneHVAC:EquipmentConnections,
   EAST ZONE,                      !Zone Name
   EAST ZONE_Zone2Equipment,                      !List Name: Zone Equipment
   EAST ZONE_Zone2PTACAirOutletNode,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   EAST ZONE_Zone 2 Node,                      !Zone Air Node Name
   EAST ZONE_Zone 2 Outlet Node;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   NORTH ZONE,                      !Zone Name
   NORTH ZONE_Zone3Equipment,                      !List Name: Zone Equipment
   NORTH ZONE_Zone3PTACAIROutletNode,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   NORTH ZONE_Zone 3 Node,                      !Zone Air Node Name
   NORTH ZONE_Zone 3 Outlet Node;                      !Zone Return Air Node Name
Boiler:HotWater,
   Boiler_Simple1,                         !Name
   Electricity,                         !Fuel Type
   autosize,                         !Nominal Capacity
   0.8,                         !Nominal Thermal Efficiency
   BoilerEfficiency,                         !Normalized Boiler Efficiency Curve Name
   ,                         !Design Water Outlet Temperature
   ,                         !Design Water Flow Rate
   0.0,                         !Minimum Part Load Ratio
   1.0,                         !Maximum Part Load Ratio
   1.0,                         !Optimum Part Load Ratio
   Boiler_Simple1_BoilerWaterInletNode,                         !Boiler Water Inlet Node Name
   Boiler_Simple1_BoilerWaterOutletNode,                         !Boiler Water Outlet Node Name
   99.9,                         !Water Outlet Upper Temperature Limit
   ,                         !Boiler Flow Mode
   ,                         !Parasitic Electric Load
   1.0;                         !Sizing Factor
Connector:Splitter,
   Steam Demand 1 Steam Splitter,                         !SplitterName
   Steam Demand 1 Steam Inlet Branch,                         !Inlet Branch Name
   NORTH ZONE_Zone3 Steam-Branch,                         !Outlet Branch Name 1
   Steam Coil Bypass Branch;                         !Outlet Branch Name 2
Connector:Splitter,
   Steam Boiler Plant Steam Supply Splitter,                         !SplitterName
   Steam Boiler Plant Steam Supply Inlet Branch,                         !Inlet Branch Name
   waterboiler,                         !Outlet Branch Name 1
   Steam Boiler Bypass Branch;                         !Outlet Branch Name 2
Connector:Mixer,
   Steam Demand 1 Steam Mixer,                         !MixerName
   Steam Demand 1 Steam Outlet Branch,                         !Outlet Branch Name
   NORTH ZONE_Zone3 Steam-Branch,                         !Inlet Branch Name 1
   Steam Coil Bypass Branch;                         !Inlet Branch Name 2
Connector:Mixer,
   Steam Boiler Plant Steam Supply Mixer,                         !MixerName
   Steam Boiler Plant Steam Supply Outlet Branch,                         !Outlet Branch Name
   waterboiler,                         !Inlet Branch Name 1
   Steam Boiler Bypass Branch;                         !Inlet Branch Name 2

