NodeList,
   WEST ZONE_OutsideAirInletNodes,                      !Node List Name
   WEST ZONE_Zone1PTHPOAInNode,                      !Node_ID_1
   WEST ZONE_Zone2PTHPOAInNode,                      !Node_ID_2
   WEST ZONE_Zone2PTHPOAInNode;                      !Node_ID_3
NodeList,
   WEST ZONE_Zone1Inlets,                      !Node List Name
   WEST ZONE_Zone1PTHPAirOutletNode;                      !Node_ID_1
NodeList,
   EAST ZONE_Zone2Inlets,                      !Node List Name
   EAST ZONE_Zone2PTHPAirOutletNode;                      !Node_ID_1
NodeList,
   NORTH ZONE_Zone3Inlets,                      !Node List Name
   NORTH ZONE_Zone3PTHPAirOutletNode;                      !Node_ID_1
NodeList,
   WEST ZONE_Zone1Exhausts,                      !Node List Name
   WEST ZONE_Zone1PTHPAirInletNode;                      !Node_ID_1
NodeList,
   EAST ZONE_Zone2Exhausts,                      !Node List Name
   EAST ZONE_Zone2PTHPAirInletNode;                      !Node_ID_1
NodeList,
   NORTH ZONE_Zone3Exhausts,                      !Node List Name
   NORTH ZONE_Zone3PTHPAirInletNode;                      !Node_ID_1
ZoneHVAC:EquipmentList,
   WEST ZONE_Zone1Equipment,                      !Name
   ZoneHVAC:PackagedTerminalHeatPump,                      !KEY--Zone Equipment Type 1
   WEST ZONE_Zone1PTHP,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   EAST ZONE_Zone2Equipment,                      !Name
   ZoneHVAC:PackagedTerminalHeatPump,                      !KEY--Zone Equipment Type 1
   EAST ZONE_Zone2PTHP,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
ZoneHVAC:EquipmentList,
   NORTH ZONE_Zone3Equipment,                      !Name
   ZoneHVAC:PackagedTerminalHeatPump,                      !KEY--Zone Equipment Type 1
   NORTH ZONE_Zone3PTHP,                      !Type Name 1
   1,                      !Cooling Priority 1
   1;                      !Heating Priority 1
OutdoorAir:NodeList,
   WEST ZONE_Zone1PTHPOAInNode,                         !1st Node name or node list name
   EAST ZONE_Zone2PTHPOAInNode,                         !2nd Node name or node list name
   NORTH ZONE_Zone3PTHPOAInNode;                         !3rd Node name or node list name
ThermostatSetpoint:SingleHeating,
   Heating Setpoint,                         !Name
   Heating Setpoints;                         !Setpoint Temperature SCHEDULE Name
ThermostatSetpoint:SingleCooling,
   Cooling Setpoint,                         !Name
   Cooling Setpoints;                         !Setpoint Temperature SCHEDULE Name
ThermostatSetpoint:DualSetpoint,
   DualSetPoint,                         !Name
   Heating Setpoints,                         !Heating Setpoint Temperature SCHEDULE Name
   Cooling Setpoints;                         !Cooling Setpoint Temperature SCHEDULE Name
SIZING:PARAMETERS,
   1.2,                         !Cooling Sizing Factor
   1.2,                         !Heating sizing factor
   ;                         !time steps in averaging window
Sizing:Plant,
   Hot Water Loop,                         !name of a PLANT LOOP or CONDENSER LOOP object
   Heating,                         !loop type
   82,                         !Design loop exit temperature
   11;                         !Design loop delta T
Sizing:Zone,
   WEST ZONE,                         !Name of a zone
   12,                         !Zone cooling design supply air temperature
   50,                         !Zone heating design supply air temperature
   0.008,                         !Zone cooling design supply air humidity ratio
   0.008,                         !Zone heating design supply air humidity ratio
   flow/person,                         !outside air method
   0.00944,                         !outside air flow per person
   ,                         !outside air flow per zone area
   ,                         !outside air flow per zone
   ,                         !zone heating sizing factor
   ,                         !zone cooling sizing factor
   DesignDay,                         !cooling design air flow method
   ,                         !cooling design air flow rate
   ,                         !cooling min air flow per zone area
   0,                         !cooling min air flow
   0,                         !cooling min air flow fraction
   DesignDay,                         !heating design air flow method
   ,                         !heating design air flow rate
   ,                         !heating max air flow per zone area
   ,                         !heating max air flow
   ;                         !heating max air flow fraction
Sizing:Zone,
   EAST ZONE,                         !Name of a zone
   12,                         !Zone cooling design supply air temperature
   50,                         !Zone heating design supply air temperature
   0.008,                         !Zone cooling design supply air humidity ratio
   0.008,                         !Zone heating design supply air humidity ratio
   flow/person,                         !outside air method
   0.00944,                         !outside air flow per person
   ,                         !outside air flow per zone area
   ,                         !outside air flow per zone
   ,                         !zone heating sizing factor
   ,                         !zone cooling sizing factor
   DesignDay,                         !cooling design air flow method
   ,                         !cooling design air flow rate
   ,                         !cooling min air flow per zone area
   ,                         !cooling min air flow
   ,                         !cooling min air flow fraction
   DesignDay,                         !heating design air flow method
   ,                         !heating design air flow rate
   ,                         !heating max air flow per zone area
   ,                         !heating max air flow
   ;                         !heating max air flow fraction
Sizing:Zone,
   NORTH ZONE,                         !Name of a zone
   12,                         !Zone cooling design supply air temperature
   50,                         !Zone heating design supply air temperature
   0.008,                         !Zone cooling design supply air humidity ratio
   0.008,                         !Zone heating design supply air humidity ratio
   flow/person,                         !outside air method
   0.00944,                         !outside air flow per person
   ,                         !outside air flow per zone area
   ,                         !outside air flow per zone
   ,                         !zone heating sizing factor
   ,                         !zone cooling sizing factor
   DesignDay,                         !cooling design air flow method
   ,                         !cooling design air flow rate
   ,                         !cooling min air flow per zone area
   ,                         !cooling min air flow
   ,                         !cooling min air flow fraction
   DesignDay,                         !heating design air flow method
   ,                         !heating design air flow rate
   ,                         !heating max air flow per zone area
   ,                         !heating max air flow
   ;                         !heating max air flow fraction
ZoneControl:Thermostat,
   Zone 1 Thermostat,                         !Thermostat Name
   WEST ZONE,                         !Zone Name
   West Zone Control Type Sched,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:DualSetpoint,                         !Control Type #1
   DualSetPoint;                         !Control Type Name #1
ZoneControl:Thermostat,
   Zone 2 Thermostat,                         !Thermostat Name
   EAST ZONE,                         !Zone Name
   Other Zone Control Type Sched,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:SingleHeating,                         !Control Type #1
   Heating Setpoint,                         !Control Type Name #1
   ThermostatSetpoint:SingleCooling,                         !Control Type #2
   Cooling Setpoint;                         !Control Type Name #2
ZoneControl:Thermostat,
   Zone 3 Thermostat,                         !Thermostat Name
   NORTH ZONE,                         !Zone Name
   Other Zone Control Type Sched,                         !Control Type SCHEDULE Name
   ThermostatSetpoint:SingleHeating,                         !Control Type #1
   Heating Setpoint,                         !Control Type Name #1
   ThermostatSetpoint:SingleCooling,                         !Control Type #2
   Cooling Setpoint;                         !Control Type Name #2
CURVE:QUADRATIC,
   HPACCoolCapFFF,                         !Name
   0.8,                         !Coeff1 Constant
   0.2,                         !Coeff2 x
   0,                         !Coeff3 x**2
   0.5,                         !minimum value of x
   1.5,                         !maximum value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
CURVE:QUADRATIC,
   HPACEIRFFF,                         !Name
   1.1552,                         !Coeff1 Constant
   -0.1808,                         !Coeff2 x
   0.0256,                         !Coeff3 x**2
   0.5,                         !minimum value of x
   1.5,                         !maximum value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
CURVE:QUADRATIC,
   HPACPLFFPLR,                         !Name
   0.85,                         !Coeff1 Constant
   0.15,                         !Coeff2 x
   0,                         !Coeff3 x**2
   0.5,                         !minimum value of x
   1,                         !maximum value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
CURVE:QUADRATIC,
   HPACHeatEIRFFF,                         !Name
   1.3824,                         !Coeff1 Constant
   -0.4336,                         !Coeff2 x
   0.0512,                         !Coeff3 x**2
   0,                         !minimum value of x
   1,                         !maximum value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
CURVE:QUADRATIC,
   HPACCOOLPLFFPLR,                         !Name
   0.75,                         !Coeff1 Constant
   0.25,                         !Coeff2 x
   0,                         !Coeff3 x**2
   0,                         !minimum value of x
   1,                         !maximum value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
Curve:Cubic,
   HPACHeatCapFT,                         !Name 
   0.758746,                         !Coefficient1 Constant
   0.027626,                         !Coefficient2 x 
   0.000148716,                         !Coefficient3 x**2
   0.0000034992,                         !Coefficient4 x**3
   -20,                         !Minimum Value of x 
   20,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Dimensionless;                         !Output Unit Type
Curve:Cubic,
   HPACHeatCapFFF,                         !Name 
   0.84,                         !Coefficient1 Constant
   0.16,                         !Coefficient2 x 
   0,                         !Coefficient3 x**2
   0,                         !Coefficient4 x**3
   0.5,                         !Minimum Value of x 
   1.5,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   ,                         !Input Unit Type for X
   ;                         !Output Unit Type
Curve:Cubic,
   HPACHeatEIRFT,                         !Name 
   1.19248,                         !Coefficient1 Constant
   -0.0300438,                         !Coefficient2 x 
   0.00103745,                         !Coefficient3 x**2
   -0.000023328,                         !Coefficient4 x**3
   -20,                         !Minimum Value of x 
   20,                         !Maximum Value of x
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   ;                         !Output Unit Type
Curve:Cubic,
   FanEffRatioCurve,                         !Name 
   0.33856828,                         !Coefficient1 Constant
   1.72644131,                         !Coefficient2 x 
   -1.49280132,                         !Coefficient3 x**2
   0.42776208,                         !Coefficient4 x**3
   0.5,                         !Minimum Value of x 
   1.5,                         !Maximum Value of x
   0.3,                         !Minimum Curve Output
   1,                         !Maximum Curve Output
   Dimensionless,                         !Input Unit Type for X
   Dimensionless;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HPACCoolCapFT,                         !Name
   0.942587793,                         !Coeff1 Constant
   0.009543347,                         !Coeff2 x
   0.00068377,                         !Coeff3 x**2
   -0.011042676,                         !Coeff4 y
   0.000005249,                         !Coeff5 y**2
   -0.00000972,                         !Coeff6 x*y
   12.77778,                         !minimum value of x
   23.88889,                         !maximum value of x
   18,                         !minimum value of y
   46.11111,                         !maximum value of y
   18,                         !Minimum Curve Output
   46.1111,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
CURVE:BIQUADRATIC,
   HPACEIRFT,                         !Name
   0.342414409,                         !Coeff1 Constant
   0.034885008,                         !Coeff2 x
   -0.0006237,                         !Coeff3 x**2
   0.004977216,                         !Coeff4 y
   0.000437951,                         !Coeff5 y**2
   -0.000728028,                         !Coeff6 x*y
   12.77778,                         !minimum value of x
   23.88889,                         !maximum value of x
   18,                         !minimum value of y
   46.1111,                         !maximum value of y
   ,                         !Minimum Curve Output
   ,                         !Maximum Curve Output
   Temperature,                         !Input Unit Type for X
   Temperature,                         !Input Unit Type for Y
   Dimensionless;                         !Output Unit Type
ZoneHVAC:PackagedTerminalHeatPump,
   WEST ZONE_Zone1PTHP,                      !Heat pump name
   FanAndCoilAvailSched,                      !Availability schedule name
   WEST ZONE_Zone1PTHPAirInletNode,                      !Air inlet node name
   WEST ZONE_Zone1PTHPAirOutletNode,                      !Air outlet node name
   WEST ZONE_Zone1PTHPOAMixer,                      !Outside air mixer name
   autosize,                      !Supply air volumetric flow rate during cooling operation
   autosize,                      !Supply air volumetric flow rate during heating operation
   autosize,                      !Supply air volumetric flow rate when no cooling or heating is needed
   autosize,                      !Outside air volumetric flow rate during cooling operation
   autosize,                      !Outside air volumetric flow rate during heating operation
   autosize,                      !Outside air volumetric flow rate when no cooling or heating is needed
   FAN:OnOff,                      !Supply air fan type
   WEST ZONE_Zone1PTHPFan,                      !Supply air fan name
   Coil:Heating:DX:SingleSpeed,                      !Heating coil type
   WEST ZONE_Zone1PTHPDXHeatCoil,                      !Heating coil name
   0.001,                      !Heating convergence tolerance
   2,                      !Minimum outdoor dry-bulb temperature for compressor operation
   Coil:Cooling:DX:SingleSpeed,                      !Cooling coil type
   WEST ZONE_Zone1PTHPDXCoolCoil,                      !Cooling coil name
   0.001,                      !Cooling convergence tolerance
   Coil:Heating:Electric,                      !Supplemental heating coil type
   WEST ZONE_Zone1PTHPSupHeater,                      !Supplemental heating coil name
   autosize,                      !Maximum supply air temperature from supplemental heater
   20,                      !Maximum outdoor dry-bulb temperature for supplemental heater operation
   blowthrough,                      !Fan placement
   ConstantFanSch;                      !Heat pump operating mode
FAN:OnOff,
   WEST ZONE_Zone1PTHPFan,                      !Fan Name
   FanAndCoilAvailSched,                      !Available Schedule
   0.5,                      !Fan Total Efficiency
   75,                      !Delta Pressure
   autosize,                      !Max Flow Rate
   0.9,                      !Motor Efficiency
   1,                      !Motor In Airstream Fraction
   WEST ZONE_Zone1PTHPOAMixerOutletNode,                      !Fan_Inlet_Node
   WEST ZONE_Zone1PTHPFanOutletNode,                      !Fan_Outlet_Node
   General;                      !End-Use Subcategory
Coil:Cooling:DX:SingleSpeed,
   WEST ZONE_Zone1PTHPDXCoolCoil,                      !Name
   CoolingCoilAvailSched,                      !Availability Schedule Name
   autosize,                      !Rated Total Cooling Capacity
   autosize,                      !Rated Sensible Heat Ratio
   3,                      !Rated COP
   autosize,                      !Rated Air Flow Rate
   ,                      !Rated Evaporator Fan Power Per Volume Flow Rate
   WEST ZONE_Zone1PTHPFanOutletNode,                      !Air Inlet Node Name
   WEST ZONE_Zone1PTHPDXCoolCoilOutletNode,                      !Air Outlet Node Name
   HPACCoolCapFT,                      !Total Cooling Capacity Function of Temperature Curve Name
   HPACCoolCapFFF,                      !Total Cooling Capacity Function of Flow Fraction Curve Name
   HPACEIRFT,                      !Energy Input Ratio Function of Temperature Curve Name
   HPACEIRFFF,                      !Energy Input Ratio Function of Flow Fraction Curve Name
   HPACPLFFPLR,                      !Part Load Fraction Correlation Curve Name
   ,                      !Nominal Time for Condensate Removal to Begin
   ,                      !Ratio of Initial Moisture Evaporation Rate and Steady State Latent Capacity
   ,                      !Maximum Cycling Rate
   ,                      !Latent Capacity Time Constant 
   ,                      !Condenser Air Inlet Node Name
   EvaporativelyCooled,                      !Condenser Type
   ,                      !Evaporative Condenser Effectiveness
   ,                      !Evaporative Condenser Air Flow Rate
   ,                      !Evaporative Condenser Pump Rated Power Consumption
   ,                      !Crankcase Heater Capacity
   ,                      !Maximum Outdoor Dry-Bulb Temperature for Crankcase Heater Operation
   ,                      !Supply Water Storage Tank Name
   ,                      !Condensate Collection Water Storage Tank Name
   ,                      !Basin Heater Capacity 
   ,                      !Basin Heater Setpoint Temperature
   ;                      !Basin Heater Operating Schedule Name
Coil:Heating:DX:SingleSpeed,
   WEST ZONE_Zone1PTHPDXHeatCoil,                      !Name
   HeatingCoilAvailSched,                      !Availability Schedule Name
   autosize,                      !Rated Total Heating Capacity 
   2.75,                      !Rated COP
   autosize,                      !Rated Air Flow Rate
   WEST ZONE_Zone1PTHPDXCoolCoilOutletNode,                      !Air Inlet Node Name
   WEST ZONE_Zone1PTHPDXHeatCoilOutletNode,                      !Air Outlet Node Name
   HPACHeatCapFT,                      !Total Heating Capacity Function of Temperature Curve Name
   HPACHeatCapFFF,                      !Total Heating Capacity Function of Flow Fraction Curve Name
   HPACHeatEIRFT,                      !Energy Input Ratio Function of Temperature Curve Name
   HPACHeatEIRFFF,                      !Energy Input Ratio Function of Flow Fraction Curve Name
   HPACCOOLPLFFPLR,                      !Part Load Fraction Correlation Curve Name
   ,                      !Defrost Energy Input Ratio Function of Temperature Curve Name
   -8,                      !Minimum Outdoor Dry-Bulb Temperature for Compressor Operation
   0,                      !Maximum Outdoor Dry-Bulb Temperature for Defrost Operation
   200,                      !Crankcase Heater Capacity
   10,                      !Maximum Outdoor Dry-Bulb Temperature for Crankcase Heater Operation
   Resistive,                      !Defrost Strategy
   Timed,                      !Defrost Control
   0.166667,                      !Defrost Time Period Fraction
   autosize;                      !Resistive Defrost Heater Capacity
COIL:Heating:Electric,
   WEST ZONE_Zone1PTHPSupHeater,                      !Coil Name
   HeatingCoilAvailSched,                      !Available Schedule
   0.8,                      !Efficiency of the Coil
   autosize,                      !Nominal Capacity of the Coil
   WEST ZONE_Zone1PTHPDXHeatCoilOutletNode,                      !Coil_Air_Inlet_Node
   WEST ZONE_Zone1PTHPAirOutletNode,                      !Coil_Air_Outlet_Node
   ;                      !Coil_Temp_Setpoint_Node
OutdoorAir:Mixer,
   WEST ZONE_Zone1PTHPOAMixer,                      !Name
   WEST ZONE_Zone1PTHPOAMixerOutletNode,                      !Mixed_Air_Node
   WEST ZONE_Zone1PTHPOAInNode,                      !Outside_Air_Stream_Node
   WEST ZONE_Zone1PTHPExhNode,                      !Relief_Air_Stream_Node
   WEST ZONE_Zone1PTHPAirInletNode;                      !Return_Air_Stream_Node
ZoneHVAC:PackagedTerminalHeatPump,
   EAST ZONE_Zone2PTHP,                      !Heat pump name
   FanAndCoilAvailSched,                      !Availability schedule name
   EAST ZONE_Zone2PTHPAirInletNode,                      !Air inlet node name
   EAST ZONE_Zone2PTHPAirOutletNode,                      !Air outlet node name
   EAST ZONE_Zone2PTHPOAMixer,                      !Outside air mixer name
   autosize,                      !Supply air volumetric flow rate during cooling operation
   autosize,                      !Supply air volumetric flow rate during heating operation
   autosize,                      !Supply air volumetric flow rate when no cooling or heating is needed
   autosize,                      !Outside air volumetric flow rate during cooling operation
   autosize,                      !Outside air volumetric flow rate during heating operation
   autosize,                      !Outside air volumetric flow rate when no cooling or heating is needed
   FAN:OnOff,                      !Supply air fan type
   EAST ZONE_Zone2PTHPFan,                      !Supply air fan name
   Coil:Heating:DX:SingleSpeed,                      !Heating coil type
   EAST ZONE_Zone2PTHPDXHeatCoil,                      !Heating coil name
   0.001,                      !Heating convergence tolerance
   2,                      !Minimum outdoor dry-bulb temperature for compressor operation
   Coil:Cooling:DX:SingleSpeed,                      !Cooling coil type
   EAST ZONE_Zone2PTHPDXCoolCoil,                      !Cooling coil name
   0.001,                      !Cooling convergence tolerance
   Coil:Heating:Electric,                      !Supplemental heating coil type
   EAST ZONE_Zone2PTHPSupHeater,                      !Supplemental heating coil name
   autosize,                      !Maximum supply air temperature from supplemental heater
   20,                      !Maximum outdoor dry-bulb temperature for supplemental heater operation
   blowthrough,                      !Fan placement
   ConstantFanSch;                      !Heat pump operating mode
FAN:OnOff,
   EAST ZONE_Zone2PTHPFan,                      !Fan Name
   FanAndCoilAvailSched,                      !Available Schedule
   0.5,                      !Fan Total Efficiency
   75,                      !Delta Pressure
   autosize,                      !Max Flow Rate
   0.9,                      !Motor Efficiency
   1,                      !Motor In Airstream Fraction
   EAST ZONE_Zone2PTHPOAMixerOutletNode,                      !Fan_Inlet_Node
   EAST ZONE_Zone2PTHPFanOutletNode,                      !Fan_Outlet_Node
   General;                      !End-Use Subcategory
Coil:Cooling:DX:SingleSpeed,
   EAST ZONE_Zone2PTHPDXCoolCoil,                      !Name
   CoolingCoilAvailSched,                      !Availability Schedule Name
   autosize,                      !Rated Total Cooling Capacity
   autosize,                      !Rated Sensible Heat Ratio
   3,                      !Rated COP
   autosize,                      !Rated Air Flow Rate
   ,                      !Rated Evaporator Fan Power Per Volume Flow Rate
   EAST ZONE_Zone2PTHPFanOutletNode,                      !Air Inlet Node Name
   EAST ZONE_Zone2PTHPCoolCoilOutletNode,                      !Air Outlet Node Name
   HPACCoolCapFT,                      !Total Cooling Capacity Function of Temperature Curve Name
   HPACCoolCapFFF,                      !Total Cooling Capacity Function of Flow Fraction Curve Name
   HPACEIRFT,                      !Energy Input Ratio Function of Temperature Curve Name
   HPACEIRFFF,                      !Energy Input Ratio Function of Flow Fraction Curve Name
   HPACPLFFPLR,                      !Part Load Fraction Correlation Curve Name
   ,                      !Nominal Time for Condensate Removal to Begin
   ,                      !Ratio of Initial Moisture Evaporation Rate and Steady State Latent Capacity
   ,                      !Maximum Cycling Rate
   ,                      !Latent Capacity Time Constant 
   ,                      !Condenser Air Inlet Node Name
   EvaporativelyCooled,                      !Condenser Type
   ,                      !Evaporative Condenser Effectiveness
   ,                      !Evaporative Condenser Air Flow Rate
   ,                      !Evaporative Condenser Pump Rated Power Consumption
   ,                      !Crankcase Heater Capacity
   ,                      !Maximum Outdoor Dry-Bulb Temperature for Crankcase Heater Operation
   ,                      !Supply Water Storage Tank Name
   ,                      !Condensate Collection Water Storage Tank Name
   ,                      !Basin Heater Capacity 
   ,                      !Basin Heater Setpoint Temperature
   ;                      !Basin Heater Operating Schedule Name
Coil:Heating:DX:SingleSpeed,
   EAST ZONE_Zone2PTHPDXHeatCoil,                      !Name
   HeatingCoilAvailSched,                      !Availability Schedule Name
   autosize,                      !Rated Total Heating Capacity 
   2.75,                      !Rated COP
   autosize,                      !Rated Air Flow Rate
   EAST ZONE_Zone2PTHPCoolCoilOutletNode,                      !Air Inlet Node Name
   EAST ZONE_Zone2PTHPDXHeatCoilOutletNode,                      !Air Outlet Node Name
   HPACEIRFT,                      !Total Heating Capacity Function of Temperature Curve Name
   HPACHeatEIRFFF,                      !Total Heating Capacity Function of Flow Fraction Curve Name
   HPACEIRFT,                      !Energy Input Ratio Function of Temperature Curve Name
   HPACEIRFFF,                      !Energy Input Ratio Function of Flow Fraction Curve Name
   HPACPLFFPLR,                      !Part Load Fraction Correlation Curve Name
   ,                      !Defrost Energy Input Ratio Function of Temperature Curve Name
   -8,                      !Minimum Outdoor Dry-Bulb Temperature for Compressor Operation
   0,                      !Maximum Outdoor Dry-Bulb Temperature for Defrost Operation
   500,                      !Crankcase Heater Capacity
   10,                      !Maximum Outdoor Dry-Bulb Temperature for Crankcase Heater Operation
   Resistive,                      !Defrost Strategy
   Timed,                      !Defrost Control
   0.166667,                      !Defrost Time Period Fraction
   autosize;                      !Resistive Defrost Heater Capacity
COIL:Heating:Electric,
   EAST ZONE_Zone2PTHPSupHeater,                      !Coil Name
   HeatingCoilAvailSched,                      !Available Schedule
   0.8,                      !Efficiency of the Coil
   autosize,                      !Nominal Capacity of the Coil
   EAST ZONE_Zone2PTHPDXHeatCoilOutletNode,                      !Coil_Air_Inlet_Node
   EAST ZONE_Zone2PTHPAirOutletNode,                      !Coil_Air_Outlet_Node
   ;                      !Coil_Temp_Setpoint_Node
OutdoorAir:Mixer,
   EAST ZONE_Zone2PTHPOAMixer,                      !Name
   EAST ZONE_Zone2PTHPOAMixerOutletNode,                      !Mixed_Air_Node
   EAST ZONE_Zone2PTHPOAInNode,                      !Outside_Air_Stream_Node
   EAST ZONE_Zone2PTHPExhNode,                      !Relief_Air_Stream_Node
   EAST ZONE_Zone2PTHPAirInletNode;                      !Return_Air_Stream_Node
ZoneHVAC:PackagedTerminalHeatPump,
   NORTH ZONE_Zone3PTHP,                      !Heat pump name
   FanAndCoilAvailSched,                      !Availability schedule name
   NORTH ZONE_Zone3PTHPAirInletNode,                      !Air inlet node name
   NORTH ZONE_Zone3PTHPAirOutletNode,                      !Air outlet node name
   NORTH ZONE_Zone3PTHPOAMixer,                      !Outside air mixer name
   autosize,                      !Supply air volumetric flow rate during cooling operation
   autosize,                      !Supply air volumetric flow rate during heating operation
   autosize,                      !Supply air volumetric flow rate when no cooling or heating is needed
   autosize,                      !Outside air volumetric flow rate during cooling operation
   autosize,                      !Outside air volumetric flow rate during heating operation
   autosize,                      !Outside air volumetric flow rate when no cooling or heating is needed
   FAN:ConstantVolume,                      !Supply air fan type
   NORTH ZONE_Zone3PTHPFan,                      !Supply air fan name
   Coil:Heating:DX:SingleSpeed,                      !Heating coil type
   NORTH ZONE_Zone3PTHPDXHeatCoil,                      !Heating coil name
   0.001,                      !Heating convergence tolerance
   -8.0,                      !Minimum outdoor dry-bulb temperature for compressor operation
   Coil:Cooling:DX:SingleSpeed,                      !Cooling coil type
   NORTH ZONE_Zone3PTHPDXCoolCoil,                      !Cooling coil name
   0.001,                      !Cooling convergence tolerance
   Coil:Heating:Electric,                      !Supplemental heating coil type
   NORTH ZONE_Zone3PTHPSupHeater,                      !Supplemental heating coil name
   autosize,                      !Maximum supply air temperature from supplemental heater
   20,                      !Maximum outdoor dry-bulb temperature for supplemental heater operation
   blowthrough,                      !Fan placement
   ConstantFanSch;                      !Heat pump operating mode
Fan:ConstantVolume,
   NORTH ZONE_Zone3PTHPFan,                      !Fan Name
   FanAndCoilAvailSched,                      !Available Schedule
   0.5,                      !Fan Total Efficiency
   75,                      !Delta Pressure
   autosize,                      !Max Flow Rate
   0.9,                      !Motor Efficiency
   1,                      !Motor In Airstream Fraction
   NORTH ZONE_Zone3PTHPOAMixerOutletNode,                      !Fan_Inlet_Node
   NORTH ZONE_Zone2PTHPFanOutletNode,                      !Fan_Outlet_Node
   General;                      !End-Use Subcategory
Coil:Cooling:DX:SingleSpeed,
   NORTH ZONE_Zone3PTHPDXCoolCoil,                      !Name
   CoolingCoilAvailSched,                      !Availability Schedule Name
   autosize,                      !Rated Total Cooling Capacity
   autosize,                      !Rated Sensible Heat Ratio
   3,                      !Rated COP
   autosize,                      !Rated Air Flow Rate
   ,                      !Rated Evaporator Fan Power Per Volume Flow Rate
   NORTH ZONE_Zone2PTHPFanOutletNode,                      !Air Inlet Node Name
   NORTH ZONE_Zone3PTHPCoolCoilOutletNode,                      !Air Outlet Node Name
   HPACCoolCapFT,                      !Total Cooling Capacity Function of Temperature Curve Name
   HPACCoolCapFFF,                      !Total Cooling Capacity Function of Flow Fraction Curve Name
   HPACEIRFT,                      !Energy Input Ratio Function of Temperature Curve Name
   HPACEIRFFF,                      !Energy Input Ratio Function of Flow Fraction Curve Name
   HPACPLFFPLR,                      !Part Load Fraction Correlation Curve Name
   ,                      !Nominal Time for Condensate Removal to Begin
   ,                      !Ratio of Initial Moisture Evaporation Rate and Steady State Latent Capacity
   ,                      !Maximum Cycling Rate
   ,                      !Latent Capacity Time Constant 
   ,                      !Condenser Air Inlet Node Name
   EvaporativelyCooled,                      !Condenser Type
   ,                      !Evaporative Condenser Effectiveness
   ,                      !Evaporative Condenser Air Flow Rate
   ,                      !Evaporative Condenser Pump Rated Power Consumption
   ,                      !Crankcase Heater Capacity
   ,                      !Maximum Outdoor Dry-Bulb Temperature for Crankcase Heater Operation
   ,                      !Supply Water Storage Tank Name
   ,                      !Condensate Collection Water Storage Tank Name
   ,                      !Basin Heater Capacity 
   ,                      !Basin Heater Setpoint Temperature
   ;                      !Basin Heater Operating Schedule Name
Coil:Heating:DX:SingleSpeed,
   NORTH ZONE_Zone3PTHPDXHeatCoil,                      !Name
   HeatingCoilAvailSched,                      !Availability Schedule Name
   autosize,                      !Rated Total Heating Capacity 
   3,                      !Rated COP
   autosize,                      !Rated Air Flow Rate
   NORTH ZONE_Zone3PTHPCoolCoilOutletNode,                      !Air Inlet Node Name
   NORTH ZONE_Zone3PTHPDXHeatCoilOutletNode,                      !Air Outlet Node Name
   HPACEIRFT,                      !Total Heating Capacity Function of Temperature Curve Name
   HPACHeatEIRFFF,                      !Total Heating Capacity Function of Flow Fraction Curve Name
   HPACEIRFT,                      !Energy Input Ratio Function of Temperature Curve Name
   HPACEIRFFF,                      !Energy Input Ratio Function of Flow Fraction Curve Name
   HPACPLFFPLR,                      !Part Load Fraction Correlation Curve Name
   HPACEIRFT,                      !Defrost Energy Input Ratio Function of Temperature Curve Name
   -8,                      !Minimum Outdoor Dry-Bulb Temperature for Compressor Operation
   0,                      !Maximum Outdoor Dry-Bulb Temperature for Defrost Operation
   200,                      !Crankcase Heater Capacity
   10,                      !Maximum Outdoor Dry-Bulb Temperature for Crankcase Heater Operation
   ReverseCycle,                      !Defrost Strategy
   Timed,                      !Defrost Control
   0.058333,                      !Defrost Time Period Fraction
   autosize;                      !Resistive Defrost Heater Capacity
COIL:Heating:Electric,
   NORTH ZONE_Zone3PTHPSupHeater,                      !Coil Name
   HeatingCoilAvailSched,                      !Available Schedule
   0.8,                      !Efficiency of the Coil
   autosize,                      !Nominal Capacity of the Coil
   NORTH ZONE_Zone3PTHPDXHeatCoilOutletNode,                      !Coil_Air_Inlet_Node
   NORTH ZONE_Zone3PTHPAirOutletNode,                      !Coil_Air_Outlet_Node
   ;                      !Coil_Temp_Setpoint_Node
OutdoorAir:Mixer,
   NORTH ZONE_Zone3PTHPOAMixer,                      !Name
   NORTH ZONE_Zone3PTHPOAMixerOutletNode,                      !Mixed_Air_Node
   NORTH ZONE_Zone3PTHPOAInNode,                      !Outside_Air_Stream_Node
   NORTH ZONE_Zone3PTHPExhNode,                      !Relief_Air_Stream_Node
   NORTH ZONE_Zone3PTHPAirInletNode;                      !Return_Air_Stream_Node
ZoneHVAC:EquipmentConnections,
   WEST ZONE,                      !Zone Name
   WEST ZONE_Zone1Equipment,                      !List Name: Zone Equipment
   WEST ZONE_Zone1PTHPAirOutletNode,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   WEST ZONE_Zone 1 Node,                      !Zone Air Node Name
   WEST ZONE_Zone1PTHPAirInletNode;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   EAST ZONE,                      !Zone Name
   EAST ZONE_Zone2Equipment,                      !List Name: Zone Equipment
   EAST ZONE_Zone2PTHPAirOutletNode,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   EAST ZONE_Zone 2 Node,                      !Zone Air Node Name
   EAST ZONE_Zone2PTHPAirInletNode;                      !Zone Return Air Node Name
ZoneHVAC:EquipmentConnections,
   NORTH ZONE,                      !Zone Name
   NORTH ZONE_Zone3Equipment,                      !List Name: Zone Equipment
   NORTH ZONE_Zone3PTHPAirOutletNode,                      !Node List or Node Name: Zone Air Inlet Node(s)
   ,                      !Node List or Node Name: Zone Air Exhaust Node(s)
   NORTH ZONE_Zone 3 Node,                      !Zone Air Node Name
   NORTH ZONE_Zone3PTHPAirInletNode;                      !Zone Return Air Node Name

