BIOS 1xx = H81M-P32
BIOS 1xx = CSM-H81M-P32
BIOS 1xx = H81M-S02
BIOS 1xx = H81M-P32L 

BIOS 2xx = B85M-P32
BIOS 2xx = CSM-B85M-P32
BIOS 2xx = B85M-P32

BIOS 3xx = H87M-P32
BIOS 3xx = H87M-P32

BIOS Axx = H81M-P33 V2

BIOS Bxx = H81M-E33 V2
BIOS Cxx = B85M-P33 V2
BIOS Dxx = B85M-E33 V2
BIOS Hxx = H87M-E35
BIOS Ixx = H81M-E35
BIOS Jxx = B85M-E35

-------------------------------------------------


H87M-P32 (MS-7846) V3.3 BIOS Release
-------------------------------------------------

1. This is AMI BIOS release

2. This BIOS fixes the following problem of the previous version:
-  Improved RAID card compatibility.
-  Improved VGA compatibility.
-  Improved memory compatibility.
-  Improved USB compatibility.


3. 2013/12/12

[Below information is Chinese language]

A. AMI BIOS 正式發行

B. 此版本修正下列問題:
-  改善與部分RAID Card的相容性.
-  改善顯示卡的相容性.
-  改善超頻記憶體相容性.
-  改善USB相容性. 

C. 更新日期: 公元2013年12月12號