NodeList,
   DHW Loop Setpoint Node List,                         !Node List Name
   Instantaneous Water Heater Outlet Node,                         !Node_ID_1
   Instantaneous Water Heater Inlet Node;                         !Node_ID_2
NodeList,
   Collector Loop Setpoint Node List,                         !Node List Name
   Storage Tank Source Loop Outlet Node;                         !Node_ID_1
BranchList,
   Storage Tank Use Branches,                         !Branch List Name
   Storage Tank Use Inlet Branch,                         !Branch Name 1
   Storage Tank Use Branch,                         !Branch Name 2
   Storage Tank Tempering Branch,                         !Branch Name 3
   Storage Tank Use Outlet Branch;                         !Branch Name 4
BranchList,
   Demand Branches,                         !Branch List Name
   Demand Inlet Branch,                         !Branch Name 1
   Domestic Hot Water Branch,                         !Branch Name 2
   Demand Outlet Branch;                         !Branch Name 3
BranchList,
   Storage Tank Source Branches,                         !Branch List Name
   Storage Tank Source Inlet Branch,                         !Branch Name 1
   Storage Tank Source Branch,                         !Branch Name 2
   Storage Tank Source Outlet Branch;                         !Branch Name 3
BranchList,
   Collector Branches,                         !Branch List Name
   Collector Inlet Branch,                         !Branch Name 1
   Collector 1 Branch,                         !Branch Name 2
   Collector 2 Branch,                         !Branch Name 3
   Collector 3 Branch,                         !Branch Name 4
   Collector Outlet Branch;                         !Branch Name 5
PlantLoop,
   DHW Loop,                         !Plant Loop Name
   Water,                         !Fluid Type
   DHW Loop Operation,                         !Plant Operation Scheme List Name
   Instantaneous Water Heater Outlet Node,                         !Loop Temperature Setpoint Node Name
   100,                         !Maximum Loop Temperature
   3,                         !Minimum Loop Temperature
   autosize,                         !Maximum Loop Volumetric Flow Rate
   0,                         !Minimum Loop Volumetric Flow Rate
   autocalculate,                         !volume of the plant loop
   Storage Tank Use Loop Inlet Node,                         !Plant Side Inlet Node Name
   Instantaneous Water Heater Outlet Node,                         !Plant Side Outlet Node Name
   Storage Tank Use Branches,                         !Plant Side Branch List Name
   Storage Tank Use Connectors,                         !Plant Side Connector List Name
   Demand Inlet Node,                         !Demand Side Inlet Node Name
   Demand Outlet Node,                         !Demand Side Outlet Nodes Name
   Demand Branches,                         !Demand Side Branch List Name
   Demand Connectors,                         !Demand Side Connector List Name
   OPTIMAL,                         !Load Distribution Scheme
   ,                         !System Availability Manager List
   ,                         !Plant Loop Demand Calculation Scheme
   ,                         !Common Pipe Simulation
   ;                         !Pressure Simulation Type
PlantLoop,
   Collector Loop,                         !Plant Loop Name
   Water,                         !Fluid Type
   Collector Loop Operation,                         !Plant Operation Scheme List Name
   Storage Tank Source Loop Outlet Node,                         !Loop Temperature Setpoint Node Name
   100,                         !Maximum Loop Temperature
   3,                         !Minimum Loop Temperature
   autosize,                         !Maximum Loop Volumetric Flow Rate
   0,                         !Minimum Loop Volumetric Flow Rate
   autocalculate,                         !volume of the plant loop
   Storage Tank Source Loop Inlet Node,                         !Plant Side Inlet Node Name
   Storage Tank Source Loop Outlet Node,                         !Plant Side Outlet Node Name
   Storage Tank Source Branches,                         !Plant Side Branch List Name
   Storage Tank Source Connectors,                         !Plant Side Connector List Name
   Collector Loop Inlet Node,                         !Demand Side Inlet Node Name
   Collector Loop Outlet Node,                         !Demand Side Outlet Nodes Name
   Collector Branches,                         !Demand Side Branch List Name
   Collector Connectors,                         !Demand Side Connector List Name
   OPTIMAL,                         !Load Distribution Scheme
   ,                         !System Availability Manager List
   ,                         !Plant Loop Demand Calculation Scheme
   ,                         !Common Pipe Simulation
   ;                         !Pressure Simulation Type
Branch,
   Storage Tank Use Inlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pump:VariableSpeed,                         !Comp1 Type
   DHW Loop Pump,                         !Comp1 Name
   Storage Tank Use Loop Inlet Node,                         !Comp1 Inlet Node Name
   DHW Use Side Pump Outlet,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Storage Tank Tempering Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   TemperingValve,                         !Comp1 Type
   DHW Anti-Scald Diverter,                         !Comp1 Name
   DHW Anti-Scald Inlet Node,                         !Comp1 Inlet Node Name
   DHW Anti-Scald Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Storage Tank Use Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   WATERHEATER:MIXED,                         !Comp1 Type
   Storage Tank,                         !Comp1 Name
   Storage Tank Use Inlet Node,                         !Comp1 Inlet Node Name
   Storage Tank Use Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Storage Tank Use Outlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   WATERHEATER:MIXED,                         !Comp1 Type
   Instantaneous Water Heater,                         !Comp1 Name
   Instantaneous Water Heater Inlet Node,                         !Comp1 Inlet Node Name
   Instantaneous Water Heater Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Demand Inlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Demand Inlet Pipe,                         !Comp1 Name
   Demand Inlet Node,                         !Comp1 Inlet Node Name
   Demand Pipe-DHW Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Domestic Hot Water Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   WaterUse:Connections,                         !Comp1 Type
   Domestic Hot Water,                         !Comp1 Name
   Domestic Hot Water Inlet Node,                         !Comp1 Inlet Node Name
   Domestic Hot Water Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Demand Outlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Demand Outlet Pipe,                         !Comp1 Name
   Demand DHW-Pipe Node,                         !Comp1 Inlet Node Name
   Demand Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Storage Tank Source Inlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pump:VariableSpeed,                         !Comp1 Type
   Collector Loop Pump,                         !Comp1 Name
   Storage Tank Source Loop Inlet Node,                         !Comp1 Inlet Node Name
   Storage Tank Source Pump-Water Heater Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Storage Tank Source Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   WATERHEATER:MIXED,                         !Comp1 Type
   Storage Tank,                         !Comp1 Name
   Storage Tank Source Inlet Node,                         !Comp1 Inlet Node Name
   Storage Tank Source Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Storage Tank Source Outlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Storage Tank Source Outlet Pipe,                         !Comp1 Name
   Storage Tank Source Water Heater-Pipe Node,                         !Comp1 Inlet Node Name
   Storage Tank Source Loop Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Collector Inlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Collector Inlet Pipe,                         !Comp1 Name
   Collector Loop Inlet Node,                         !Comp1 Inlet Node Name
   Collector Pipe-Collector Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
Branch,
   Collector 1 Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   SolarCollector:FlatPlate:Water,                         !Comp1 Type
   Collector 1,                         !Comp1 Name
   Collector 1 Inlet Node,                         !Comp1 Inlet Node Name
   Collector 1 Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Collector 2 Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   SolarCollector:FlatPlate:Water,                         !Comp1 Type
   Collector 2,                         !Comp1 Name
   Collector 2 Inlet Node,                         !Comp1 Inlet Node Name
   Collector 2 Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Collector 3 Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   SolarCollector:FlatPlate:Water,                         !Comp1 Type
   Collector 3,                         !Comp1 Name
   Collector 3 Inlet Node,                         !Comp1 Inlet Node Name
   Collector 3 Outlet Node,                         !Comp1 Outlet Node Name
   ACTIVE;                         !Comp1 Branch Control Type
Branch,
   Collector Outlet Branch,                         !Branch Name
   autosize,                         !Maximum Branch Flow Rate
   ,                         !Pressure Drop Curve Name
   Pipe:Adiabatic,                         !Comp1 Type
   Collector Outlet Pipe,                         !Comp1 Name
   Collector Collector-Pipe Node,                         !Comp1 Inlet Node Name
   Collector Loop Outlet Node,                         !Comp1 Outlet Node Name
   PASSIVE;                         !Comp1 Branch Control Type
ConnectorList,
   Storage Tank Use Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   Storage Tank Use Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   Storage Tank Use Mixer;                         !Name of Connector 2
ConnectorList,
   Demand Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   Demand Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   Demand Mixer;                         !Name of Connector 2
ConnectorList,
   Storage Tank Source Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   Storage Tank Source Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   Storage Tank Source Mixer;                         !Name of Connector 2
ConnectorList,
   Collector Connectors,                         !Connector List Name
   Connector:Splitter,                         !Type of Connector 1
   Collector Splitter,                         !Name of Connector 1
   Connector:Mixer,                         !Type of Connector 2
   Collector Mixer;                         !Name of Connector 2
PlantEquipmentOperationSchemes,
   DHW Loop Operation,                         !PlantOperationSchemeName
   PlantEquipmentOperation:HeatingLoad,                         !KEY--Control Scheme 1
   DHW Control Scheme,                         !Control Scheme Name 1
   AlwaysOnSchedule;                         !Control Scheme Schedule 1
PlantEquipmentOperationSchemes,
   Collector Loop Operation,                         !PlantOperationSchemeName
   PlantEquipmentOperation:HeatingLoad,                         !KEY--Control Scheme 1
   Collector Control Scheme,                         !Control Scheme Name 1
   AlwaysOnSchedule;                         !Control Scheme Schedule 1
PlantEquipmentOperation:HeatingLoad,
   DHW Control Scheme,                         !Name
   0,                         !Load Range Lower Limit 1
   10000000,                         !Load Range Upper Limit 1
   DHW Plant Equipment;                         !Priority Control Equip List Name 1
PlantEquipmentOperation:HeatingLoad,
   Collector Control Scheme,                         !Name
   0,                         !Load Range Lower Limit 1
   10000000,                         !Load Range Upper Limit 1
   Collector Plant Equipment;                         !Priority Control Equip List Name 1
PlantEquipmentList,
   DHW Plant Equipment,                         !Equip List Name
   TemperingValve,                         !KEY--Plant Equip 1
   DHW Anti-Scald Diverter,                         !Equip Name 1
   WATERHEATER:MIXED,                         !KEY--Plant Equip 2
   Storage Tank,                         !Equip Name 2
   WATERHEATER:MIXED,                         !KEY--Plant Equip 3
   Instantaneous Water Heater;                         !Equip Name 3
PlantEquipmentList,
   Collector Plant Equipment,                         !Equip List Name
   WATERHEATER:MIXED,                         !KEY--Plant Equip 1
   Storage Tank;                         !Equip Name 1
AvailabilityManagerAssignmentList,
   Collector Loop Availability Manager List,                         !Name
   AvailabilityManager:DifferentialThermostat,                         !System Availability Manager Type 1
   Differential Thermostat Availability Manager,                         !System Availability Manager Name 1
   AvailabilityManager:HighTemperatureTurnOff,                         !System Availability Manager Type 2
   High Temperature Turn Off Availability Manager,                         !System Availability Manager Name 2
   AvailabilityManager:LowTemperatureTu,                         !System Availability Manager Type 3
   Low Temperature Turn On Availability Manager;                         !System Availability Manager Name 3
AvailabilityManager:DifferentialThermostat,
   Differential Thermostat Availability Manager,                         !Name
   Collector 1 Outlet Node,                         !Hot Node
   Storage Tank Source Outlet Node,                         !Cold Node
   10,                         !Temperature Difference On Limit
   2;                         !Temperature Difference Off Limit
AvailabilityManager:HighTemperatureTurnOff,
   High Temperature Turn Off Availability Manager,                         !Name
   Storage Tank Use Outlet Node,                         !Sensor Node
   60;                         !Temperature
AvailabilityManager:LowTemperatureTurnOn,
   Low Temperature Turn On Availability Manager,                         !Name
   Collector 1 Outlet Node,                         !Sensor Node
   0;                         !Temperature
SetpointManager:Scheduled,
   DHW Loop Setpoint Manager,                         !Name
   Temperature,                         !Control variable
   Hot Water Setpoint Temp Schedule,                         !Schedule Name
   DHW Loop Setpoint Node List;                         !Name of the set point Node or Node List
SetpointManager:Scheduled,
   Collector Loop Setpoint Manager,                         !Name
   Temperature,                         !Control variable
   Loop Temperature Schedule,                         !Schedule Name
   Collector Loop Setpoint Node List;                         !Name of the set point Node or Node List
Sizing:Plant,
   DHW Loop,                         !name of a PLANT LOOP or CONDENSER LOOP object
   Heating,                         !loop type
   82,                         !Design loop exit temperature
   11;                         !Design loop delta T
Sizing:Plant,
   Collector Loop,                         !name of a PLANT LOOP or CONDENSER LOOP object
   Heating,                         !loop type
   82,                         !Design loop exit temperature
   11;                         !Design loop delta T
SolarCollector:FlatPlate:Water,
   Collector 1,                         !Name
   Alternate Energy Technologies AE-1,                         !Solar Collector Performance Name
   Collector Surface 1,                         !Surface Name
   Collector 1 Inlet Node,                         !Inlet Node
   Collector 1 Outlet Node,                         !Outlet Node
   0.00001;                         !Maximum Volumetric Flow Rate
SolarCollectorPerformance:FlatPlate,
   Alternate Energy Technologies AE-1,                         !Name
   2.9646,                         !Gross Area
   Water,                         !Test Fluid
   0.0000388,                         !Test Volumetric Flow Rate
   INLET,                         !Test Correlation Type
   0.691,                         !Coefficient 1 of Efficiency Equation (Y-Intercept)
   -3.396,                         !Coefficient 2 of Efficiency Equation (1st Order)
   -0.00193,                         !Coefficient 3 of Efficiency Equation (2nd Order)
   -0.1939,                         !Coefficient 2 of Incident Angle Modifier (1st Order)
   -0.0055;                         !Coefficient 3 of Incident Angle Modifier (2nd Order)
SolarCollector:FlatPlate:Water,
   Collector 2,                         !Name
   Alternate Energy Technologies AE-2,                         !Solar Collector Performance Name
   Collector Surface 2,                         !Surface Name
   Collector 2 Inlet Node,                         !Inlet Node
   Collector 2 Outlet Node,                         !Outlet Node
   0.00001;                         !Maximum Volumetric Flow Rate
SolarCollectorPerformance:FlatPlate,
   Alternate Energy Technologies AE-2,                         !Name
   2.9646,                         !Gross Area
   Water,                         !Test Fluid
   0.0000388,                         !Test Volumetric Flow Rate
   INLET,                         !Test Correlation Type
   0.691,                         !Coefficient 1 of Efficiency Equation (Y-Intercept)
   -3.396,                         !Coefficient 2 of Efficiency Equation (1st Order)
   -0.00193,                         !Coefficient 3 of Efficiency Equation (2nd Order)
   -0.1939,                         !Coefficient 2 of Incident Angle Modifier (1st Order)
   -0.0055;                         !Coefficient 3 of Incident Angle Modifier (2nd Order)
SolarCollector:FlatPlate:Water,
   Collector 3,                         !Name
   Alternate Energy Technologies AE-3,                         !Solar Collector Performance Name
   Collector Surface 3,                         !Surface Name
   Collector 3 Inlet Node,                         !Inlet Node
   Collector 3 Outlet Node,                         !Outlet Node
   0.00001;                         !Maximum Volumetric Flow Rate
SolarCollectorPerformance:FlatPlate,
   Alternate Energy Technologies AE-3,                         !Name
   2.9646,                         !Gross Area
   Water,                         !Test Fluid
   0.0000388,                         !Test Volumetric Flow Rate
   INLET,                         !Test Correlation Type
   0.691,                         !Coefficient 1 of Efficiency Equation (Y-Intercept)
   -3.396,                         !Coefficient 2 of Efficiency Equation (1st Order)
   -0.00193,                         !Coefficient 3 of Efficiency Equation (2nd Order)
   -0.1939,                         !Coefficient 2 of Incident Angle Modifier (1st Order)
   -0.0055;                         !Coefficient 3 of Incident Angle Modifier (2nd Order)
WaterHeater:Mixed,
   Instantaneous Water Heater,                         !Name
   0.00568,                         !Tank Volume
   Hot Water Setpoint Temp Schedule,                         !Setpoint Temperature Schedule
   ,                         !Deadband Temperature Difference
   82.2222,                         !Maximum Temperature Limit
   MODULATE,                         !Heater Control Type
   80000,                         !Heater Maximum Capacity
   ,                         !Heater Minimum Capacity
   0,                         !Heater Ignition Minimum Flow Rate
   0,                         !Heater Ignition Delay
   Electricity,                         !Heater Fuel Type
   0.9,                         !Heater Thermal Efficiency
   ,                         !Part Load Factor Curve
   ,                         !Off-Cycle Parasitic Fuel Consumption Rate
   ,                         !Off-Cycle Parasitic Fuel Type
   ,                         !Off-Cycle Parasitic Heat Fraction To Tank
   ,                         !On-Cycle Parasitic Fuel Consumption Rate
   ,                         !On-Cycle Parasitic Fuel Type
   ,                         !On-Cycle Parasitic Heat Fraction To Tank
   SCHEDULE,                         !Ambient Temperature Indicator
   Ambient Temp Schedule,                         !Ambient Temperature Schedule
   ,                         !Ambient Temperature Zone
   ,                         !Ambient Temperature Outside Air Node
   1,                         !Off-Cycle Loss Coefficient To Ambient Temperature
   1,                         !Off-Cycle Loss Fraction To Zone
   1,                         !On-Cycle Loss Coefficient To Ambient Temperature
   1,                         !On-Cycle Loss Fraction To Zone
   ,                         !Peak Volumetric Use Flow Rate
   ,                         !Use Flow Rate Fraction Schedule
   ,                         !Cold Water Supply Temperature Schedule
   Instantaneous Water Heater Inlet Node,                         !Use Side Inlet Node
   Instantaneous Water Heater Outlet Node,                         !Use Side Outlet Node
   1,                         !Use Side Effectiveness
   ,                         !Source Side Inlet Node
   ,                         !Source Side Outlet Node
   ,                         !Source Side Effectiveness
   autosize,                         !Use Side Design Flow Rate
   autosize,                         !Source Side Design Flow Rate
   ;                         !Indirect Water Heating Recovery Time 
WaterHeater:Mixed,
   Storage Tank,                         !Name
   1.5,                         !Tank Volume
   Hot Water Setpoint Temp Schedule,                         !Setpoint Temperature Schedule
   5,                         !Deadband Temperature Difference
   82.2222,                         !Maximum Temperature Limit
   CYCLE,                         !Heater Control Type
   ,                         !Heater Maximum Capacity
   ,                         !Heater Minimum Capacity
   ,                         !Heater Ignition Minimum Flow Rate
   ,                         !Heater Ignition Delay
   Electricity,                         !Heater Fuel Type
   0.9,                         !Heater Thermal Efficiency
   ,                         !Part Load Factor Curve
   0,                         !Off-Cycle Parasitic Fuel Consumption Rate
   ,                         !Off-Cycle Parasitic Fuel Type
   0,                         !Off-Cycle Parasitic Heat Fraction To Tank
   0,                         !On-Cycle Parasitic Fuel Consumption Rate
   ,                         !On-Cycle Parasitic Fuel Type
   0,                         !On-Cycle Parasitic Heat Fraction To Tank
   SCHEDULE,                         !Ambient Temperature Indicator
   Ambient Temp Schedule,                         !Ambient Temperature Schedule
   ,                         !Ambient Temperature Zone
   ,                         !Ambient Temperature Outside Air Node
   5,                         !Off-Cycle Loss Coefficient To Ambient Temperature
   ,                         !Off-Cycle Loss Fraction To Zone
   5,                         !On-Cycle Loss Coefficient To Ambient Temperature
   ,                         !On-Cycle Loss Fraction To Zone
   ,                         !Peak Volumetric Use Flow Rate
   ,                         !Use Flow Rate Fraction Schedule
   ,                         !Cold Water Supply Temperature Schedule
   Storage Tank Use Inlet Node,                         !Use Side Inlet Node
   Storage Tank Use Outlet Node,                         !Use Side Outlet Node
   1,                         !Use Side Effectiveness
   Storage Tank Source Inlet Node,                         !Source Side Inlet Node
   Storage Tank Source Outlet Node,                         !Source Side Outlet Node
   1,                         !Source Side Effectiveness
   autosize,                         !Use Side Design Flow Rate
   autosize,                         !Source Side Design Flow Rate
   1.5;                         !Indirect Water Heating Recovery Time 
Pump:VariableSpeed,
   Collector Loop Pump,                         !Pump Name
   Storage Tank Source Loop Inlet Node,                         !Inlet_Node
   Storage Tank Source Pump-Water Heater Node,                         !Outlet_Node
   autosize,                         !Rated Volumetric Flow Rate
   300000,                         !Rated Pump Head
   autosize,                         !Rated Power Consumption
   0.87,                         !Motor Efficiency
   0,                         !Fraction of Motor Inefficiencies to Fluid Stream
   0,                         !Coefficient1 of the Part Load Performance Curve
   1,                         !Coefficient2 of the Part Load Performance Curve
   0,                         !Coefficient3 of the Part Load Performance Curve
   0,                         !Coefficient4 of the Part Load Performance Curve
   0,                         !Min Flow Rate while operating in variable flow capacity
   INTERMITTENT,                         !Pump Control Type
   ;                         !Pump Flow Rate Schedule Name
Pipe:Adiabatic,
   Storage Tank Source Outlet Pipe,                         !Name
   Storage Tank Source Water Heater-Pipe Node,                         !Inlet Node Name
   Storage Tank Source Loop Outlet Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Collector Inlet Pipe,                         !Name
   Collector Loop Inlet Node,                         !Inlet Node Name
   Collector Pipe-Collector Node;                         !Outlet Node Name
Pipe:Adiabatic,
   Collector Outlet Pipe,                         !Name
   Collector Collector-Pipe Node,                         !Inlet Node Name
   Collector Loop Outlet Node;                         !Outlet Node Name
Pump:VariableSpeed,
   DHW Loop Pump,                         !Pump Name
   Storage Tank Use Loop Inlet Node,                         !Inlet_Node
   DHW Use Side Pump Outlet,                         !Outlet_Node
   autosize,                         !Rated Volumetric Flow Rate
   300000,                         !Rated Pump Head
   autosize,                         !Rated Power Consumption
   0.87,                         !Motor Efficiency
   0,                         !Fraction of Motor Inefficiencies to Fluid Stream
   0,                         !Coefficient1 of the Part Load Performance Curve
   1,                         !Coefficient2 of the Part Load Performance Curve
   0,                         !Coefficient3 of the Part Load Performance Curve
   0,                         !Coefficient4 of the Part Load Performance Curve
   0,                         !Min Flow Rate while operating in variable flow capacity
   INTERMITTENT,                         !Pump Control Type
   ;                         !Pump Flow Rate Schedule Name
TemperingValve,
   DHW Anti-Scald Diverter,                         !Name 
   DHW Anti-Scald Inlet Node,                         !Inlet Node Name
   DHW Anti-Scald Outlet Node,                         !Outlet Node Name
   Storage Tank Use Outlet Node,                         !Stream 2 Source Node Name
   Instantaneous Water Heater Outlet Node,                         !Temperature Setpoint Node Name
   DHW Use Side Pump Outlet;                         !Pump Outlet Node Name
Pipe:Adiabatic,
   Demand Inlet Pipe,                         !Name
   Demand Inlet Node,                         !Inlet Node Name
   Demand Pipe-DHW Node;                         !Outlet Node Name
WaterUse:Equipment,
   Showers,                         !Name
   Showers,                         !End-Use Subcategory
   0.000189,                         !Peak Flow Rate
   Showers,                         !Flow Rate Fraction Schedule Name
   Sinks and Showers Temp Schedule,                         !Target Temperature Schedule Name
   ,                         !Hot Water Supply Temperature Schedule Name
   ,                         !Cold Water Supply Temperature Schedule Name
   ,                         !Zone Name
   ,                         !Sensible Fraction Schedule Name
   ;                         !Latent Fraction Schedule Name
WaterUse:Connections,
   Domestic Hot Water,                         !Name
   Domestic Hot Water Inlet Node,                         !Inlet Node Name
   Domestic Hot Water Outlet Node,                         !Outlet Node Name
   ,                         !Supply Water Storage Tank Name
   ,                         !Reclamation Water Storage Tank Name
   ,                         !Hot Water Supply Temperature Schedule Name
   ,                         !Cold Water Supply Temperature Schedule Name
   None,                         !Drain Water Heat Exchanger Type
   ,                         !Drain Water Heat Exchanger Destination
   ,                         !Drain Water Heat Exchanger U-Factor Times Area
   Showers,                         !Water Use Equipment 1 Name
   Clotheswasher,                         !Water Use Equipment 2 Name
   Dishwasher;                         !Water Use Equipment 3 Name
Pipe:Adiabatic,
   Demand Outlet Pipe,                         !Name
   Demand DHW-Pipe Node,                         !Inlet Node Name
   Demand Outlet Node;                         !Outlet Node Name
WaterUse:Equipment,
   Clotheswasher,                         !Name
   Clotheswasher,                         !End-Use Subcategory
   0.000063,                         !Peak Flow Rate
   Clotheswasher,                         !Flow Rate Fraction Schedule Name
   Washers Temp Schedule,                         !Target Temperature Schedule Name
   ,                         !Hot Water Supply Temperature Schedule Name
   ,                         !Cold Water Supply Temperature Schedule Name
   ,                         !Zone Name
   ,                         !Sensible Fraction Schedule Name
   ;                         !Latent Fraction Schedule Name
WaterUse:Equipment,
   Dishwasher,                         !Name
   Dishwasher,                         !End-Use Subcategory
   0.000126,                         !Peak Flow Rate
   Dishwasher,                         !Flow Rate Fraction Schedule Name
   Washers Temp Schedule,                         !Target Temperature Schedule Name
   ,                         !Hot Water Supply Temperature Schedule Name
   ,                         !Cold Water Supply Temperature Schedule Name
   ,                         !Zone Name
   ,                         !Sensible Fraction Schedule Name
   ;                         !Latent Fraction Schedule Name
Connector:Splitter,
   Storage Tank Source Splitter,                         !SplitterName
   Storage Tank Source Inlet Branch,                         !Inlet Branch Name
   Storage Tank Source Branch;                         !Outlet Branch Name 1
Connector:Mixer,
   Storage Tank Source Mixer,                         !MixerName
   Storage Tank Source Outlet Branch,                         !Outlet Branch Name
   Storage Tank Source Branch;                         !Inlet Branch Name 1
Connector:Splitter,
   Collector Splitter,                         !SplitterName
   Collector Inlet Branch,                         !Inlet Branch Name
   Collector 1 Branch,                         !Outlet Branch Name 1
   Collector 2 Branch,                         !Outlet Branch Name 2
   Collector 3 Branch;                         !Outlet Branch Name 3
Connector:Mixer,
   Collector Mixer,                         !MixerName
   Collector Outlet Branch,                         !Outlet Branch Name
   Collector 1 Branch,                         !Inlet Branch Name 1
   Collector 2 Branch,                         !Inlet Branch Name 2
   Collector 3 Branch;                         !Inlet Branch Name 3
Connector:Splitter,
   Storage Tank Use Splitter,                         !SplitterName
   Storage Tank Use Inlet Branch,                         !Inlet Branch Name
   Storage Tank Tempering Branch,                         !Outlet Branch Name 1
   Storage Tank Use Branch;                         !Outlet Branch Name 2
Connector:Mixer,
   Storage Tank Use Mixer,                         !MixerName
   Storage Tank Use Outlet Branch,                         !Outlet Branch Name
   Storage Tank Tempering Branch,                         !Inlet Branch Name 1
   Storage Tank Use Branch;                         !Inlet Branch Name 2
Connector:Splitter,
   Demand Splitter,                         !SplitterName
   Demand Inlet Branch,                         !Inlet Branch Name
   Domestic Hot Water Branch;                         !Outlet Branch Name 1
Connector:Mixer,
   Demand Mixer,                         !MixerName
   Demand Outlet Branch,                         !Outlet Branch Name
   Domestic Hot Water Branch;                         !Inlet Branch Name 1

