


VERSION,
  2.2.0;

TIMESTEP IN HOUR,
  4;

System Convergence Limits,
  0,
  20;

Building,
  TTT.bdl,
  0,
  City,
  0.04,
  0.4,
  FullExterior,
  25;

INSIDE CONVECTION ALGORITHM,
  Detailed;

OUTSIDE CONVECTION ALGORITHM,
  Detailed;

Solution Algorithm,
  CTF,
  200;

Shadowing Calculations,
  20,
  15000;

DIAGNOSTICS,
  DisplayExtraWarnings;

Zone Volume Capacitance Multiplier,
  1.0;

Run Control,
  No,
  No,
  No,
  Yes,
  Yes;


Location, ±±¾©      ,
  39.92,
  -116.27,
   -8,
    31.5;

RunPeriod,
  1,
  1,
  12,
  31,
  Tuesday,
  No,
  Yes,
  Yes,
  Yes,
  Yes,
  1;

SpecialDayPeriod, New Year's Day, 1/1, 1, Holiday;

SpecialDayPeriod, Spring Festival, 2/1, 3, Holiday;

SpecialDayPeriod, Tomb-sweeping Day, 4/4, 1, Holiday;

SpecialDayPeriod, Labor Day, 5/1, 1, Holiday;

SpecialDayPeriod, Dragon Boat Festival, 6/15, 1, Holiday;

SpecialDayPeriod, Mid-autumn Festival, 9/15, 1, Holiday;

SpecialDayPeriod, National Day, 10/1, 3, Holiday;


ScheduleType, Fraction, 0.0 : 1.0, CONTINUOUS;
ScheduleType, Temperature, -60 : 200, CONTINUOUS;
ScheduleType, On/Off, 0 : 1, DISCRETE;
ScheduleType, Control Type, 0 : 4, DISCRETE;
ScheduleType, Any Number; !Not limited






MATERIAL:Regular, Ê¯»ÒË®ÄàÉ°½¬1700 ,
Rough,
0.1,
 0.87,
 1700,
 1050,
0.7,
0.7,
0.95;
MATERIAL:Regular, ¸Ö½î»ìÄýÍÁ2500 ,
Rough,
0.1,
 1.74,
 2500,
  920,
0.7,
0.7,
0.95;
MATERIAL:Regular, 190µ¥ÅÅ¿×»ìÄýÍÁÆö¿é ,
Rough,
0.1,
 0.95,
 1200,
  600,
0.7,
0.7,
0.95;
MATERIAL:Regular, ¾Û±½ÒÒÏ©ÅÝÄ­ËÜÁÏ30 ,
Rough,
0.1,
 0.04,
   30,
 1380,
0.7,
0.7,
0.95;
MATERIAL:Regular,¾øÈÈ°å²ÄÁÏ,
Smooth,
0.1,
0.0001,
2500,
1000,
0.1,
0.1,
1.0;
MATERIAL:Regular,ÐéÄâÇ½²ÄÁÏ,
VerySmooth,
0.001,
410.00,
1.0,
0.1,
0.1,
0.1,
0.1;
MATERIAL:Air,AIR30,
0.16;



CONSTRUCTION,EW,
Ê¯»ÒË®ÄàÉ°½¬1700 ,
¾Û±½ÒÒÏ©ÅÝÄ­ËÜÁÏ30 ,
¸Ö½î»ìÄýÍÁ2500 ,
Ê¯»ÒË®ÄàÉ°½¬1700 ;
CONSTRUCTION,Roof,
Ê¯»ÒË®ÄàÉ°½¬1700 ,
¾Û±½ÒÒÏ©ÅÝÄ­ËÜÁÏ30 ,
¸Ö½î»ìÄýÍÁ2500 ,
Ê¯»ÒË®ÄàÉ°½¬1700 ;
CONSTRUCTION,IW,
Ê¯»ÒË®ÄàÉ°½¬1700 ,
¸Ö½î»ìÄýÍÁ2500 ,
Ê¯»ÒË®ÄàÉ°½¬1700 ;
CONSTRUCTION,GRND,
Ê¯»ÒË®ÄàÉ°½¬1700 ,
¾Û±½ÒÒÏ©ÅÝÄ­ËÜÁÏ30 ,
¸Ö½î»ìÄýÍÁ2500 ,
Ê¯»ÒË®ÄàÉ°½¬1700 ;
CONSTRUCTION,¾øÈÈÇ½,
Ê¯»ÒË®ÄàÉ°½¬1700 ;
CONSTRUCTION,¾øÈÈ°å,
¾øÈÈ°å²ÄÁÏ;
CONSTRUCTION,ÐéÄâÇ½,
ÐéÄâÇ½²ÄÁÏ;
CONSTRUCTION,ÐéÄâ°å,
ÐéÄâÇ½²ÄÁÏ;


! SCHEDULE:




!CONSTRUCTION of EWall, IWall, Roof, Floor, Ground:

MATERIAL:WINDOWGLASS,
    Win0,               !- Name
    SpectralAverage,         !- Optical Data Type
    ,                        !- Name of Window Glass Spectral Data Set
    0.003,                   !- Thickness {m}
    0.837,                   !- Solar Transmittance at Normal Incidence
    0.075,                   !- Solar Reflectance at Normal Incidence: Front Side
    0.075,                   !- Solar Reflectance at Normal Incidence: Back Side
    0.898,                   !- Visible Transmittance at Normal Incidence
    0.081,                   !- Visible Reflectance at Normal Incidence: Front Side
    0.081,                   !- Visible Reflectance at Normal Incidence: Back Side
    0.0,                     !- IR Transmittance at Normal Incidence
    0.84,                    !- IR Hemispherical Emissivity: Front Side
    0.84,                    !- IR Hemispherical Emissivity: Back Side
    0.9;                     !- Conductivity {W/m-K}
MATERIAL:WINDOWGLASS,
    Win1,               !- Name
    SpectralAverage,         !- Optical Data Type
    ,                        !- Name of Window Glass Spectral Data Set
    0.003,                   !- Thickness {m}
    0.837,                   !- Solar Transmittance at Normal Incidence
    0.075,                   !- Solar Reflectance at Normal Incidence: Front Side
    0.075,                   !- Solar Reflectance at Normal Incidence: Back Side
    0.898,                   !- Visible Transmittance at Normal Incidence
    0.081,                   !- Visible Reflectance at Normal Incidence: Front Side
    0.081,                   !- Visible Reflectance at Normal Incidence: Back Side
    0.0,                     !- IR Transmittance at Normal Incidence
    0.84,                    !- IR Hemispherical Emissivity: Front Side
    0.84,                    !- IR Hemispherical Emissivity: Back Side
    0.9;                     !- Conductivity {W/m-K}
MATERIAL:REGULAR-R,
    Door0,                   !- Name
    Rough,                   !- Roughness
     0.5882353,               !- Thermal Resistance {m2-K/W}
    0.9000000,               !- Absorptance:Thermal
    0.7500000,               !- Absorptance:Solar
    0.7500000;               !- Absorptance:Visible
MATERIAL:REGULAR-R,
    Door1,                   !- Name
    Rough,                   !- Roughness
     0.3030303,               !- Thermal Resistance {m2-K/W}
    0.9000000,               !- Absorptance:Thermal
    0.7500000,               !- Absorptance:Solar
    0.7500000;               !- Absorptance:Visible

!-   =================== µÚ  1 ²ã ======================
!-   ===========  ALL OBJECTS IN CLASS: ZONE ===========
! Room 1001**********
ZONE,
    Rm01001,      !Zone Name
    0,                       !- Relative North (to building) {deg}
    0, 0, 0,                 !- X,Y,Z  {m}
    1,                       !- Type
    1,                       !- Multiplier
    Autocalculate,           !- Ceiling Height {m}
    Autocalculate;           !- Volume {m3}

!-   ===========  ALL OBJECTS IN CLASS: SURFACEGEOMETRY ===========
SurfaceGeometry,
    UpperLeftCorner,         !- SurfaceStartingPosition
    CounterClockWise,        !- VertexEntry
    WorldCoordinateSystem;   !- CoordinateSystem


Surface:HeatTransfer,
    Rm01001:EW01001, 
    Wall,                    !- Surface Type
    E-W0,                    !- Construction Name of the Surface
    Rm01001,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
	,                        !- OutsideFaceEnvironment Object
    SunExposed,              !- Sun Exposure
    WindExposed,             !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
     8.10, 2.00, 0.00,   !- X,Y,Z ==> Vertex 1
     4.30, 2.00, 0.00,   !- X,Y,Z ==> Vertex 2
     4.30, 2.00, 2.80,   !- X,Y,Z ==> Vertex 3
     8.10, 2.00, 2.80;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer:Sub,
    Rm01001:EW01001:DOOR-EW01001, 
    Door,                    !- Surface Type
    Door0,                                   !- Construction Name of the Surface
    EW01001,                !- Base Surface Name
    ,                        !- OutsideFaceEnvironment Object
    0.50,                    !- View Factor to Ground
    ,                        !- Name of shading control
    ,                        !- WindowFrameAndDivider Name
    1.000000,                !- Multiplier
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
     6.90, 2.00, 0.04,   !- X,Y,Z ==> Vertex 1
     5.80, 2.00, 0.04,   !- X,Y,Z ==> Vertex 2
     5.80, 2.00, 2.04,   !- X,Y,Z ==> Vertex 3
     6.90, 2.00, 2.04;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer,
    Rm01001:EW01002, 
    Wall,                    !- Surface Type
    E-W0,                    !- Construction Name of the Surface
    Rm01001,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
	,                        !- OutsideFaceEnvironment Object
    SunExposed,              !- Sun Exposure
    WindExposed,             !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    11.90, 8.20, 0.00,   !- X,Y,Z ==> Vertex 1
    15.70, 8.20, 0.00,   !- X,Y,Z ==> Vertex 2
    15.70, 8.20, 2.80,   !- X,Y,Z ==> Vertex 3
    11.90, 8.20, 2.80;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer:Sub,
    Rm01001:EW01002:WIN-EW01002, 
    Window,                  !- Surface Type
    Win0,                    !- Construction Name of the Surface
    EW01002,                !- Base Surface Name
    ,                        !- OutsideFaceEnvironment Object
    0.50,                    !- View Factor to Ground
    ,                        !- Name of shading control
    ,                        !- WindowFrameAndDivider Name
    1.000000,                !- Multiplier
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    13.07, 8.20, 0.90,   !- X,Y,Z ==> Vertex 1
    14.54, 8.20, 0.90,   !- X,Y,Z ==> Vertex 2
    14.54, 8.20, 2.37,   !- X,Y,Z ==> Vertex 3
    13.07, 8.20, 2.37;   !- X,Y,Z ==> Vertex 4
 

Surface:HeatTransfer,
    Rm01001:EW01003, 
    Wall,                    !- Surface Type
    E-W0,                    !- Construction Name of the Surface
    Rm01001,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
	,                        !- OutsideFaceEnvironment Object
    SunExposed,              !- Sun Exposure
    WindExposed,             !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
     8.10, 8.20, 0.00,   !- X,Y,Z ==> Vertex 1
     8.10,14.40, 0.00,   !- X,Y,Z ==> Vertex 2
     8.10,14.40, 2.80,   !- X,Y,Z ==> Vertex 3
     8.10, 8.20, 2.80;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer:Sub,
    Rm01001:EW01003:WIN-EW01003, 
    Window,                  !- Surface Type
    Win0,                    !- Construction Name of the Surface
    EW01003,                !- Base Surface Name
    ,                        !- OutsideFaceEnvironment Object
    0.50,                    !- View Factor to Ground
    ,                        !- Name of shading control
    ,                        !- WindowFrameAndDivider Name
    1.000000,                !- Multiplier
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
     8.10,10.57, 0.90,   !- X,Y,Z ==> Vertex 1
     8.10,12.04, 0.90,   !- X,Y,Z ==> Vertex 2
     8.10,12.04, 2.37,   !- X,Y,Z ==> Vertex 3
     8.10,10.57, 2.37;   !- X,Y,Z ==> Vertex 4
 

Surface:HeatTransfer,
    Rm01001:IW01001, 
    Wall,                    !- Surface Type
    I-W0,                    !- Construction Name of the Surface
    Rm01001,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
    ,                        !- OutsideFaceEnvironment Object
    NoSun,                   !- Sun Exposure
    NoWind,                  !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
     0.00, 0.00, 0.00,   !- X,Y,Z ==> Vertex 1
     0.00, 0.00, 0.00,   !- X,Y,Z ==> Vertex 2
     0.00, 0.00, 0.00,   !- X,Y,Z ==> Vertex 3
     0.00, 0.00, 0.00;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer,
    Rm01001:RF04001, 
    Floor,                    !- Surface Type
    FLR0,                    !- Construction Name of the Surface
    Rm01001,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
     ,                        !- OutsideFaceEnvironment Object
    NoSun,             !- Sun Exposure
    NoWind,             !- Wind Exposure
    0.00,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    11.90, 8.20, 2.80,   !- X,Y,Z ==> Vertex 1
     5.70, 8.20, 2.80,   !- X,Y,Z ==> Vertex 2
     5.70, 4.40, 2.80,   !- X,Y,Z ==> Vertex 3
    11.90, 4.40, 2.80;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer,
    Rm01001:FL01001, 
    Floor,                   !- Surface Type
    GRND0,                    !- Construction Name of the Surface
    Rm01001,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
   ,                        !- OutsideFaceEnvironment Object
    NoSun,             !- Sun Exposure
    NoWind,             !- Wind Exposure
    1.00,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    11.90, 2.00, 0.00,   !- X,Y,Z ==> Vertex 1
     5.70, 2.00, 0.00,   !- X,Y,Z ==> Vertex 2
     5.70,-1.80, 0.00,   !- X,Y,Z ==> Vertex 3
    11.90,-1.80, 0.00;   !- X,Y,Z ==> Vertex 4

!-   ===========  ALL OBJECTS IN CLASS: ZONE ===========
! Room 1002**********
ZONE,
    Rm01002,      !Zone Name
    0,                       !- Relative North (to building) {deg}
    0, 0, 0,                 !- X,Y,Z  {m}
    1,                       !- Type
    1,                       !- Multiplier
    Autocalculate,           !- Ceiling Height {m}
    Autocalculate;           !- Volume {m3}

!-   ===========  ALL OBJECTS IN CLASS: SURFACEGEOMETRY ===========

Surface:HeatTransfer,
    Rm01002:EW01004, 
    Wall,                    !- Surface Type
    E-W0,                    !- Construction Name of the Surface
    Rm01002,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
	,                        !- OutsideFaceEnvironment Object
    SunExposed,              !- Sun Exposure
    WindExposed,             !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    11.90, 2.00, 0.00,   !- X,Y,Z ==> Vertex 1
     8.10, 2.00, 0.00,   !- X,Y,Z ==> Vertex 2
     8.10, 2.00, 2.80,   !- X,Y,Z ==> Vertex 3
    11.90, 2.00, 2.80;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer:Sub,
    Rm01002:EW01004:WIN-EW01004, 
    Window,                  !- Surface Type
    Win0,                    !- Construction Name of the Surface
    EW01004,                !- Base Surface Name
    ,                        !- OutsideFaceEnvironment Object
    0.50,                    !- View Factor to Ground
    ,                        !- Name of shading control
    ,                        !- WindowFrameAndDivider Name
    1.000000,                !- Multiplier
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    10.73, 2.00, 0.90,   !- X,Y,Z ==> Vertex 1
     9.26, 2.00, 0.90,   !- X,Y,Z ==> Vertex 2
     9.26, 2.00, 2.37,   !- X,Y,Z ==> Vertex 3
    10.73, 2.00, 2.37;   !- X,Y,Z ==> Vertex 4
 

Surface:HeatTransfer,
    Rm01002:EW01005, 
    Wall,                    !- Surface Type
    E-W0,                    !- Construction Name of the Surface
    Rm01002,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
	,                        !- OutsideFaceEnvironment Object
    SunExposed,              !- Sun Exposure
    WindExposed,             !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    15.70, 2.00, 0.00,   !- X,Y,Z ==> Vertex 1
    15.70,-4.20, 0.00,   !- X,Y,Z ==> Vertex 2
    15.70,-4.20, 2.80,   !- X,Y,Z ==> Vertex 3
    15.70, 2.00, 2.80;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer:Sub,
    Rm01002:EW01005:WIN-EW01005, 
    Window,                  !- Surface Type
    Win0,                    !- Construction Name of the Surface
    EW01005,                !- Base Surface Name
    ,                        !- OutsideFaceEnvironment Object
    0.50,                    !- View Factor to Ground
    ,                        !- Name of shading control
    ,                        !- WindowFrameAndDivider Name
    1.000000,                !- Multiplier
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    15.70,-0.37, 0.90,   !- X,Y,Z ==> Vertex 1
    15.70,-1.84, 0.90,   !- X,Y,Z ==> Vertex 2
    15.70,-1.84, 2.37,   !- X,Y,Z ==> Vertex 3
    15.70,-0.37, 2.37;   !- X,Y,Z ==> Vertex 4
 

Surface:HeatTransfer,
    Rm01002:EW01006, 
    Wall,                    !- Surface Type
    E-W0,                    !- Construction Name of the Surface
    Rm01002,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
	,                        !- OutsideFaceEnvironment Object
    SunExposed,              !- Sun Exposure
    WindExposed,             !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    15.70, 8.20, 0.00,   !- X,Y,Z ==> Vertex 1
    19.50, 8.20, 0.00,   !- X,Y,Z ==> Vertex 2
    19.50, 8.20, 2.80,   !- X,Y,Z ==> Vertex 3
    15.70, 8.20, 2.80;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer:Sub,
    Rm01002:EW01006:WIN-EW01006, 
    Window,                  !- Surface Type
    Win0,                    !- Construction Name of the Surface
    EW01006,                !- Base Surface Name
    ,                        !- OutsideFaceEnvironment Object
    0.50,                    !- View Factor to Ground
    ,                        !- Name of shading control
    ,                        !- WindowFrameAndDivider Name
    1.000000,                !- Multiplier
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    16.87, 8.20, 0.90,   !- X,Y,Z ==> Vertex 1
    18.34, 8.20, 0.90,   !- X,Y,Z ==> Vertex 2
    18.34, 8.20, 2.37,   !- X,Y,Z ==> Vertex 3
    16.87, 8.20, 2.37;   !- X,Y,Z ==> Vertex 4
 

Surface:HeatTransfer,
    Rm01002:RF04002, 
    Floor,                    !- Surface Type
    FLR0,                    !- Construction Name of the Surface
    Rm01002,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
     ,                        !- OutsideFaceEnvironment Object
    NoSun,             !- Sun Exposure
    NoWind,             !- Wind Exposure
    0.00,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    15.70, 8.20, 2.80,   !- X,Y,Z ==> Vertex 1
    11.90, 8.20, 2.80,   !- X,Y,Z ==> Vertex 2
    11.90, 2.00, 2.80,   !- X,Y,Z ==> Vertex 3
    15.70, 2.00, 2.80;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer,
    Rm01002:FL01002, 
    Floor,                   !- Surface Type
    GRND0,                    !- Construction Name of the Surface
    Rm01002,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
   ,                        !- OutsideFaceEnvironment Object
    NoSun,             !- Sun Exposure
    NoWind,             !- Wind Exposure
    1.00,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    15.70, 2.00, 0.00,   !- X,Y,Z ==> Vertex 1
    11.90, 2.00, 0.00,   !- X,Y,Z ==> Vertex 2
    11.90,-4.20, 0.00,   !- X,Y,Z ==> Vertex 3
    15.70,-4.20, 0.00;   !- X,Y,Z ==> Vertex 4

!-   =================== µÚ  2 ²ã ======================
!-   ===========  ALL OBJECTS IN CLASS: ZONE ===========
! Room 2001**********
ZONE,
    Rm02001,      !Zone Name
    0,                       !- Relative North (to building) {deg}
    0, 0, 0,                 !- X,Y,Z  {m}
    1,                       !- Type
    1,                       !- Multiplier
    Autocalculate,           !- Ceiling Height {m}
    Autocalculate;           !- Volume {m3}

!-   ===========  ALL OBJECTS IN CLASS: SURFACEGEOMETRY ===========

Surface:HeatTransfer,
    Rm02001:EW02001, 
    Wall,                    !- Surface Type
    E-W0,                    !- Construction Name of the Surface
    Rm02001,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
	,                        !- OutsideFaceEnvironment Object
    SunExposed,              !- Sun Exposure
    WindExposed,             !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
     8.10, 2.00, 2.80,   !- X,Y,Z ==> Vertex 1
     4.30, 2.00, 2.80,   !- X,Y,Z ==> Vertex 2
     4.30, 2.00, 5.60,   !- X,Y,Z ==> Vertex 3
     8.10, 2.00, 5.60;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer:Sub,
    Rm02001:EW02001:WIN-EW02001, 
    Window,                  !- Surface Type
    Win0,                    !- Construction Name of the Surface
    EW02001,                !- Base Surface Name
    ,                        !- OutsideFaceEnvironment Object
    0.50,                    !- View Factor to Ground
    ,                        !- Name of shading control
    ,                        !- WindowFrameAndDivider Name
    1.000000,                !- Multiplier
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
     6.93, 2.00, 3.70,   !- X,Y,Z ==> Vertex 1
     5.46, 2.00, 3.70,   !- X,Y,Z ==> Vertex 2
     5.46, 2.00, 5.17,   !- X,Y,Z ==> Vertex 3
     6.93, 2.00, 5.17;   !- X,Y,Z ==> Vertex 4
 

Surface:HeatTransfer,
    Rm02001:EW02002, 
    Wall,                    !- Surface Type
    E-W0,                    !- Construction Name of the Surface
    Rm02001,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
	,                        !- OutsideFaceEnvironment Object
    SunExposed,              !- Sun Exposure
    WindExposed,             !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    11.90, 8.20, 2.80,   !- X,Y,Z ==> Vertex 1
    15.70, 8.20, 2.80,   !- X,Y,Z ==> Vertex 2
    15.70, 8.20, 5.60,   !- X,Y,Z ==> Vertex 3
    11.90, 8.20, 5.60;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer:Sub,
    Rm02001:EW02002:WIN-EW02002, 
    Window,                  !- Surface Type
    Win0,                    !- Construction Name of the Surface
    EW02002,                !- Base Surface Name
    ,                        !- OutsideFaceEnvironment Object
    0.50,                    !- View Factor to Ground
    ,                        !- Name of shading control
    ,                        !- WindowFrameAndDivider Name
    1.000000,                !- Multiplier
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    13.07, 8.20, 3.70,   !- X,Y,Z ==> Vertex 1
    14.54, 8.20, 3.70,   !- X,Y,Z ==> Vertex 2
    14.54, 8.20, 5.17,   !- X,Y,Z ==> Vertex 3
    13.07, 8.20, 5.17;   !- X,Y,Z ==> Vertex 4
 

Surface:HeatTransfer,
    Rm02001:EW02003, 
    Wall,                    !- Surface Type
    E-W0,                    !- Construction Name of the Surface
    Rm02001,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
	,                        !- OutsideFaceEnvironment Object
    SunExposed,              !- Sun Exposure
    WindExposed,             !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
     8.10, 8.20, 2.80,   !- X,Y,Z ==> Vertex 1
     8.10,14.40, 2.80,   !- X,Y,Z ==> Vertex 2
     8.10,14.40, 5.60,   !- X,Y,Z ==> Vertex 3
     8.10, 8.20, 5.60;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer:Sub,
    Rm02001:EW02003:WIN-EW02003, 
    Window,                  !- Surface Type
    Win0,                    !- Construction Name of the Surface
    EW02003,                !- Base Surface Name
    ,                        !- OutsideFaceEnvironment Object
    0.50,                    !- View Factor to Ground
    ,                        !- Name of shading control
    ,                        !- WindowFrameAndDivider Name
    1.000000,                !- Multiplier
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
     8.10,10.57, 3.70,   !- X,Y,Z ==> Vertex 1
     8.10,12.04, 3.70,   !- X,Y,Z ==> Vertex 2
     8.10,12.04, 5.17,   !- X,Y,Z ==> Vertex 3
     8.10,10.57, 5.17;   !- X,Y,Z ==> Vertex 4
 

Surface:HeatTransfer,
    Rm02001:IW02001, 
    Wall,                    !- Surface Type
    I-W0,                    !- Construction Name of the Surface
    Rm02001,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
    ,                        !- OutsideFaceEnvironment Object
    NoSun,                   !- Sun Exposure
    NoWind,                  !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
     0.00, 0.00, 0.00,   !- X,Y,Z ==> Vertex 1
     0.00, 0.00, 0.00,   !- X,Y,Z ==> Vertex 2
     0.00, 0.00, 0.00,   !- X,Y,Z ==> Vertex 3
     0.00, 0.00, 0.00;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer,
    Rm02001:RF04001, 
    Floor,                    !- Surface Type
    FLR0,                    !- Construction Name of the Surface
    Rm02001,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
     ,                        !- OutsideFaceEnvironment Object
    NoSun,             !- Sun Exposure
    NoWind,             !- Wind Exposure
    0.00,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    11.90, 8.20, 2.80,   !- X,Y,Z ==> Vertex 1
     5.70, 8.20, 2.80,   !- X,Y,Z ==> Vertex 2
     5.70, 4.40, 2.80,   !- X,Y,Z ==> Vertex 3
    11.90, 4.40, 2.80;   !- X,Y,Z ==> Vertex 4

!-   ===========  ALL OBJECTS IN CLASS: ZONE ===========
! Room 2002**********
ZONE,
    Rm02002,      !Zone Name
    0,                       !- Relative North (to building) {deg}
    0, 0, 0,                 !- X,Y,Z  {m}
    1,                       !- Type
    1,                       !- Multiplier
    Autocalculate,           !- Ceiling Height {m}
    Autocalculate;           !- Volume {m3}

!-   ===========  ALL OBJECTS IN CLASS: SURFACEGEOMETRY ===========
Surface:HeatTransfer,
    Rm02002:EW02004, 
    Wall,                    !- Surface Type
    E-W0,                    !- Construction Name of the Surface
    Rm02002,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
	,                        !- OutsideFaceEnvironment Object
    SunExposed,              !- Sun Exposure
    WindExposed,             !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    11.90, 2.00, 2.80,   !- X,Y,Z ==> Vertex 1
     8.10, 2.00, 2.80,   !- X,Y,Z ==> Vertex 2
     8.10, 2.00, 5.60,   !- X,Y,Z ==> Vertex 3
    11.90, 2.00, 5.60;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer:Sub,
    Rm02002:EW02004:WIN-EW02004, 
    Window,                  !- Surface Type
    Win0,                    !- Construction Name of the Surface
    EW02004,                !- Base Surface Name
    ,                        !- OutsideFaceEnvironment Object
    0.50,                    !- View Factor to Ground
    ,                        !- Name of shading control
    ,                        !- WindowFrameAndDivider Name
    1.000000,                !- Multiplier
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    10.73, 2.00, 3.70,   !- X,Y,Z ==> Vertex 1
     9.26, 2.00, 3.70,   !- X,Y,Z ==> Vertex 2
     9.26, 2.00, 5.17,   !- X,Y,Z ==> Vertex 3
    10.73, 2.00, 5.17;   !- X,Y,Z ==> Vertex 4
 

Surface:HeatTransfer,
    Rm02002:EW02005, 
    Wall,                    !- Surface Type
    E-W0,                    !- Construction Name of the Surface
    Rm02002,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
	,                        !- OutsideFaceEnvironment Object
    SunExposed,              !- Sun Exposure
    WindExposed,             !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    15.70, 2.00, 2.80,   !- X,Y,Z ==> Vertex 1
    15.70,-4.20, 2.80,   !- X,Y,Z ==> Vertex 2
    15.70,-4.20, 5.60,   !- X,Y,Z ==> Vertex 3
    15.70, 2.00, 5.60;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer:Sub,
    Rm02002:EW02005:WIN-EW02005, 
    Window,                  !- Surface Type
    Win0,                    !- Construction Name of the Surface
    EW02005,                !- Base Surface Name
    ,                        !- OutsideFaceEnvironment Object
    0.50,                    !- View Factor to Ground
    ,                        !- Name of shading control
    ,                        !- WindowFrameAndDivider Name
    1.000000,                !- Multiplier
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    15.70,-0.37, 3.70,   !- X,Y,Z ==> Vertex 1
    15.70,-1.84, 3.70,   !- X,Y,Z ==> Vertex 2
    15.70,-1.84, 5.17,   !- X,Y,Z ==> Vertex 3
    15.70,-0.37, 5.17;   !- X,Y,Z ==> Vertex 4
 

Surface:HeatTransfer,
    Rm02002:EW02006, 
    Wall,                    !- Surface Type
    E-W0,                    !- Construction Name of the Surface
    Rm02002,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
	,                        !- OutsideFaceEnvironment Object
    SunExposed,              !- Sun Exposure
    WindExposed,             !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    15.70, 8.20, 2.80,   !- X,Y,Z ==> Vertex 1
    19.50, 8.20, 2.80,   !- X,Y,Z ==> Vertex 2
    19.50, 8.20, 5.60,   !- X,Y,Z ==> Vertex 3
    15.70, 8.20, 5.60;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer:Sub,
    Rm02002:EW02006:WIN-EW02006, 
    Window,                  !- Surface Type
    Win0,                    !- Construction Name of the Surface
    EW02006,                !- Base Surface Name
    ,                        !- OutsideFaceEnvironment Object
    0.50,                    !- View Factor to Ground
    ,                        !- Name of shading control
    ,                        !- WindowFrameAndDivider Name
    1.000000,                !- Multiplier
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    16.87, 8.20, 3.70,   !- X,Y,Z ==> Vertex 1
    18.34, 8.20, 3.70,   !- X,Y,Z ==> Vertex 2
    18.34, 8.20, 5.17,   !- X,Y,Z ==> Vertex 3
    16.87, 8.20, 5.17;   !- X,Y,Z ==> Vertex 4
 

Surface:HeatTransfer,
    Rm02002:RF04002, 
    Floor,                    !- Surface Type
    FLR0,                    !- Construction Name of the Surface
    Rm02002,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
     ,                        !- OutsideFaceEnvironment Object
    NoSun,             !- Sun Exposure
    NoWind,             !- Wind Exposure
    0.00,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    15.70, 8.20, 2.80,   !- X,Y,Z ==> Vertex 1
    11.90, 8.20, 2.80,   !- X,Y,Z ==> Vertex 2
    11.90, 2.00, 2.80,   !- X,Y,Z ==> Vertex 3
    15.70, 2.00, 2.80;   !- X,Y,Z ==> Vertex 4

!-   =================== µÚ  3 ²ã ======================
!-   ===========  ALL OBJECTS IN CLASS: ZONE ===========
! Room 3001**********
ZONE,
    Rm03001,      !Zone Name
    0,                       !- Relative North (to building) {deg}
    0, 0, 0,                 !- X,Y,Z  {m}
    1,                       !- Type
    1,                       !- Multiplier
    Autocalculate,           !- Ceiling Height {m}
    Autocalculate;           !- Volume {m3}

!-   ===========  ALL OBJECTS IN CLASS: SURFACEGEOMETRY ===========
Surface:HeatTransfer,
    Rm03001:EW03001, 
    Wall,                    !- Surface Type
    E-W0,                    !- Construction Name of the Surface
    Rm03001,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
	,                        !- OutsideFaceEnvironment Object
    SunExposed,              !- Sun Exposure
    WindExposed,             !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
     8.10, 2.00, 5.60,   !- X,Y,Z ==> Vertex 1
     4.30, 2.00, 5.60,   !- X,Y,Z ==> Vertex 2
     4.30, 2.00, 8.40,   !- X,Y,Z ==> Vertex 3
     8.10, 2.00, 8.40;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer:Sub,
    Rm03001:EW03001:WIN-EW03001, 
    Window,                  !- Surface Type
    Win0,                    !- Construction Name of the Surface
    EW03001,                !- Base Surface Name
    ,                        !- OutsideFaceEnvironment Object
    0.50,                    !- View Factor to Ground
    ,                        !- Name of shading control
    ,                        !- WindowFrameAndDivider Name
    1.000000,                !- Multiplier
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
     6.93, 2.00, 6.50,   !- X,Y,Z ==> Vertex 1
     5.46, 2.00, 6.50,   !- X,Y,Z ==> Vertex 2
     5.46, 2.00, 7.97,   !- X,Y,Z ==> Vertex 3
     6.93, 2.00, 7.97;   !- X,Y,Z ==> Vertex 4
 

Surface:HeatTransfer,
    Rm03001:EW03002, 
    Wall,                    !- Surface Type
    E-W0,                    !- Construction Name of the Surface
    Rm03001,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
	,                        !- OutsideFaceEnvironment Object
    SunExposed,              !- Sun Exposure
    WindExposed,             !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    11.90, 8.20, 5.60,   !- X,Y,Z ==> Vertex 1
    15.70, 8.20, 5.60,   !- X,Y,Z ==> Vertex 2
    15.70, 8.20, 8.40,   !- X,Y,Z ==> Vertex 3
    11.90, 8.20, 8.40;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer:Sub,
    Rm03001:EW03002:WIN-EW03002, 
    Window,                  !- Surface Type
    Win0,                    !- Construction Name of the Surface
    EW03002,                !- Base Surface Name
    ,                        !- OutsideFaceEnvironment Object
    0.50,                    !- View Factor to Ground
    ,                        !- Name of shading control
    ,                        !- WindowFrameAndDivider Name
    1.000000,                !- Multiplier
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    13.07, 8.20, 6.50,   !- X,Y,Z ==> Vertex 1
    14.54, 8.20, 6.50,   !- X,Y,Z ==> Vertex 2
    14.54, 8.20, 7.97,   !- X,Y,Z ==> Vertex 3
    13.07, 8.20, 7.97;   !- X,Y,Z ==> Vertex 4
 

Surface:HeatTransfer,
    Rm03001:EW03003, 
    Wall,                    !- Surface Type
    E-W0,                    !- Construction Name of the Surface
    Rm03001,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
	,                        !- OutsideFaceEnvironment Object
    SunExposed,              !- Sun Exposure
    WindExposed,             !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
     8.10, 8.20, 5.60,   !- X,Y,Z ==> Vertex 1
     8.10,14.40, 5.60,   !- X,Y,Z ==> Vertex 2
     8.10,14.40, 8.40,   !- X,Y,Z ==> Vertex 3
     8.10, 8.20, 8.40;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer:Sub,
    Rm03001:EW03003:WIN-EW03003, 
    Window,                  !- Surface Type
    Win0,                    !- Construction Name of the Surface
    EW03003,                !- Base Surface Name
    ,                        !- OutsideFaceEnvironment Object
    0.50,                    !- View Factor to Ground
    ,                        !- Name of shading control
    ,                        !- WindowFrameAndDivider Name
    1.000000,                !- Multiplier
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
     8.10,10.57, 6.50,   !- X,Y,Z ==> Vertex 1
     8.10,12.04, 6.50,   !- X,Y,Z ==> Vertex 2
     8.10,12.04, 7.97,   !- X,Y,Z ==> Vertex 3
     8.10,10.57, 7.97;   !- X,Y,Z ==> Vertex 4
 

Surface:HeatTransfer,
    Rm03001:IW03001, 
    Wall,                    !- Surface Type
    I-W0,                    !- Construction Name of the Surface
    Rm03001,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
    ,                        !- OutsideFaceEnvironment Object
    NoSun,                   !- Sun Exposure
    NoWind,                  !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
     0.00, 0.00, 0.00,   !- X,Y,Z ==> Vertex 1
     0.00, 0.00, 0.00,   !- X,Y,Z ==> Vertex 2
     0.00, 0.00, 0.00,   !- X,Y,Z ==> Vertex 3
     0.00, 0.00, 0.00;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer,
    Rm03001:RF04001, 
    Roof,                    !- Surface Type
    ROOF0,                    !- Construction Name of the Surface
    Rm03001,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
    ,                        !- OutsideFaceEnvironment Object
    SunExposed,              !- Sun Exposure
    WindExposed,             !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    14.30, 2.00, 2.80,   !- X,Y,Z ==> Vertex 2
    14.30, 5.80, 2.80,   !- X,Y,Z ==> Vertex 3
     8.10, 5.80, 2.80;   !- X,Y,Z ==> Vertex 4

!-   ===========  ALL OBJECTS IN CLASS: ZONE ===========
! Room 3002**********
ZONE,
    Rm03002,      !Zone Name
    0,                       !- Relative North (to building) {deg}
    0, 0, 0,                 !- X,Y,Z  {m}
    1,                       !- Type
    1,                       !- Multiplier
    Autocalculate,           !- Ceiling Height {m}
    Autocalculate;           !- Volume {m3}

!-   ===========  ALL OBJECTS IN CLASS: SURFACEGEOMETRY ===========
Surface:HeatTransfer,
    Rm03002:EW03004, 
    Wall,                    !- Surface Type
    E-W0,                    !- Construction Name of the Surface
    Rm03002,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
	,                        !- OutsideFaceEnvironment Object
    SunExposed,              !- Sun Exposure
    WindExposed,             !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    11.90, 2.00, 5.60,   !- X,Y,Z ==> Vertex 1
     8.10, 2.00, 5.60,   !- X,Y,Z ==> Vertex 2
     8.10, 2.00, 8.40,   !- X,Y,Z ==> Vertex 3
    11.90, 2.00, 8.40;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer:Sub,
    Rm03002:EW03004:WIN-EW03004, 
    Window,                  !- Surface Type
    Win0,                    !- Construction Name of the Surface
    EW03004,                !- Base Surface Name
    ,                        !- OutsideFaceEnvironment Object
    0.50,                    !- View Factor to Ground
    ,                        !- Name of shading control
    ,                        !- WindowFrameAndDivider Name
    1.000000,                !- Multiplier
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    10.73, 2.00, 6.50,   !- X,Y,Z ==> Vertex 1
     9.26, 2.00, 6.50,   !- X,Y,Z ==> Vertex 2
     9.26, 2.00, 7.97,   !- X,Y,Z ==> Vertex 3
    10.73, 2.00, 7.97;   !- X,Y,Z ==> Vertex 4
 

Surface:HeatTransfer,
    Rm03002:EW03005, 
    Wall,                    !- Surface Type
    E-W0,                    !- Construction Name of the Surface
    Rm03002,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
	,                        !- OutsideFaceEnvironment Object
    SunExposed,              !- Sun Exposure
    WindExposed,             !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    15.70, 2.00, 5.60,   !- X,Y,Z ==> Vertex 1
    15.70,-4.20, 5.60,   !- X,Y,Z ==> Vertex 2
    15.70,-4.20, 8.40,   !- X,Y,Z ==> Vertex 3
    15.70, 2.00, 8.40;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer:Sub,
    Rm03002:EW03005:WIN-EW03005, 
    Window,                  !- Surface Type
    Win0,                    !- Construction Name of the Surface
    EW03005,                !- Base Surface Name
    ,                        !- OutsideFaceEnvironment Object
    0.50,                    !- View Factor to Ground
    ,                        !- Name of shading control
    ,                        !- WindowFrameAndDivider Name
    1.000000,                !- Multiplier
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    15.70,-0.37, 6.50,   !- X,Y,Z ==> Vertex 1
    15.70,-1.84, 6.50,   !- X,Y,Z ==> Vertex 2
    15.70,-1.84, 7.97,   !- X,Y,Z ==> Vertex 3
    15.70,-0.37, 7.97;   !- X,Y,Z ==> Vertex 4
 

Surface:HeatTransfer,
    Rm03002:EW03006, 
    Wall,                    !- Surface Type
    E-W0,                    !- Construction Name of the Surface
    Rm03002,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
	,                        !- OutsideFaceEnvironment Object
    SunExposed,              !- Sun Exposure
    WindExposed,             !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    15.70, 8.20, 5.60,   !- X,Y,Z ==> Vertex 1
    19.50, 8.20, 5.60,   !- X,Y,Z ==> Vertex 2
    19.50, 8.20, 8.40,   !- X,Y,Z ==> Vertex 3
    15.70, 8.20, 8.40;   !- X,Y,Z ==> Vertex 4

Surface:HeatTransfer:Sub,
    Rm03002:EW03006:WIN-EW03006, 
    Window,                  !- Surface Type
    Win0,                    !- Construction Name of the Surface
    EW03006,                !- Base Surface Name
    ,                        !- OutsideFaceEnvironment Object
    0.50,                    !- View Factor to Ground
    ,                        !- Name of shading control
    ,                        !- WindowFrameAndDivider Name
    1.000000,                !- Multiplier
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    16.87, 8.20, 6.50,   !- X,Y,Z ==> Vertex 1
    18.34, 8.20, 6.50,   !- X,Y,Z ==> Vertex 2
    18.34, 8.20, 7.97,   !- X,Y,Z ==> Vertex 3
    16.87, 8.20, 7.97;   !- X,Y,Z ==> Vertex 4
 

Surface:HeatTransfer,
    Rm03002:RF04002, 
    Roof,                    !- Surface Type
    ROOF0,                    !- Construction Name of the Surface
    Rm03002,                 !- Zone Name
    ExteriorEnvironment,     !- OutsideFaceEnvironment
    ,                        !- OutsideFaceEnvironment Object
    SunExposed,              !- Sun Exposure
    WindExposed,             !- Wind Exposure
    0.50,                    !- View Factor to Ground
    4,                       !- Number of Surface Vertex Groups -- Number of (X,Y,Z) groups in this surface
    15.70, 2.00, 2.80,   !- X,Y,Z ==> Vertex 2
    15.70, 8.20, 2.80,   !- X,Y,Z ==> Vertex 3
    11.90, 8.20, 2.80;   !- X,Y,Z ==> Vertex 4
SCHEDULETYPE,
	Fraction,		!ScheduleType Name
	0.0:1.0,		!range
	CONTINUOUS;		!Numeric Type

SCHEDULETYPE,
	On/Off,		!ScheduleType Name
	0:1,		!range
	DISCRETE;		!Numeric Type

SCHEDULETYPE,
	Temperature,		!ScheduleType Name
	-60:200,		!range
	CONTINUOUS;		!Numeric Type

SCHEDULETYPE,
	Control Type,		!ScheduleType Name
	0:4,		!range
	DISCRETE;		!Numeric Type

SCHEDULETYPE,
	Any Number,		!ScheduleType Name
	,		!range
	;		!Numeric Type

SCHEDULE:COMPACT,
	ALWAYS_ON,		!Name
	Fraction,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,1.0;		!Complex Field #3

SCHEDULE:COMPACT,
	ALWAYS_OFF,		!Name
	Fraction,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,0.0;		!Complex Field #3

SCHEDULE:COMPACT,
	HVAC_SCH,		!Name
	On/Off,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: Weekdays,		!Complex Field #2
	Until: 07:00,0.0,		!Complex Field #3
	Until: 18:00,1.0,		!Complex Field #4
	Until: 24:00,0.0,		!Complex Field #5
	For: WeekEnds Holiday,		!Complex Field #6
	Until: 24:00,0.0,		!Complex Field #7
	For: WinterDesignDay,		!Complex Field #8
	Until: 24:00,1.0,		!Complex Field #9
	For: SummerDesignDay,		!Complex Field #10
	Until: 24:00,1.0,		!Complex Field #11
	For: AllOtherDays,		!Complex Field #12
	Until: 24:00,0.0;		!Complex Field #13

SCHEDULE:COMPACT,
	Plant_SCH,		!Name
	On/Off,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,1.0;		!Complex Field #3

SCHEDULE:COMPACT,
	FAN_SCH,		!Name
	Fraction,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,1.0;		!Complex Field #3

SCHEDULE:COMPACT,
	ReheatCoi_SCH,		!Name
	Fraction,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,1.0;		!Complex Field #3

SCHEDULE:COMPACT,
	CoolingCoil_SCH,		!Name
	Fraction,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,1.0;		!Complex Field #3

SCHEDULE:COMPACT,
	HTGSETP_SCH,		!Name
	Temperature,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: WeekDays,		!Complex Field #2
	Until: 06:00,12,		!Complex Field #3
	Until: 07:00,18,		!Complex Field #4
	Until: 18:00,20.0,		!Complex Field #5
	Until: 24:00,12.0,		!Complex Field #6
	For: WeekEnds Holiday,		!Complex Field #7
	Until: 24:00,12.0,		!Complex Field #8
	For: WinterDesignDay,		!Complex Field #9
	Until: 24:00,20.0,		!Complex Field #10
	For: SummerDesignDay,		!Complex Field #11
	Until: 24:00,12.0,		!Complex Field #12
	For: AllOtherDays,		!Complex Field #13
	Until: 24:00,12.0;		!Complex Field #14

SCHEDULE:COMPACT,
	CLGSETP_SCH,		!Name
	Temperature,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: WeekDays,		!Complex Field #2
	Until: 06:00,37,		!Complex Field #3
	Until: 07:00,28,		!Complex Field #4
	Until: 18:00,26,		!Complex Field #5
	Until: 24:00,37.0,		!Complex Field #6
	For: WeekEnds Holiday,		!Complex Field #7
	Until: 24:00,37.0,		!Complex Field #8
	For: WinterDesignDay,		!Complex Field #9
	Until: 24:00,37.0,		!Complex Field #10
	For: SummerDesignDay,		!Complex Field #11
	Until: 24:00,26.0,		!Complex Field #12
	For: AllOtherDays,		!Complex Field #13
	Until: 24:00,26.0;		!Complex Field #14

SCHEDULE:COMPACT,
	Summer On,		!Name
	Fraction,		!ScheduleType
	Through: 4/30,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,0.0,		!Complex Field #3
	Through: 9/30,		!Complex Field #4
	For: AllDays,		!Complex Field #5
	Until: 24:00,1.0,		!Complex Field #6
	Through: 12/31,		!Complex Field #7
	For: AllDays,		!Complex Field #8
	Until: 24:00,0.0;		!Complex Field #9

SCHEDULE:COMPACT,
	Winter On,		!Name
	Fraction,		!ScheduleType
	Through: 4/30,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,1.0,		!Complex Field #3
	Through: 9/30,		!Complex Field #4
	For: AllDays,		!Complex Field #5
	Until: 24:00,0.0,		!Complex Field #6
	Through: 12/31,		!Complex Field #7
	For: AllDays,		!Complex Field #8
	Until: 24:00,1;		!Complex Field #9

SCHEDULE:COMPACT,
	MinOA_SCH,		!Name
	Fraction,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,1.0;		!Complex Field #3

SCHEDULE:COMPACT,
	Dual Zone Control Type Sched,		!Name
	Control Type,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,4;		!Complex Field #3

SCHEDULE:COMPACT,
	Seasonal Reset Supply Air Temp Sched,		!Name
	Temperature,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,13.0;		!Complex Field #3

SCHEDULE:COMPACT,
	CW Loop Temp Sched,		!Name
	Temperature,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,6.7;		!Complex Field #3

SCHEDULE:COMPACT,
	HW Loop Temp Sched,		!Name
	Temperature,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,60.0;		!Complex Field #3

SCHEDULE:COMPACT,
	Heating Supply Air Temp Sched,		!Name
	Temperature,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,16.0;		!Complex Field #3

SCHEDULE:COMPACT,
	Chilled Water Loop CndW Temp Sched,		!Name
	Temperature,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,29.4;		!Complex Field #3

SCHEDULE:COMPACT,
	COMPACT HVAC-ALWAYS 1,		!Name
	Any Number,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,1;		!Complex Field #3

SCHEDULE:COMPACT,
	COMPACT HVAC-ALWAYS 4.0,		!Name
	Any Number,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,4;		!Complex Field #3

SCHEDULE:COMPACT,
	COMPACT HVAC-ALWAYS 5,		!Name
	Any Number,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,5;		!Complex Field #3

SCHEDULE:COMPACT,
	COMPACT HVAC-ALWAYS 7.22,		!Name
	Any Number,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,7.22;		!Complex Field #3

SCHEDULE:COMPACT,
	COMPACT HVAC-ALWAYS 10.0,		!Name
	Any Number,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,10;		!Complex Field #3

SCHEDULE:COMPACT,
	COMPACT HVAC-ALWAYS 29.4,		!Name
	Any Number,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,29.4;		!Complex Field #3

SCHEDULE:COMPACT,
	COMPACT HVAC-ALWAYS 82,		!Name
	Any Number,		!ScheduleType
	Through: 12/31,		!Complex Field #1
	For: AllDays,		!Complex Field #2
	Until: 24:00,82;		!Complex Field #3

ZONE EQUIPMENT LIST,
	Zone_EquipList1,		!Name
	PURCHASED AIR,		!KEY--Zone Equipment Type 1
	Purchased_Air1,		!Type Name 1
	1,		!Cooling Priority 1
	1;		!Heating Priority 1

CONTROLLED ZONE EQUIP CONFIGURATION,
	ZoneGroup1,		!Zone Name
	Zone_EquipList1,		!List Name: Zone Equipment
	Purchased_Air1_ZoneSupplyAirNodeName,		!Node List or Node Name: Zone Air Inlet Node(s)
	ZoneGroup1_ZoneAirExhaustNodes,		!Node List or Node Name: Zone Air Exhaust Node(s)
	ZoneGroup1_ZoneAirNodeName,		!Zone Air Node Name
	ZoneGroup1_ZoneReturnAirNodeName;		!Zone Return Air Node Name

PURCHASED AIR,
	Purchased_Air1,		!Purchased Air Name
	Purchased_Air1_ZoneSupplyAirNodeName,		!Zone Supply Air Node Name
	50,		!Heating Supply Air Temp
	13,		!Cooling Supply Air Temp
	0.013,		!Heating Supply Air Humidity Ratio
	0.013,		!Cooling Supply Air Humidity Ratio
	NO LIMIT,		!heating limit
	autosize,		!Maximum heating air flow rate
	NO LIMIT,		!cooling limit
	autosize,		!Maximum cooling air flow rate
	OUTSIDE AIR,		!outside air
	autosize,		!Outside air flow rate
	ALWAYS_ON,		!heating availability schedule
	ALWAYS_ON;		!cooling availability schedule

!-   ===========  ALL OBJECTS IN CLASS: REPORT VARIABLE ===========
Report Variable,
    *,                       !- Key_Value
    Total Electric Demand,  !- Variable_Name
    Monthly;                  !- Reporting_Frequency

Report Variable,
    *,                       !- Key_Value
    Boiler Electric Consumption,  !- Variable_Name
    Monthly;                  !- Reporting_Frequency

Report Variable,
    *,                       !- Key_Value
    Boiler Electric Consumption,  !- Variable_Name
    RunPeriod;                  !- Reporting_Frequency

Report Variable,
    *,                       !- Key_Value
    Direct Fired Absorption Chiller Cooling Gas Consumption,  !- Variable_Name
    Monthly;                  !- Reporting_Frequency

Report Variable,
    *,                       !- Key_Value
    Direct Fired Absorption Chiller Cooling Gas Consumption,  !- Variable_Name
    RunPeriod;                  !- Reporting_Frequency

!-   ===========  ALL OBJECTS IN CLASS: REPORT METERFILEONLY ===========
Report MeterFileOnly,
    Electricity:Facility,    !- Meter_Name
    Hourly;                  !- Reporting_Frequency

Report MeterFileOnly,
    Electricity:Facility,    !- Meter_Name
    Monthly;                  !- Reporting_Frequency

Report MeterFileOnly,
    Electricity:Building,    !- Meter_Name
    Monthly;                  !- Reporting_Frequency

Report MeterFileOnly,
    InteriorLights:Electricity,  !- Meter_Name
    Monthly;                  !- Reporting_Frequency

Report MeterFileOnly,
    ExteriorLights:Electricity,  !- Meter_Name
    Monthly;                  !- Reporting_Frequency

Report MeterFileOnly,
    InteriorEquipment:Electricity,  !- Meter_Name
    Monthly;                  !- Reporting_Frequency

Report MeterFileOnly,
    ExteriorEquipment:Electricity,  !- Meter_Name
    Monthly;                  !- Reporting_Frequency

Report MeterFileOnly,
    Electricity:Plant,       !- Meter_Name
    Monthly;                  !- Reporting_Frequency

Report MeterFileOnly,
    Pumps:Electricity,       !- Meter_Name
    Monthly;                  !- Reporting_Frequency

Report MeterFileOnly,
    Fans:Electricity,        !- Meter_Name
    Monthly;                  !- Reporting_Frequency

Report MeterFileOnly,
    HeatRejection:Electricity,  !- Meter_Name
    Monthly;                  !- Reporting_Frequency

Report MeterFileOnly,
    Gas:Facility,            !- Meter_Name
Monthly;                  !- Reporting_Frequency

Report MeterFileOnly,
    Heating:Gas,            !- Meter_Name
Monthly;                  !- Reporting_Frequency

Report MeterFileOnly,
    Diesel:Facility,            !- Meter_Name
Monthly;                  !- Reporting_Frequency

Report MeterFileOnly,
    Heating:Diesel,            !- Meter_Name
Monthly;                  !- Reporting_Frequency

Report MeterFileOnly,
    Electricity:Facility,    !- Meter_Name
RunPeriod;                  !- Reporting_Frequency

Report MeterFileOnly,
    Electricity:Building,    !- Meter_Name
    RunPeriod;                  !- Reporting_Frequency

Report MeterFileOnly,
    InteriorLights:Electricity,  !- Meter_Name
    RunPeriod;                  !- Reporting_Frequency

Report MeterFileOnly,
    ExteriorLights:Electricity,  !- Meter_Name
    RunPeriod;                  !- Reporting_Frequency

Report MeterFileOnly,
    InteriorEquipment:Electricity,  !- Meter_Name
    RunPeriod;                 !- Reporting_Frequency

Report MeterFileOnly,
    ExteriorEquipment:Electricity,  !- Meter_Name
    RunPeriod;                  !- Reporting_Frequency

Report MeterFileOnly,
    Electricity:Plant,       !- Meter_Name
    RunPeriod;                 !- Reporting_Frequency

Report MeterFileOnly,
    Pumps:Electricity,       !- Meter_Name
    RunPeriod;                  !- Reporting_Frequency

Report MeterFileOnly,
    Fans:Electricity,        !- Meter_Name
    RunPeriod;                  !- Reporting_Frequency

Report MeterFileOnly,
    HeatRejection:Electricity,  !- Meter_Name
    RunPeriod;                 !- Reporting_Frequency

Report MeterFileOnly,
    Gas:Facility,            !- Meter_Name
RunPeriod;                  !- Reporting_Frequency

Report MeterFileOnly,
    Heating:Gas,            !- Meter_Name
RunPeriod;                 !- Reporting_Frequency

Report MeterFileOnly,
    Diesel:Facility,            !- Meter_Name
RunPeriod;                  !- Reporting_Frequency

Report MeterFileOnly,
    Heating:Diesel,            !- Meter_Name
RunPeriod;                  !- Reporting_Frequency

!-   ===========  ALL OBJECTS IN CLASS: REPORT ===========

Report,
    Variable Dictionary;     !- Type_of_Report

Report,
    surfaces,                !- Type_of_Report
    dxf;                     !- Name_of_Report

Report,
    construction;            !- Type_of_Report
